# Computation and result analysis

## Reference

All computations of FIDES Lab follow to the requirements of FIDES Guide 2022. This software is 100% compatible with the guide. In this help we won't describe the formulas used for the computation of component failure rate, please refer to the guide for formulas. A component family has its own set of formulas, if you don't have access to the FIDES guide you can see the formulas thanks to the info button next to the family drop down menu.

Note: It is possible to double-click on the image in order to open it in the operating system default viewer.

All failure rates are in FIT (10-9 h10-1)

## Computation configuration panel

Computations are done in a separate window. To open the computation window click on the

The computation window is empty by default:

At the top, it contains several field that will be filled after computation:

- Computed lambda: The lambda of the product. it is the sum of the lambda of all components
- Computation date: when you did the last computation
- Compliance: a flag that says is this document is compliant with FIDES standard, it won't be if you ie values out of scope or custom families
- Up to date: checked is the model was not modified since the last computation

In the middle part, there is a button and a progress bar. once computation will be done, the button will become a Clear button.

At the bottom, there are 4 tabs related to the results :

- Log: that shows the computation process
- Detailed values
- List values
- Compliance

Here, the only thing you can do is using the , it will start FIDES computation. While the software is computing, you can see the details of the computation in the log tab

### Detailed values

Once computation is done, the Detailed panel is selected and display 2 tables. The first panel on the left contains the overall result for each container or component, it is the weighted value over the full profile duration.

It contains the following columns:

- Type: System, sub-system, equipment, …., component
- ID: a unique ID that identifies the different containers/components is case they have the same name
- Parent: the parent in the hierarchy
- Name: the name of the entity
- Quantity: for components, the value of the quantity parameter
- Family
- Mission profile
- λcst_unit: the constant Lambda per unit
- λcst_total: the total constant Lambda for the line (value of the previous column multiplied by the quantity)
- λwear_out_unit: the Lambda wear-out per unit
- λwear_out_total: the total Lambda wear-out for the line (value of the previous column multiplied by the quantity)
- λunitary: the sum of λcst_unit and λwear_out_unit
- λtotal: the sum of λcst_total and λwear_out_total

In the left table, you don't have access to the decomposition of the failure rate for a component, but once you have selected a line, the table on the right displays the details per phase and per stress for the selected component. Warning: all the failure rates in this table is weighted values. On a line the value is not the one directly computed for the phase but the value_computed_for_the_phase * duration_of_the_phase / duration_of_the profile.

Doing like this you have the part of the total lambda (for the total duration) that is due to a phase, and you can do the sum of the values per phase to have the full lambda for the total duration of the profile.

### Synthesis

The synthesis tab contains all the data available in the Detail tab but in only one table. A component with a profile containing N phase will be displayed over N+1 lines, the first line for the total (over the profile duration) and then one line per phase. The table has a very large number of column since its displays all the possible λ for a component or a container.

### Compliance

The compliance tab gathers all the things that are not compliant with the FIDES Guide. A top banner displays the number of deviation, and the table explains what is not compliant and must be fixed (if you want to be compliant)

## Start a new computation

After any modification on your BOM or profiles, you need to restart the computation. Since the computation window handle only one result, you have to clear the previous results before starting a new computation.