<?xml version="1.0" encoding="UTF-8" ?>
<open-fides-notice open-fides-version="1.1">
    <macro-family code="ec">
        <family code="ec_ic" name="Integrated circuits">
            <family-param code="ec_icds_pkg" name="Package" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="EC_IC_PKG_01" name="PDIP [EC_IC]" value="1"/>
                <list-param-item code="EC_IC_PKG_02" name="CERDIP, CDIP [EC_IC]" value="2"/>
                <list-param-item code="EC_IC_PKG_03" name="PQFP [EC_IC]" value="3"/>
                <list-param-item code="EC_IC_PKG_04" name="TQFP, LQFP [EC_IC]" value="4"/>
                <list-param-item code="EC_IC_PKG_05" name="Power QFP [EC_IC]" value="5"/>
                <list-param-item code="EC_IC_PKG_06" name="CERPACK [EC_IC]" value="6"/>
                <list-param-item code="EC_IC_PKG_07" name="CQFP [EC_IC]" value="7"/>
                <list-param-item code="EC_IC_PKG_08" name="PLCC [EC_IC]" value="8"/>
                <list-param-item code="EC_IC_PKG_09" name="J-LCC [EC_IC]" value="9"/>
                <list-param-item code="EC_IC_PKG_10" name="CLCC [EC_IC]" value="10"/>
                <list-param-item code="EC_IC_PKG_11" name="SOJ [EC_IC]" value="11"/>
                <list-param-item code="EC_IC_PKG_12" name="SO [EC_IC]" value="12"/>
                <list-param-item code="EC_IC_PKG_13" name="TSOP [EC_IC]" value="13"/>
                <list-param-item code="EC_IC_PKG_14" name="SSOP, QSOP [EC_IC]" value="14"/>
                <list-param-item code="EC_IC_PKG_15" name="TSSOP, MSOP [EC_IC]" value="15"/>
                <list-param-item code="EC_IC_PKG_16" name="QFN, DFN ≥0.5 mm [EC_IC]" value="16"/>
                <list-param-item code="EC_IC_PKG_17" name="QFN 0.4 mm [EC_IC]" value="17"/>
                <list-param-item code="EC_IC_PKG_18" name="LGA Plastic [EC_IC]" value="18"/>
                <list-param-item code="EC_IC_PKG_19" name="PBGA &lt;0.5 mm [EC_IC]" value="19"/>
                <list-param-item code="EC_IC_PKG_20" name="PBGA 0.5 mm [EC_IC]" value="20"/>
                <list-param-item code="EC_IC_PKG_21" name="PBGA 0.65 mm [EC_IC]" value="21"/>
                <list-param-item code="EC_IC_PKG_22" name="PBGA BT 0.8 mm [EC_IC]" value="22"/>
                <list-param-item code="EC_IC_PKG_23" name="PBGA flex 0.8 mm [EC_IC]" value="23"/>
                <list-param-item code="EC_IC_PKG_24" name="PBGA BOC 0.8 mm (memories) [EC_IC]" value="24"/>
                <list-param-item code="EC_IC_PKG_25" name="PBGA BT 1.00 mm [EC_IC]" value="25"/>
                <list-param-item code="EC_IC_PKG_26" name="PBGA 1.27 mm [EC_IC]" value="26"/>
                <list-param-item code="EC_IC_PKG_27" name="Power BGA [EC_IC]" value="27"/>
                <list-param-item code="EC_IC_PKG_28" name="BGA WLP &lt;0.5 mm [EC_IC]" value="28"/>
                <list-param-item code="EC_IC_PKG_29" name="BGA WLP 0.5 mm [EC_IC]" value="29"/>
                <list-param-item code="EC_IC_PKG_30" name="FC-PBGA 0.8 mm [EC_IC]" value="30"/>
                <list-param-item code="EC_IC_PKG_31" name="FC-PBGA 1 mm [EC_IC]" value="31"/>
                <list-param-item code="EC_IC_PKG_32" name="CBGA [EC_IC]" value="32"/>
                <list-param-item code="EC_IC_PKG_33" name="DBGA [EC_IC]" value="33"/>
                <list-param-item code="EC_IC_PKG_34" name="CI CGA [EC_IC]" value="34"/>
                <list-param-item code="EC_IC_PKG_35" name="CPGA [EC_IC]" value="35"/>
                <list-param-item code="EC_DS_PKG_01" name="CB417 [EC_DS]" value="101"/>
                <list-param-item code="EC_DS_PKG_02" name="CB429 [EC_DS]" value="102"/>
                <list-param-item code="EC_DS_PKG_03" name="DO13, DO202AA [EC_DS]" value="103"/>
                <list-param-item code="EC_DS_PKG_04" name="DO15, DO204AC [EC_DS]" value="104"/>
                <list-param-item code="EC_DS_PKG_05" name="DO27, DO201AA [EC_DS]" value="105"/>
                <list-param-item code="EC_DS_PKG_06" name="DO35, DO204AH [EC_DS]" value="106"/>
                <list-param-item code="EC_DS_PKG_07" name="DO41, DO204AL [EC_DS]" value="107"/>
                <list-param-item code="EC_DS_PKG_08" name="DO92 [EC_DS]" value="108"/>
                <list-param-item code="EC_DS_PKG_09" name="F126 [EC_DS]" value="109"/>
                <list-param-item code="EC_DS_PKG_10" name="SIL, SIP, ZIP [EC_DS]" value="110"/>
                <list-param-item code="EC_DS_PKG_11" name="TO92, SOT54, SC43, TO226AA [EC_DS]" value="111"/>
                <list-param-item code="EC_DS_PKG_12" name="TO126, SOT32, TO225AA [EC_DS]" value="112"/>
                <list-param-item code="EC_DS_PKG_13" name="TO202 [EC_DS]" value="113"/>
                <list-param-item code="EC_DS_PKG_14" name="SOT23-3, TO236AB [EC_DS]" value="114"/>
                <list-param-item code="EC_DS_PKG_15" name="SOT23-5, SC74A, SOT25 [EC_DS]" value="115"/>
                <list-param-item code="EC_DS_PKG_16" name="SOT23-6, SC74, SOT26, SOT457 [EC_DS]" value="116"/>
                <list-param-item code="EC_DS_PKG_17" name="SOT143, TO253AA, SC61B [EC_DS]" value="117"/>
                <list-param-item code="EC_DS_PKG_18" name="SOT323, SC70 [EC_DS]" value="118"/>
                <list-param-item code="EC_DS_PKG_19" name="SOT346, SC59, TO236AA [EC_DS]" value="119"/>
                <list-param-item code="EC_DS_PKG_20" name="SOT353, SC70-5, SC88A [EC_DS]" value="120"/>
                <list-param-item code="EC_DS_PKG_21" name="SOT363, SC70-6, SC88 [EC_DS]" value="121"/>
                <list-param-item code="EC_DS_PKG_22" name="SOD123 [EC_DS]" value="122"/>
                <list-param-item code="EC_DS_PKG_23" name="SOD323, SC76 [EC_DS]" value="123"/>
                <list-param-item code="EC_DS_PKG_24" name="SOD523, SC79 [EC_DS]" value="124"/>
                <list-param-item code="EC_DS_PKG_25" name="SOT223, SC73, TO261AA [EC_DS]" value="125"/>
                <list-param-item code="EC_DS_PKG_26" name="SOT243 [EC_DS]" value="126"/>
                <list-param-item code="EC_DS_PKG_27" name="SOT343, SC82 [EC_DS]" value="127"/>
                <list-param-item code="EC_DS_PKG_28" name="SOT89, SC62, TO243AA [EC_DS]" value="128"/>
                <list-param-item code="EC_DS_PKG_29" name="SOT194 [EC_DS]" value="129"/>
                <list-param-item code="EC_DS_PKG_30" name="TO218, ISOWATT218 [EC_DS]" value="130"/>
                <list-param-item code="EC_DS_PKG_31" name="TO220, TO220-5, ISOWATT220, TO220XX [EC_DS]" value="131"/>
                <list-param-item code="EC_DS_PKG_32" name="TO247, Max247, Super247, SOT429 [EC_DS]" value="132"/>
                <list-param-item code="EC_DS_PKG_33" name="ISOWATT [EC_DS]" value="133"/>
                <list-param-item code="EC_DS_PKG_34" name="DO220 [EC_DS]" value="134"/>
                <list-param-item code="EC_DS_PKG_35" name="IPACK, TO251AA [EC_DS]" value="135"/>
                <list-param-item code="EC_DS_PKG_36" name="SOT82, TO225 [EC_DS]" value="136"/>
                <list-param-item code="EC_DS_PKG_37" name="SOD6, DO214AA, SMB-J [EC_DS]" value="137"/>
                <list-param-item code="EC_DS_PKG_38" name="SOD15, DO214AB, SMC-J [EC_DS]" value="138"/>
                <list-param-item code="EC_DS_PKG_39" name="DPAK, TO252AA, SC63, SOT428 [EC_DS]" value="139"/>
                <list-param-item code="EC_DS_PKG_40" name="D2PAK, TO263, SC83A, SMD220 [EC_DS]" value="140"/>
                <list-param-item code="EC_DS_PKG_41" name="D3PAK, TO268 [EC_DS]" value="141"/>
                <list-param-item code="EC_DS_PKG_42" name="ISOTOP, SOT227, TO244, Half-Pak [EC_DS]" value="142"/>
                <list-param-item code="EC_DS_PKG_43" name="SOD80, Mini-MELF, DO213AA [EC_DS]" value="143"/>
                <list-param-item code="EC_DS_PKG_44" name="SOD87, MELF, DO213AB [EC_DS]" value="144"/>
                <list-param-item code="EC_DS_PKG_45" name="TO18, TO71, TO72, SOT31, SOT18 [EC_DS]" value="145"/>
                <list-param-item code="EC_DS_PKG_46" name="TO39, SOT5 [EC_DS]" value="146"/>
                <list-param-item code="EC_DS_PKG_47" name="TO52 [EC_DS]" value="147"/>
                <list-param-item code="EC_DS_PKG_48" name="SOT553 [EC_DS]" value="148"/>
                <list-param-item code="EC_DS_PKG_49" name="SOT563 [EC_DS]" value="149"/>
                <list-param-item code="EC_DS_PKG_50" name="SOT563F [EC_DS]" value="150"/>
                <list-param-item code="EC_DS_PKG_51" name="SOT663 [EC_DS]" value="151"/>
                <list-param-item code="EC_DS_PKG_52" name="SOT666 [EC_DS]" value="152"/>
                <list-param-item code="EC_DS_PKG_53" name="SOT66 [EC_DS]" value="153"/>
                <list-param-item code="EC_DS_PKG_54" name="SOT665 [EC_DS]" value="154"/>
                <list-param-item code="EC_DS_PKG_55" name="SOT490 [EC_DS]" value="155"/>
            </family-param>
            <family-param code="ec_ic_chip" name="Chip" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="EC_IC_CHIP_01" name="FPGA, CPLD, FPGA Antifuse, PAL" value="1"/>
                <list-param-item code="EC_IC_CHIP_02" name="Analog and mixed circuit (MOS, Bipolar, BiCMOS)" value="2"/>
                <list-param-item code="EC_IC_CHIP_03" name="Microprocessor, Microcontroller, DSP" value="3"/>
                <list-param-item code="EC_IC_CHIP_04" name="Flash, EEPROM, EPROM" value="4"/>
                <list-param-item code="EC_IC_CHIP_05" name="SRAM" value="5"/>
                <list-param-item code="EC_IC_CHIP_06" name="DRAM" value="6"/>
                <list-param-item code="EC_IC_CHIP_07" name="Digital circuit (MOS, Bipolar, BiCMOS)" value="7"/>
            </family-param>
            <family-param code="ec_np" name="Np" value-type="NUMERIC" optional="true" in-hmc="false"/>
            <family-param code="ec_underfill" name="Underfill" value-type="BOOL" optional="true" in-hmc="false"/>
            <app-stress code="ec_delta_t" name="ΔT" value-type="NUMERIC" unit="°C" optional="false" in-hmc="false"/>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="ec_asic" name="Application Specific Integrated Circuit">
            <family-param code="ec_icds_pkg" name="Package" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="EC_IC_PKG_01" name="PDIP [EC_IC]" value="1"/>
                <list-param-item code="EC_IC_PKG_02" name="CERDIP, CDIP [EC_IC]" value="2"/>
                <list-param-item code="EC_IC_PKG_03" name="PQFP [EC_IC]" value="3"/>
                <list-param-item code="EC_IC_PKG_04" name="TQFP, LQFP [EC_IC]" value="4"/>
                <list-param-item code="EC_IC_PKG_05" name="Power QFP [EC_IC]" value="5"/>
                <list-param-item code="EC_IC_PKG_06" name="CERPACK [EC_IC]" value="6"/>
                <list-param-item code="EC_IC_PKG_07" name="CQFP [EC_IC]" value="7"/>
                <list-param-item code="EC_IC_PKG_08" name="PLCC [EC_IC]" value="8"/>
                <list-param-item code="EC_IC_PKG_09" name="J-LCC [EC_IC]" value="9"/>
                <list-param-item code="EC_IC_PKG_10" name="CLCC [EC_IC]" value="10"/>
                <list-param-item code="EC_IC_PKG_11" name="SOJ [EC_IC]" value="11"/>
                <list-param-item code="EC_IC_PKG_12" name="SO [EC_IC]" value="12"/>
                <list-param-item code="EC_IC_PKG_13" name="TSOP [EC_IC]" value="13"/>
                <list-param-item code="EC_IC_PKG_14" name="SSOP, QSOP [EC_IC]" value="14"/>
                <list-param-item code="EC_IC_PKG_15" name="TSSOP, MSOP [EC_IC]" value="15"/>
                <list-param-item code="EC_IC_PKG_16" name="QFN, DFN ≥0.5 mm [EC_IC]" value="16"/>
                <list-param-item code="EC_IC_PKG_17" name="QFN 0.4 mm [EC_IC]" value="17"/>
                <list-param-item code="EC_IC_PKG_18" name="LGA Plastic [EC_IC]" value="18"/>
                <list-param-item code="EC_IC_PKG_19" name="PBGA &lt;0.5 mm [EC_IC]" value="19"/>
                <list-param-item code="EC_IC_PKG_20" name="PBGA 0.5 mm [EC_IC]" value="20"/>
                <list-param-item code="EC_IC_PKG_21" name="PBGA 0.65 mm [EC_IC]" value="21"/>
                <list-param-item code="EC_IC_PKG_22" name="PBGA BT 0.8 mm [EC_IC]" value="22"/>
                <list-param-item code="EC_IC_PKG_23" name="PBGA flex 0.8 mm [EC_IC]" value="23"/>
                <list-param-item code="EC_IC_PKG_24" name="PBGA BOC 0.8 mm (memories) [EC_IC]" value="24"/>
                <list-param-item code="EC_IC_PKG_25" name="PBGA BT 1.00 mm [EC_IC]" value="25"/>
                <list-param-item code="EC_IC_PKG_26" name="PBGA 1.27 mm [EC_IC]" value="26"/>
                <list-param-item code="EC_IC_PKG_27" name="Power BGA [EC_IC]" value="27"/>
                <list-param-item code="EC_IC_PKG_28" name="BGA WLP &lt;0.5 mm [EC_IC]" value="28"/>
                <list-param-item code="EC_IC_PKG_29" name="BGA WLP 0.5 mm [EC_IC]" value="29"/>
                <list-param-item code="EC_IC_PKG_30" name="FC-PBGA 0.8 mm [EC_IC]" value="30"/>
                <list-param-item code="EC_IC_PKG_31" name="FC-PBGA 1 mm [EC_IC]" value="31"/>
                <list-param-item code="EC_IC_PKG_32" name="CBGA [EC_IC]" value="32"/>
                <list-param-item code="EC_IC_PKG_33" name="DBGA [EC_IC]" value="33"/>
                <list-param-item code="EC_IC_PKG_34" name="CI CGA [EC_IC]" value="34"/>
                <list-param-item code="EC_IC_PKG_35" name="CPGA [EC_IC]" value="35"/>
                <list-param-item code="EC_DS_PKG_01" name="CB417 [EC_DS]" value="101"/>
                <list-param-item code="EC_DS_PKG_02" name="CB429 [EC_DS]" value="102"/>
                <list-param-item code="EC_DS_PKG_03" name="DO13, DO202AA [EC_DS]" value="103"/>
                <list-param-item code="EC_DS_PKG_04" name="DO15, DO204AC [EC_DS]" value="104"/>
                <list-param-item code="EC_DS_PKG_05" name="DO27, DO201AA [EC_DS]" value="105"/>
                <list-param-item code="EC_DS_PKG_06" name="DO35, DO204AH [EC_DS]" value="106"/>
                <list-param-item code="EC_DS_PKG_07" name="DO41, DO204AL [EC_DS]" value="107"/>
                <list-param-item code="EC_DS_PKG_08" name="DO92 [EC_DS]" value="108"/>
                <list-param-item code="EC_DS_PKG_09" name="F126 [EC_DS]" value="109"/>
                <list-param-item code="EC_DS_PKG_10" name="SIL, SIP, ZIP [EC_DS]" value="110"/>
                <list-param-item code="EC_DS_PKG_11" name="TO92, SOT54, SC43, TO226AA [EC_DS]" value="111"/>
                <list-param-item code="EC_DS_PKG_12" name="TO126, SOT32, TO225AA [EC_DS]" value="112"/>
                <list-param-item code="EC_DS_PKG_13" name="TO202 [EC_DS]" value="113"/>
                <list-param-item code="EC_DS_PKG_14" name="SOT23-3, TO236AB [EC_DS]" value="114"/>
                <list-param-item code="EC_DS_PKG_15" name="SOT23-5, SC74A, SOT25 [EC_DS]" value="115"/>
                <list-param-item code="EC_DS_PKG_16" name="SOT23-6, SC74, SOT26, SOT457 [EC_DS]" value="116"/>
                <list-param-item code="EC_DS_PKG_17" name="SOT143, TO253AA, SC61B [EC_DS]" value="117"/>
                <list-param-item code="EC_DS_PKG_18" name="SOT323, SC70 [EC_DS]" value="118"/>
                <list-param-item code="EC_DS_PKG_19" name="SOT346, SC59, TO236AA [EC_DS]" value="119"/>
                <list-param-item code="EC_DS_PKG_20" name="SOT353, SC70-5, SC88A [EC_DS]" value="120"/>
                <list-param-item code="EC_DS_PKG_21" name="SOT363, SC70-6, SC88 [EC_DS]" value="121"/>
                <list-param-item code="EC_DS_PKG_22" name="SOD123 [EC_DS]" value="122"/>
                <list-param-item code="EC_DS_PKG_23" name="SOD323, SC76 [EC_DS]" value="123"/>
                <list-param-item code="EC_DS_PKG_24" name="SOD523, SC79 [EC_DS]" value="124"/>
                <list-param-item code="EC_DS_PKG_25" name="SOT223, SC73, TO261AA [EC_DS]" value="125"/>
                <list-param-item code="EC_DS_PKG_26" name="SOT243 [EC_DS]" value="126"/>
                <list-param-item code="EC_DS_PKG_27" name="SOT343, SC82 [EC_DS]" value="127"/>
                <list-param-item code="EC_DS_PKG_28" name="SOT89, SC62, TO243AA [EC_DS]" value="128"/>
                <list-param-item code="EC_DS_PKG_29" name="SOT194 [EC_DS]" value="129"/>
                <list-param-item code="EC_DS_PKG_30" name="TO218, ISOWATT218 [EC_DS]" value="130"/>
                <list-param-item code="EC_DS_PKG_31" name="TO220, TO220-5, ISOWATT220, TO220XX [EC_DS]" value="131"/>
                <list-param-item code="EC_DS_PKG_32" name="TO247, Max247, Super247, SOT429 [EC_DS]" value="132"/>
                <list-param-item code="EC_DS_PKG_33" name="ISOWATT [EC_DS]" value="133"/>
                <list-param-item code="EC_DS_PKG_34" name="DO220 [EC_DS]" value="134"/>
                <list-param-item code="EC_DS_PKG_35" name="IPACK, TO251AA [EC_DS]" value="135"/>
                <list-param-item code="EC_DS_PKG_36" name="SOT82, TO225 [EC_DS]" value="136"/>
                <list-param-item code="EC_DS_PKG_37" name="SOD6, DO214AA, SMB-J [EC_DS]" value="137"/>
                <list-param-item code="EC_DS_PKG_38" name="SOD15, DO214AB, SMC-J [EC_DS]" value="138"/>
                <list-param-item code="EC_DS_PKG_39" name="DPAK, TO252AA, SC63, SOT428 [EC_DS]" value="139"/>
                <list-param-item code="EC_DS_PKG_40" name="D2PAK, TO263, SC83A, SMD220 [EC_DS]" value="140"/>
                <list-param-item code="EC_DS_PKG_41" name="D3PAK, TO268 [EC_DS]" value="141"/>
                <list-param-item code="EC_DS_PKG_42" name="ISOTOP, SOT227, TO244, Half-Pak [EC_DS]" value="142"/>
                <list-param-item code="EC_DS_PKG_43" name="SOD80, Mini-MELF, DO213AA [EC_DS]" value="143"/>
                <list-param-item code="EC_DS_PKG_44" name="SOD87, MELF, DO213AB [EC_DS]" value="144"/>
                <list-param-item code="EC_DS_PKG_45" name="TO18, TO71, TO72, SOT31, SOT18 [EC_DS]" value="145"/>
                <list-param-item code="EC_DS_PKG_46" name="TO39, SOT5 [EC_DS]" value="146"/>
                <list-param-item code="EC_DS_PKG_47" name="TO52 [EC_DS]" value="147"/>
                <list-param-item code="EC_DS_PKG_48" name="SOT553 [EC_DS]" value="148"/>
                <list-param-item code="EC_DS_PKG_49" name="SOT563 [EC_DS]" value="149"/>
                <list-param-item code="EC_DS_PKG_50" name="SOT563F [EC_DS]" value="150"/>
                <list-param-item code="EC_DS_PKG_51" name="SOT663 [EC_DS]" value="151"/>
                <list-param-item code="EC_DS_PKG_52" name="SOT666 [EC_DS]" value="152"/>
                <list-param-item code="EC_DS_PKG_53" name="SOT66 [EC_DS]" value="153"/>
                <list-param-item code="EC_DS_PKG_54" name="SOT665 [EC_DS]" value="154"/>
                <list-param-item code="EC_DS_PKG_55" name="SOT490 [EC_DS]" value="155"/>
            </family-param>
            <family-param code="ec_asic_chip" name="Chip" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="EC_ASIC_CHIP_01" name="Silicon MOS - Digital ASIC, simple function" value="1"/>
                <list-param-item code="EC_ASIC_CHIP_02"
                                 name="Silicon MOS - Digital ASIC, complex function (with IP and/or μP core, memory blocks)"
                                 value="2"/>
                <list-param-item code="EC_ASIC_CHIP_03" name="Silicon MOS - Analog, mixed ASIC" value="3"/>
                <list-param-item code="EC_ASIC_CHIP_04" name="Silicon bipolar, BICMOS - Digital ASIC" value="4"/>
                <list-param-item code="EC_ASIC_CHIP_05" name="Silicon bipolar, BICMOS - Mixed, analog ASIC" value="5"/>
            </family-param>
            <family-param code="ec_np" name="Np" value-type="NUMERIC" optional="true" in-hmc="false"/>
            <family-param code="ec_underfill" name="Underfill" value-type="BOOL" optional="true" in-hmc="false"/>
            <app-stress code="ec_delta_t" name="ΔT" value-type="NUMERIC" unit="°C" optional="false" in-hmc="false"/>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="ec_ds" name="Discrete semiconductors">
            <family-param code="ec_icds_pkg" name="Package" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="EC_IC_PKG_01" name="PDIP [EC_IC]" value="1"/>
                <list-param-item code="EC_IC_PKG_02" name="CERDIP, CDIP [EC_IC]" value="2"/>
                <list-param-item code="EC_IC_PKG_03" name="PQFP [EC_IC]" value="3"/>
                <list-param-item code="EC_IC_PKG_04" name="TQFP, LQFP [EC_IC]" value="4"/>
                <list-param-item code="EC_IC_PKG_05" name="Power QFP [EC_IC]" value="5"/>
                <list-param-item code="EC_IC_PKG_06" name="CERPACK [EC_IC]" value="6"/>
                <list-param-item code="EC_IC_PKG_07" name="CQFP [EC_IC]" value="7"/>
                <list-param-item code="EC_IC_PKG_08" name="PLCC [EC_IC]" value="8"/>
                <list-param-item code="EC_IC_PKG_09" name="J-LCC [EC_IC]" value="9"/>
                <list-param-item code="EC_IC_PKG_10" name="CLCC [EC_IC]" value="10"/>
                <list-param-item code="EC_IC_PKG_11" name="SOJ [EC_IC]" value="11"/>
                <list-param-item code="EC_IC_PKG_12" name="SO [EC_IC]" value="12"/>
                <list-param-item code="EC_IC_PKG_13" name="TSOP [EC_IC]" value="13"/>
                <list-param-item code="EC_IC_PKG_14" name="SSOP, QSOP [EC_IC]" value="14"/>
                <list-param-item code="EC_IC_PKG_15" name="TSSOP, MSOP [EC_IC]" value="15"/>
                <list-param-item code="EC_IC_PKG_16" name="QFN, DFN ≥0.5 mm [EC_IC]" value="16"/>
                <list-param-item code="EC_IC_PKG_17" name="QFN 0.4 mm [EC_IC]" value="17"/>
                <list-param-item code="EC_IC_PKG_18" name="LGA Plastic [EC_IC]" value="18"/>
                <list-param-item code="EC_IC_PKG_19" name="PBGA &lt;0.5 mm [EC_IC]" value="19"/>
                <list-param-item code="EC_IC_PKG_20" name="PBGA 0.5 mm [EC_IC]" value="20"/>
                <list-param-item code="EC_IC_PKG_21" name="PBGA 0.65 mm [EC_IC]" value="21"/>
                <list-param-item code="EC_IC_PKG_22" name="PBGA BT 0.8 mm [EC_IC]" value="22"/>
                <list-param-item code="EC_IC_PKG_23" name="PBGA flex 0.8 mm [EC_IC]" value="23"/>
                <list-param-item code="EC_IC_PKG_24" name="PBGA BOC 0.8 mm (memories) [EC_IC]" value="24"/>
                <list-param-item code="EC_IC_PKG_25" name="PBGA BT 1.00 mm [EC_IC]" value="25"/>
                <list-param-item code="EC_IC_PKG_26" name="PBGA 1.27 mm [EC_IC]" value="26"/>
                <list-param-item code="EC_IC_PKG_27" name="Power BGA [EC_IC]" value="27"/>
                <list-param-item code="EC_IC_PKG_28" name="BGA WLP &lt;0.5 mm [EC_IC]" value="28"/>
                <list-param-item code="EC_IC_PKG_29" name="BGA WLP 0.5 mm [EC_IC]" value="29"/>
                <list-param-item code="EC_IC_PKG_30" name="FC-PBGA 0.8 mm [EC_IC]" value="30"/>
                <list-param-item code="EC_IC_PKG_31" name="FC-PBGA 1 mm [EC_IC]" value="31"/>
                <list-param-item code="EC_IC_PKG_32" name="CBGA [EC_IC]" value="32"/>
                <list-param-item code="EC_IC_PKG_33" name="DBGA [EC_IC]" value="33"/>
                <list-param-item code="EC_IC_PKG_34" name="CI CGA [EC_IC]" value="34"/>
                <list-param-item code="EC_IC_PKG_35" name="CPGA [EC_IC]" value="35"/>
                <list-param-item code="EC_DS_PKG_01" name="CB417 [EC_DS]" value="101"/>
                <list-param-item code="EC_DS_PKG_02" name="CB429 [EC_DS]" value="102"/>
                <list-param-item code="EC_DS_PKG_03" name="DO13, DO202AA [EC_DS]" value="103"/>
                <list-param-item code="EC_DS_PKG_04" name="DO15, DO204AC [EC_DS]" value="104"/>
                <list-param-item code="EC_DS_PKG_05" name="DO27, DO201AA [EC_DS]" value="105"/>
                <list-param-item code="EC_DS_PKG_06" name="DO35, DO204AH [EC_DS]" value="106"/>
                <list-param-item code="EC_DS_PKG_07" name="DO41, DO204AL [EC_DS]" value="107"/>
                <list-param-item code="EC_DS_PKG_08" name="DO92 [EC_DS]" value="108"/>
                <list-param-item code="EC_DS_PKG_09" name="F126 [EC_DS]" value="109"/>
                <list-param-item code="EC_DS_PKG_10" name="SIL, SIP, ZIP [EC_DS]" value="110"/>
                <list-param-item code="EC_DS_PKG_11" name="TO92, SOT54, SC43, TO226AA [EC_DS]" value="111"/>
                <list-param-item code="EC_DS_PKG_12" name="TO126, SOT32, TO225AA [EC_DS]" value="112"/>
                <list-param-item code="EC_DS_PKG_13" name="TO202 [EC_DS]" value="113"/>
                <list-param-item code="EC_DS_PKG_14" name="SOT23-3, TO236AB [EC_DS]" value="114"/>
                <list-param-item code="EC_DS_PKG_15" name="SOT23-5, SC74A, SOT25 [EC_DS]" value="115"/>
                <list-param-item code="EC_DS_PKG_16" name="SOT23-6, SC74, SOT26, SOT457 [EC_DS]" value="116"/>
                <list-param-item code="EC_DS_PKG_17" name="SOT143, TO253AA, SC61B [EC_DS]" value="117"/>
                <list-param-item code="EC_DS_PKG_18" name="SOT323, SC70 [EC_DS]" value="118"/>
                <list-param-item code="EC_DS_PKG_19" name="SOT346, SC59, TO236AA [EC_DS]" value="119"/>
                <list-param-item code="EC_DS_PKG_20" name="SOT353, SC70-5, SC88A [EC_DS]" value="120"/>
                <list-param-item code="EC_DS_PKG_21" name="SOT363, SC70-6, SC88 [EC_DS]" value="121"/>
                <list-param-item code="EC_DS_PKG_22" name="SOD123 [EC_DS]" value="122"/>
                <list-param-item code="EC_DS_PKG_23" name="SOD323, SC76 [EC_DS]" value="123"/>
                <list-param-item code="EC_DS_PKG_24" name="SOD523, SC79 [EC_DS]" value="124"/>
                <list-param-item code="EC_DS_PKG_25" name="SOT223, SC73, TO261AA [EC_DS]" value="125"/>
                <list-param-item code="EC_DS_PKG_26" name="SOT243 [EC_DS]" value="126"/>
                <list-param-item code="EC_DS_PKG_27" name="SOT343, SC82 [EC_DS]" value="127"/>
                <list-param-item code="EC_DS_PKG_28" name="SOT89, SC62, TO243AA [EC_DS]" value="128"/>
                <list-param-item code="EC_DS_PKG_29" name="SOT194 [EC_DS]" value="129"/>
                <list-param-item code="EC_DS_PKG_30" name="TO218, ISOWATT218 [EC_DS]" value="130"/>
                <list-param-item code="EC_DS_PKG_31" name="TO220, TO220-5, ISOWATT220, TO220XX [EC_DS]" value="131"/>
                <list-param-item code="EC_DS_PKG_32" name="TO247, Max247, Super247, SOT429 [EC_DS]" value="132"/>
                <list-param-item code="EC_DS_PKG_33" name="ISOWATT [EC_DS]" value="133"/>
                <list-param-item code="EC_DS_PKG_34" name="DO220 [EC_DS]" value="134"/>
                <list-param-item code="EC_DS_PKG_35" name="IPACK, TO251AA [EC_DS]" value="135"/>
                <list-param-item code="EC_DS_PKG_36" name="SOT82, TO225 [EC_DS]" value="136"/>
                <list-param-item code="EC_DS_PKG_37" name="SOD6, DO214AA, SMB-J [EC_DS]" value="137"/>
                <list-param-item code="EC_DS_PKG_38" name="SOD15, DO214AB, SMC-J [EC_DS]" value="138"/>
                <list-param-item code="EC_DS_PKG_39" name="DPAK, TO252AA, SC63, SOT428 [EC_DS]" value="139"/>
                <list-param-item code="EC_DS_PKG_40" name="D2PAK, TO263, SC83A, SMD220 [EC_DS]" value="140"/>
                <list-param-item code="EC_DS_PKG_41" name="D3PAK, TO268 [EC_DS]" value="141"/>
                <list-param-item code="EC_DS_PKG_42" name="ISOTOP, SOT227, TO244, Half-Pak [EC_DS]" value="142"/>
                <list-param-item code="EC_DS_PKG_43" name="SOD80, Mini-MELF, DO213AA [EC_DS]" value="143"/>
                <list-param-item code="EC_DS_PKG_44" name="SOD87, MELF, DO213AB [EC_DS]" value="144"/>
                <list-param-item code="EC_DS_PKG_45" name="TO18, TO71, TO72, SOT31, SOT18 [EC_DS]" value="145"/>
                <list-param-item code="EC_DS_PKG_46" name="TO39, SOT5 [EC_DS]" value="146"/>
                <list-param-item code="EC_DS_PKG_47" name="TO52 [EC_DS]" value="147"/>
                <list-param-item code="EC_DS_PKG_48" name="SOT553 [EC_DS]" value="148"/>
                <list-param-item code="EC_DS_PKG_49" name="SOT563 [EC_DS]" value="149"/>
                <list-param-item code="EC_DS_PKG_50" name="SOT563F [EC_DS]" value="150"/>
                <list-param-item code="EC_DS_PKG_51" name="SOT663 [EC_DS]" value="151"/>
                <list-param-item code="EC_DS_PKG_52" name="SOT666 [EC_DS]" value="152"/>
                <list-param-item code="EC_DS_PKG_53" name="SOT66 [EC_DS]" value="153"/>
                <list-param-item code="EC_DS_PKG_54" name="SOT665 [EC_DS]" value="154"/>
                <list-param-item code="EC_DS_PKG_55" name="SOT490 [EC_DS]" value="155"/>
            </family-param>
            <family-param code="ec_np" name="Np" value-type="NUMERIC" optional="true" in-hmc="false"/>
            <family-param code="ec_underfill" name="Underfill" value-type="BOOL" optional="true" in-hmc="false"/>
            <family-param code="ec_ds_chip" name="Chip" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="EC_DS_CHIP_01" name="Signal diodes up to 1A (PIN, Schottky,signal, varactor)"
                                 value="1"/>
                <list-param-item code="EC_DS_CHIP_02" name="Rectifier diodes 1A to 3A" value="2"/>
                <list-param-item code="EC_DS_CHIP_03" name="Zener regulation diodes up to 1.5W" value="3"/>
                <list-param-item code="EC_DS_CHIP_04" name="Protection diodes up to 3kW (peak 10ms/ 100ms) (TVS)"
                                 value="4"/>
                <list-param-item code="EC_DS_CHIP_05" name="Silicon, bipolar &lt; 5W" value="5"/>
                <list-param-item code="EC_DS_CHIP_06" name="Silicon, MOS &lt; 5W" value="6"/>
                <list-param-item code="EC_DS_CHIP_07" name="Silicon, JFET &lt; 5W" value="7"/>
                <list-param-item code="EC_DS_CHIP_08" name="Thyristors, triacs over 3A" value="8"/>
                <list-param-item code="EC_DS_CHIP_09" name="Rectifier diodes &gt; 3A" value="9"/>
                <list-param-item code="EC_DS_CHIP_10" name="Zener regulation diodes over 1.5W" value="10"/>
                <list-param-item code="EC_DS_CHIP_11" name="Protection diodes over 3kW (peak 10ms / 100ms) (TVS)"
                                 value="11"/>
                <list-param-item code="EC_DS_CHIP_12" name="Silicon, bipolar &gt; 5W" value="12"/>
            </family-param>
            <family-param code="ec_elmt_nb" name="Nb elements" value-type="NUMERIC" optional="false" in-hmc="false"/>
            <family-param code="ec_v_rated" name="V_rated" value-type="NUMERIC" unit="V" optional="false"
                          in-hmc="false"/>
            <app-stress code="ec_v_appl" name="V_applied" value-type="NUMERIC" unit="V" optional="false"
                        in-hmc="false"/>
            <app-stress code="ec_delta_t" name="ΔT" value-type="NUMERIC" unit="°C" optional="false" in-hmc="false"/>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="ec_dps" name="Discrete power semiconductors">
            <family-param code="ec_icds_pkg" name="Package" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="EC_IC_PKG_01" name="PDIP [EC_IC]" value="1"/>
                <list-param-item code="EC_IC_PKG_02" name="CERDIP, CDIP [EC_IC]" value="2"/>
                <list-param-item code="EC_IC_PKG_03" name="PQFP [EC_IC]" value="3"/>
                <list-param-item code="EC_IC_PKG_04" name="TQFP, LQFP [EC_IC]" value="4"/>
                <list-param-item code="EC_IC_PKG_05" name="Power QFP [EC_IC]" value="5"/>
                <list-param-item code="EC_IC_PKG_06" name="CERPACK [EC_IC]" value="6"/>
                <list-param-item code="EC_IC_PKG_07" name="CQFP [EC_IC]" value="7"/>
                <list-param-item code="EC_IC_PKG_08" name="PLCC [EC_IC]" value="8"/>
                <list-param-item code="EC_IC_PKG_09" name="J-LCC [EC_IC]" value="9"/>
                <list-param-item code="EC_IC_PKG_10" name="CLCC [EC_IC]" value="10"/>
                <list-param-item code="EC_IC_PKG_11" name="SOJ [EC_IC]" value="11"/>
                <list-param-item code="EC_IC_PKG_12" name="SO [EC_IC]" value="12"/>
                <list-param-item code="EC_IC_PKG_13" name="TSOP [EC_IC]" value="13"/>
                <list-param-item code="EC_IC_PKG_14" name="SSOP, QSOP [EC_IC]" value="14"/>
                <list-param-item code="EC_IC_PKG_15" name="TSSOP, MSOP [EC_IC]" value="15"/>
                <list-param-item code="EC_IC_PKG_16" name="QFN, DFN ≥0.5 mm [EC_IC]" value="16"/>
                <list-param-item code="EC_IC_PKG_17" name="QFN 0.4 mm [EC_IC]" value="17"/>
                <list-param-item code="EC_IC_PKG_18" name="LGA Plastic [EC_IC]" value="18"/>
                <list-param-item code="EC_IC_PKG_19" name="PBGA &lt;0.5 mm [EC_IC]" value="19"/>
                <list-param-item code="EC_IC_PKG_20" name="PBGA 0.5 mm [EC_IC]" value="20"/>
                <list-param-item code="EC_IC_PKG_21" name="PBGA 0.65 mm [EC_IC]" value="21"/>
                <list-param-item code="EC_IC_PKG_22" name="PBGA BT 0.8 mm [EC_IC]" value="22"/>
                <list-param-item code="EC_IC_PKG_23" name="PBGA flex 0.8 mm [EC_IC]" value="23"/>
                <list-param-item code="EC_IC_PKG_24" name="PBGA BOC 0.8 mm (memories) [EC_IC]" value="24"/>
                <list-param-item code="EC_IC_PKG_25" name="PBGA BT 1.00 mm [EC_IC]" value="25"/>
                <list-param-item code="EC_IC_PKG_26" name="PBGA 1.27 mm [EC_IC]" value="26"/>
                <list-param-item code="EC_IC_PKG_27" name="Power BGA [EC_IC]" value="27"/>
                <list-param-item code="EC_IC_PKG_28" name="BGA WLP &lt;0.5 mm [EC_IC]" value="28"/>
                <list-param-item code="EC_IC_PKG_29" name="BGA WLP 0.5 mm [EC_IC]" value="29"/>
                <list-param-item code="EC_IC_PKG_30" name="FC-PBGA 0.8 mm [EC_IC]" value="30"/>
                <list-param-item code="EC_IC_PKG_31" name="FC-PBGA 1 mm [EC_IC]" value="31"/>
                <list-param-item code="EC_IC_PKG_32" name="CBGA [EC_IC]" value="32"/>
                <list-param-item code="EC_IC_PKG_33" name="DBGA [EC_IC]" value="33"/>
                <list-param-item code="EC_IC_PKG_34" name="CI CGA [EC_IC]" value="34"/>
                <list-param-item code="EC_IC_PKG_35" name="CPGA [EC_IC]" value="35"/>
                <list-param-item code="EC_DS_PKG_01" name="CB417 [EC_DS]" value="101"/>
                <list-param-item code="EC_DS_PKG_02" name="CB429 [EC_DS]" value="102"/>
                <list-param-item code="EC_DS_PKG_03" name="DO13, DO202AA [EC_DS]" value="103"/>
                <list-param-item code="EC_DS_PKG_04" name="DO15, DO204AC [EC_DS]" value="104"/>
                <list-param-item code="EC_DS_PKG_05" name="DO27, DO201AA [EC_DS]" value="105"/>
                <list-param-item code="EC_DS_PKG_06" name="DO35, DO204AH [EC_DS]" value="106"/>
                <list-param-item code="EC_DS_PKG_07" name="DO41, DO204AL [EC_DS]" value="107"/>
                <list-param-item code="EC_DS_PKG_08" name="DO92 [EC_DS]" value="108"/>
                <list-param-item code="EC_DS_PKG_09" name="F126 [EC_DS]" value="109"/>
                <list-param-item code="EC_DS_PKG_10" name="SIL, SIP, ZIP [EC_DS]" value="110"/>
                <list-param-item code="EC_DS_PKG_11" name="TO92, SOT54, SC43, TO226AA [EC_DS]" value="111"/>
                <list-param-item code="EC_DS_PKG_12" name="TO126, SOT32, TO225AA [EC_DS]" value="112"/>
                <list-param-item code="EC_DS_PKG_13" name="TO202 [EC_DS]" value="113"/>
                <list-param-item code="EC_DS_PKG_14" name="SOT23-3, TO236AB [EC_DS]" value="114"/>
                <list-param-item code="EC_DS_PKG_15" name="SOT23-5, SC74A, SOT25 [EC_DS]" value="115"/>
                <list-param-item code="EC_DS_PKG_16" name="SOT23-6, SC74, SOT26, SOT457 [EC_DS]" value="116"/>
                <list-param-item code="EC_DS_PKG_17" name="SOT143, TO253AA, SC61B [EC_DS]" value="117"/>
                <list-param-item code="EC_DS_PKG_18" name="SOT323, SC70 [EC_DS]" value="118"/>
                <list-param-item code="EC_DS_PKG_19" name="SOT346, SC59, TO236AA [EC_DS]" value="119"/>
                <list-param-item code="EC_DS_PKG_20" name="SOT353, SC70-5, SC88A [EC_DS]" value="120"/>
                <list-param-item code="EC_DS_PKG_21" name="SOT363, SC70-6, SC88 [EC_DS]" value="121"/>
                <list-param-item code="EC_DS_PKG_22" name="SOD123 [EC_DS]" value="122"/>
                <list-param-item code="EC_DS_PKG_23" name="SOD323, SC76 [EC_DS]" value="123"/>
                <list-param-item code="EC_DS_PKG_24" name="SOD523, SC79 [EC_DS]" value="124"/>
                <list-param-item code="EC_DS_PKG_25" name="SOT223, SC73, TO261AA [EC_DS]" value="125"/>
                <list-param-item code="EC_DS_PKG_26" name="SOT243 [EC_DS]" value="126"/>
                <list-param-item code="EC_DS_PKG_27" name="SOT343, SC82 [EC_DS]" value="127"/>
                <list-param-item code="EC_DS_PKG_28" name="SOT89, SC62, TO243AA [EC_DS]" value="128"/>
                <list-param-item code="EC_DS_PKG_29" name="SOT194 [EC_DS]" value="129"/>
                <list-param-item code="EC_DS_PKG_30" name="TO218, ISOWATT218 [EC_DS]" value="130"/>
                <list-param-item code="EC_DS_PKG_31" name="TO220, TO220-5, ISOWATT220, TO220XX [EC_DS]" value="131"/>
                <list-param-item code="EC_DS_PKG_32" name="TO247, Max247, Super247, SOT429 [EC_DS]" value="132"/>
                <list-param-item code="EC_DS_PKG_33" name="ISOWATT [EC_DS]" value="133"/>
                <list-param-item code="EC_DS_PKG_34" name="DO220 [EC_DS]" value="134"/>
                <list-param-item code="EC_DS_PKG_35" name="IPACK, TO251AA [EC_DS]" value="135"/>
                <list-param-item code="EC_DS_PKG_36" name="SOT82, TO225 [EC_DS]" value="136"/>
                <list-param-item code="EC_DS_PKG_37" name="SOD6, DO214AA, SMB-J [EC_DS]" value="137"/>
                <list-param-item code="EC_DS_PKG_38" name="SOD15, DO214AB, SMC-J [EC_DS]" value="138"/>
                <list-param-item code="EC_DS_PKG_39" name="DPAK, TO252AA, SC63, SOT428 [EC_DS]" value="139"/>
                <list-param-item code="EC_DS_PKG_40" name="D2PAK, TO263, SC83A, SMD220 [EC_DS]" value="140"/>
                <list-param-item code="EC_DS_PKG_41" name="D3PAK, TO268 [EC_DS]" value="141"/>
                <list-param-item code="EC_DS_PKG_42" name="ISOTOP, SOT227, TO244, Half-Pak [EC_DS]" value="142"/>
                <list-param-item code="EC_DS_PKG_43" name="SOD80, Mini-MELF, DO213AA [EC_DS]" value="143"/>
                <list-param-item code="EC_DS_PKG_44" name="SOD87, MELF, DO213AB [EC_DS]" value="144"/>
                <list-param-item code="EC_DS_PKG_45" name="TO18, TO71, TO72, SOT31, SOT18 [EC_DS]" value="145"/>
                <list-param-item code="EC_DS_PKG_46" name="TO39, SOT5 [EC_DS]" value="146"/>
                <list-param-item code="EC_DS_PKG_47" name="TO52 [EC_DS]" value="147"/>
                <list-param-item code="EC_DS_PKG_48" name="SOT553 [EC_DS]" value="148"/>
                <list-param-item code="EC_DS_PKG_49" name="SOT563 [EC_DS]" value="149"/>
                <list-param-item code="EC_DS_PKG_50" name="SOT563F [EC_DS]" value="150"/>
                <list-param-item code="EC_DS_PKG_51" name="SOT663 [EC_DS]" value="151"/>
                <list-param-item code="EC_DS_PKG_52" name="SOT666 [EC_DS]" value="152"/>
                <list-param-item code="EC_DS_PKG_53" name="SOT66 [EC_DS]" value="153"/>
                <list-param-item code="EC_DS_PKG_54" name="SOT665 [EC_DS]" value="154"/>
                <list-param-item code="EC_DS_PKG_55" name="SOT490 [EC_DS]" value="155"/>
            </family-param>
            <family-param code="ec_dps_chip" name="Chip" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="EC_DPS_CHIP_01" name="Silicon, MOS &gt; 5W" value="1"/>
                <list-param-item code="EC_DPS_CHIP_02" name="IGBT" value="2"/>
            </family-param>
            <family-param code="ec_np" name="Np" value-type="NUMERIC" optional="true" in-hmc="false"/>
            <family-param code="ec_underfill" name="Underfill" value-type="BOOL" optional="true" in-hmc="false"/>
            <family-param code="ec_elmt_nb" name="Nb elements" value-type="NUMERIC" optional="false" in-hmc="false"/>
            <app-stress code="ec_delta_t" name="ΔT" value-type="NUMERIC" unit="°C" optional="false" in-hmc="false"/>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="ec_led" name="Light-emitting diodes">
            <family-param code="ec_led_pkg" name="Type" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="EC_LED_PKG_TYPE_01"
                                 name="If_max &lt; 150mA / Through-hole / T1-x / Plastic / 2 to 4 pins" value="1"/>
                <list-param-item code="EC_LED_PKG_TYPE_02"
                                 name="If_max &lt; 150mA / Through-hole / High flux / Plastic / 4 pins" value="2"/>
                <list-param-item code="EC_LED_PKG_TYPE_03" name="If_max &lt; 150mA / SMD / Chip / Plastic / 2 pins"
                                 value="3"/>
                <list-param-item code="EC_LED_PKG_TYPE_04" name="If_max &lt; 150mA / SMD / PLCC / Plastic / Mini 2 pins"
                                 value="4"/>
                <list-param-item code="EC_LED_PKG_TYPE_05" name="If_max &lt; 150mA / SMD / PLCC / Plastic / 2 pins"
                                 value="5"/>
                <list-param-item code="EC_LED_PKG_TYPE_06" name="If_max &lt; 150mA / SMD / PLCC / Plastic / 3 pins"
                                 value="6"/>
                <list-param-item code="EC_LED_PKG_TYPE_07" name="If_max &lt; 150mA / SMD / PLCC / Plastic / 4 pins"
                                 value="7"/>
                <list-param-item code="EC_LED_PKG_TYPE_08" name="If_max &lt; 150mA / SMD / PLCC / Plastic / 6 pins"
                                 value="8"/>
                <list-param-item code="EC_LED_PKG_TYPE_09" name="If_max &lt; 150mA / SMD / Round / Plastic / 2 pins"
                                 value="9"/>
                <list-param-item code="EC_LED_PKG_TYPE_10" name="If_max &lt; 150mA / SMD / LGA / Plastic / 2 pins"
                                 value="10"/>
                <list-param-item code="EC_LED_PKG_TYPE_11" name="If_max &lt; 150mA / SMD / LGA / Ceramic / 2 pins"
                                 value="11"/>
                <list-param-item code="EC_LED_PKG_TYPE_12" name="If_max &lt; 150mA / SMD / Plastic" value="12"/>
                <list-param-item code="EC_LED_PKG_TYPE_13" name="If_max &lt; 150mA / SMD / Ceramic" value="13"/>
                <list-param-item code="EC_LED_PKG_TYPE_14" name="If_max ≥ 150mA / SMD / Plastic" value="14"/>
                <list-param-item code="EC_LED_PKG_TYPE_15" name="If_max ≥ 150mA / SMD / Ceramic" value="15"/>
            </family-param>
            <family-param code="ec_color" name="Color" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="EC_LED_COLOR_01" name="COLOUR" value="1"/>
                <list-param-item code="EC_LED_COLOR_02" name="WHITE" value="2"/>
            </family-param>
            <family-param code="ec_elmt_nb" name="Nb elements" value-type="NUMERIC" optional="false" in-hmc="false"/>
            <app-stress code="ec_delta_t" name="ΔT" value-type="NUMERIC" unit="°C" optional="false" in-hmc="false"/>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="ec_op" name="Optocouplers">
            <family-param code="ec_icds_pkg" name="Package" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="EC_IC_PKG_01" name="PDIP [EC_IC]" value="1"/>
                <list-param-item code="EC_IC_PKG_02" name="CERDIP, CDIP [EC_IC]" value="2"/>
                <list-param-item code="EC_IC_PKG_03" name="PQFP [EC_IC]" value="3"/>
                <list-param-item code="EC_IC_PKG_04" name="TQFP, LQFP [EC_IC]" value="4"/>
                <list-param-item code="EC_IC_PKG_05" name="Power QFP [EC_IC]" value="5"/>
                <list-param-item code="EC_IC_PKG_06" name="CERPACK [EC_IC]" value="6"/>
                <list-param-item code="EC_IC_PKG_07" name="CQFP [EC_IC]" value="7"/>
                <list-param-item code="EC_IC_PKG_08" name="PLCC [EC_IC]" value="8"/>
                <list-param-item code="EC_IC_PKG_09" name="J-LCC [EC_IC]" value="9"/>
                <list-param-item code="EC_IC_PKG_10" name="CLCC [EC_IC]" value="10"/>
                <list-param-item code="EC_IC_PKG_11" name="SOJ [EC_IC]" value="11"/>
                <list-param-item code="EC_IC_PKG_12" name="SO [EC_IC]" value="12"/>
                <list-param-item code="EC_IC_PKG_13" name="TSOP [EC_IC]" value="13"/>
                <list-param-item code="EC_IC_PKG_14" name="SSOP, QSOP [EC_IC]" value="14"/>
                <list-param-item code="EC_IC_PKG_15" name="TSSOP, MSOP [EC_IC]" value="15"/>
                <list-param-item code="EC_IC_PKG_16" name="QFN, DFN ≥0.5 mm [EC_IC]" value="16"/>
                <list-param-item code="EC_IC_PKG_17" name="QFN 0.4 mm [EC_IC]" value="17"/>
                <list-param-item code="EC_IC_PKG_18" name="LGA Plastic [EC_IC]" value="18"/>
                <list-param-item code="EC_IC_PKG_19" name="PBGA &lt;0.5 mm [EC_IC]" value="19"/>
                <list-param-item code="EC_IC_PKG_20" name="PBGA 0.5 mm [EC_IC]" value="20"/>
                <list-param-item code="EC_IC_PKG_21" name="PBGA 0.65 mm [EC_IC]" value="21"/>
                <list-param-item code="EC_IC_PKG_22" name="PBGA BT 0.8 mm [EC_IC]" value="22"/>
                <list-param-item code="EC_IC_PKG_23" name="PBGA flex 0.8 mm [EC_IC]" value="23"/>
                <list-param-item code="EC_IC_PKG_24" name="PBGA BOC 0.8 mm (memories) [EC_IC]" value="24"/>
                <list-param-item code="EC_IC_PKG_25" name="PBGA BT 1.00 mm [EC_IC]" value="25"/>
                <list-param-item code="EC_IC_PKG_26" name="PBGA 1.27 mm [EC_IC]" value="26"/>
                <list-param-item code="EC_IC_PKG_27" name="Power BGA [EC_IC]" value="27"/>
                <list-param-item code="EC_IC_PKG_28" name="BGA WLP &lt;0.5 mm [EC_IC]" value="28"/>
                <list-param-item code="EC_IC_PKG_29" name="BGA WLP 0.5 mm [EC_IC]" value="29"/>
                <list-param-item code="EC_IC_PKG_30" name="FC-PBGA 0.8 mm [EC_IC]" value="30"/>
                <list-param-item code="EC_IC_PKG_31" name="FC-PBGA 1 mm [EC_IC]" value="31"/>
                <list-param-item code="EC_IC_PKG_32" name="CBGA [EC_IC]" value="32"/>
                <list-param-item code="EC_IC_PKG_33" name="DBGA [EC_IC]" value="33"/>
                <list-param-item code="EC_IC_PKG_34" name="CI CGA [EC_IC]" value="34"/>
                <list-param-item code="EC_IC_PKG_35" name="CPGA [EC_IC]" value="35"/>
                <list-param-item code="EC_DS_PKG_01" name="CB417 [EC_DS]" value="101"/>
                <list-param-item code="EC_DS_PKG_02" name="CB429 [EC_DS]" value="102"/>
                <list-param-item code="EC_DS_PKG_03" name="DO13, DO202AA [EC_DS]" value="103"/>
                <list-param-item code="EC_DS_PKG_04" name="DO15, DO204AC [EC_DS]" value="104"/>
                <list-param-item code="EC_DS_PKG_05" name="DO27, DO201AA [EC_DS]" value="105"/>
                <list-param-item code="EC_DS_PKG_06" name="DO35, DO204AH [EC_DS]" value="106"/>
                <list-param-item code="EC_DS_PKG_07" name="DO41, DO204AL [EC_DS]" value="107"/>
                <list-param-item code="EC_DS_PKG_08" name="DO92 [EC_DS]" value="108"/>
                <list-param-item code="EC_DS_PKG_09" name="F126 [EC_DS]" value="109"/>
                <list-param-item code="EC_DS_PKG_10" name="SIL, SIP, ZIP [EC_DS]" value="110"/>
                <list-param-item code="EC_DS_PKG_11" name="TO92, SOT54, SC43, TO226AA [EC_DS]" value="111"/>
                <list-param-item code="EC_DS_PKG_12" name="TO126, SOT32, TO225AA [EC_DS]" value="112"/>
                <list-param-item code="EC_DS_PKG_13" name="TO202 [EC_DS]" value="113"/>
                <list-param-item code="EC_DS_PKG_14" name="SOT23-3, TO236AB [EC_DS]" value="114"/>
                <list-param-item code="EC_DS_PKG_15" name="SOT23-5, SC74A, SOT25 [EC_DS]" value="115"/>
                <list-param-item code="EC_DS_PKG_16" name="SOT23-6, SC74, SOT26, SOT457 [EC_DS]" value="116"/>
                <list-param-item code="EC_DS_PKG_17" name="SOT143, TO253AA, SC61B [EC_DS]" value="117"/>
                <list-param-item code="EC_DS_PKG_18" name="SOT323, SC70 [EC_DS]" value="118"/>
                <list-param-item code="EC_DS_PKG_19" name="SOT346, SC59, TO236AA [EC_DS]" value="119"/>
                <list-param-item code="EC_DS_PKG_20" name="SOT353, SC70-5, SC88A [EC_DS]" value="120"/>
                <list-param-item code="EC_DS_PKG_21" name="SOT363, SC70-6, SC88 [EC_DS]" value="121"/>
                <list-param-item code="EC_DS_PKG_22" name="SOD123 [EC_DS]" value="122"/>
                <list-param-item code="EC_DS_PKG_23" name="SOD323, SC76 [EC_DS]" value="123"/>
                <list-param-item code="EC_DS_PKG_24" name="SOD523, SC79 [EC_DS]" value="124"/>
                <list-param-item code="EC_DS_PKG_25" name="SOT223, SC73, TO261AA [EC_DS]" value="125"/>
                <list-param-item code="EC_DS_PKG_26" name="SOT243 [EC_DS]" value="126"/>
                <list-param-item code="EC_DS_PKG_27" name="SOT343, SC82 [EC_DS]" value="127"/>
                <list-param-item code="EC_DS_PKG_28" name="SOT89, SC62, TO243AA [EC_DS]" value="128"/>
                <list-param-item code="EC_DS_PKG_29" name="SOT194 [EC_DS]" value="129"/>
                <list-param-item code="EC_DS_PKG_30" name="TO218, ISOWATT218 [EC_DS]" value="130"/>
                <list-param-item code="EC_DS_PKG_31" name="TO220, TO220-5, ISOWATT220, TO220XX [EC_DS]" value="131"/>
                <list-param-item code="EC_DS_PKG_32" name="TO247, Max247, Super247, SOT429 [EC_DS]" value="132"/>
                <list-param-item code="EC_DS_PKG_33" name="ISOWATT [EC_DS]" value="133"/>
                <list-param-item code="EC_DS_PKG_34" name="DO220 [EC_DS]" value="134"/>
                <list-param-item code="EC_DS_PKG_35" name="IPACK, TO251AA [EC_DS]" value="135"/>
                <list-param-item code="EC_DS_PKG_36" name="SOT82, TO225 [EC_DS]" value="136"/>
                <list-param-item code="EC_DS_PKG_37" name="SOD6, DO214AA, SMB-J [EC_DS]" value="137"/>
                <list-param-item code="EC_DS_PKG_38" name="SOD15, DO214AB, SMC-J [EC_DS]" value="138"/>
                <list-param-item code="EC_DS_PKG_39" name="DPAK, TO252AA, SC63, SOT428 [EC_DS]" value="139"/>
                <list-param-item code="EC_DS_PKG_40" name="D2PAK, TO263, SC83A, SMD220 [EC_DS]" value="140"/>
                <list-param-item code="EC_DS_PKG_41" name="D3PAK, TO268 [EC_DS]" value="141"/>
                <list-param-item code="EC_DS_PKG_42" name="ISOTOP, SOT227, TO244, Half-Pak [EC_DS]" value="142"/>
                <list-param-item code="EC_DS_PKG_43" name="SOD80, Mini-MELF, DO213AA [EC_DS]" value="143"/>
                <list-param-item code="EC_DS_PKG_44" name="SOD87, MELF, DO213AB [EC_DS]" value="144"/>
                <list-param-item code="EC_DS_PKG_45" name="TO18, TO71, TO72, SOT31, SOT18 [EC_DS]" value="145"/>
                <list-param-item code="EC_DS_PKG_46" name="TO39, SOT5 [EC_DS]" value="146"/>
                <list-param-item code="EC_DS_PKG_47" name="TO52 [EC_DS]" value="147"/>
                <list-param-item code="EC_DS_PKG_48" name="SOT553 [EC_DS]" value="148"/>
                <list-param-item code="EC_DS_PKG_49" name="SOT563 [EC_DS]" value="149"/>
                <list-param-item code="EC_DS_PKG_50" name="SOT563F [EC_DS]" value="150"/>
                <list-param-item code="EC_DS_PKG_51" name="SOT663 [EC_DS]" value="151"/>
                <list-param-item code="EC_DS_PKG_52" name="SOT666 [EC_DS]" value="152"/>
                <list-param-item code="EC_DS_PKG_53" name="SOT66 [EC_DS]" value="153"/>
                <list-param-item code="EC_DS_PKG_54" name="SOT665 [EC_DS]" value="154"/>
                <list-param-item code="EC_DS_PKG_55" name="SOT490 [EC_DS]" value="155"/>
            </family-param>
            <family-param code="ec_np" name="Np" value-type="NUMERIC" optional="true" in-hmc="false"/>
            <family-param code="ec_underfill" name="Underfill" value-type="BOOL" optional="true" in-hmc="false"/>
            <family-param code="ec_op_type" name="Type" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="EC_OP_TYPE_01" name="Photodiode optocoupler" value="1"/>
                <list-param-item code="EC_OP_TYPE_02" name="Phototransistor optocoupler" value="2"/>
            </family-param>
            <family-param code="ec_elmt_nb" name="Nb elements" value-type="NUMERIC" optional="false" in-hmc="false"/>
            <app-stress code="ec_delta_t" name="ΔT" value-type="NUMERIC" unit="°C" optional="false" in-hmc="false"/>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="ec_re" name="Resistors">
            <family-param code="ec_re_type" name="Type" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="EC_RE_TYPE_01"
                                 name="&quot;MiniMELF&quot; fixed resistor, low-power, thin film, current use (RC), high-stability (RS)"
                                 value="1"/>
                <list-param-item code="EC_RE_TYPE_02" name="Fixed resistor, high-power (≥1W), thick film" value="2"/>
                <list-param-item code="EC_RE_TYPE_03" name="Fixed resistor, low-power, wirewound, precision" value="3"/>
                <list-param-item code="EC_RE_TYPE_04" name="Fixed resistor, high-power (≥1W), wirewound" value="4"/>
                <list-param-item code="EC_RE_TYPE_05" name="Potentiometer, non-wirewound" value="5"/>
                <list-param-item code="EC_RE_TYPE_06" name="Fixed resistor, SMD, thick film" value="6"/>
                <list-param-item code="EC_RE_TYPE_07" name="Resistor network, SMD" value="7"/>
                <list-param-item code="EC_RE_TYPE_08" name="Fixed resistor, thin film, precision, high-stability (SMD)"
                                 value="8"/>
            </family-param>
            <family-param code="ec_smd_thl" name="SMD/Through hole" value-type="LIST" optional="true" in-hmc="false">
                <list-param-item code="EC_SMD_THL_01" name="SMD" value="1"/>
                <list-param-item code="EC_SMD_THL_02" name="Through-hole" value="2"/>
            </family-param>
            <family-param code="ec_ohm" name="Ohm" value-type="NUMERIC" unit="kΩ" optional="true" in-hmc="false"/>
            <family-param code="ec_elmt_nb" name="Nb elements" value-type="NUMERIC" optional="true" in-hmc="false"/>
            <family-param code="ec_p_rated" name="P_rated" value-type="NUMERIC" unit="W" optional="false"
                          in-hmc="false"/>
            <app-stress code="ec_p_appl" name="P_applied" value-type="NUMERIC" unit="W" optional="false"
                        in-hmc="false"/>
            <family-param code="hmc_mount_type" name="Mount type (H&amp;M)" value-type="LIST" optional="false"
                          in-hmc="true">
                <list-param-item code="HMC_MOUNT_TYPE_01" name="By gluing (conductive glue)" value="1"/>
                <list-param-item code="HMC_MOUNT_TYPE_02" name="By soldering (solder)" value="2"/>
            </family-param>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="ec_fu" name="Fuses">
            <family-param code="ec_i_rated" name="I_rated" value-type="NUMERIC" unit="A" optional="false"
                          in-hmc="false"/>
            <app-stress code="ec_i_appl" name="I_applied" value-type="NUMERIC" unit="A" optional="false"
                        in-hmc="false"/>
            <family-param code="hmc_mount_type" name="Mount type (H&amp;M)" value-type="LIST" optional="false"
                          in-hmc="true">
                <list-param-item code="HMC_MOUNT_TYPE_01" name="By gluing (conductive glue)" value="1"/>
                <list-param-item code="HMC_MOUNT_TYPE_02" name="By soldering (solder)" value="2"/>
            </family-param>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="ec_cc" name="Ceramic capacitors">
            <family-param code="ec_cc_type" name="Type" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="EC_CC_TYPE_01"
                                 name="Ceramic capacitor with defined temperature coefficient (Type I)" value="1"/>
                <list-param-item code="EC_CC_TYPE_02"
                                 name="Ceramic capacitor with non-defined temperature coefficient (Type II X5R)"
                                 value="2"/>
                <list-param-item code="EC_CC_TYPE_03"
                                 name="Ceramic capacitor with non-defined temperature coefficient (Type II X7R)"
                                 value="3"/>
                <list-param-item code="EC_CC_TYPE_04"
                                 name="Ceramic capacitor with polymer terminations and a non-defined temperature coefficient (Type II X5R)"
                                 value="4"/>
                <list-param-item code="EC_CC_TYPE_05"
                                 name="Ceramic capacitor with polymer terminations and a non-defined temperature coefficient (Type II X7R)"
                                 value="5"/>
            </family-param>
            <family-param code="ec_top_end" name="Top end" value-type="BOOL" optional="false" in-hmc="false"/>
            <family-param code="ec_c_rated" name="C" value-type="NUMERIC" unit="F" optional="false" in-hmc="false"/>
            <family-param code="ec_v_rated" name="V_rated" value-type="NUMERIC" unit="V" optional="false"
                          in-hmc="false"/>
            <app-stress code="ec_v_appl" name="V_applied" value-type="NUMERIC" unit="V" optional="false"
                        in-hmc="false"/>
            <family-param code="hmc_mount_type" name="Mount type (H&amp;M)" value-type="LIST" optional="false"
                          in-hmc="true">
                <list-param-item code="HMC_MOUNT_TYPE_01" name="By gluing (conductive glue)" value="1"/>
                <list-param-item code="HMC_MOUNT_TYPE_02" name="By soldering (solder)" value="2"/>
            </family-param>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="ec_ac" name="Aluminium capacitors">
            <family-param code="ec_ac_type" name="Type" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="EC_AC_TYPE_01" name="Wet aluminium electrolytic capacitor" value="1"/>
                <list-param-item code="EC_AC_TYPE_02" name="Solid aluminium electrolytic capacitor" value="2"/>
            </family-param>
            <family-param code="ec_v_rated" name="V_rated" value-type="NUMERIC" unit="V" optional="false"
                          in-hmc="false"/>
            <app-stress code="ec_v_appl" name="V_applied" value-type="NUMERIC" unit="V" optional="false"
                        in-hmc="false"/>
            <family-param code="hmc_mount_type" name="Mount type (H&amp;M)" value-type="LIST" optional="false"
                          in-hmc="true">
                <list-param-item code="HMC_MOUNT_TYPE_01" name="By gluing (conductive glue)" value="1"/>
                <list-param-item code="HMC_MOUNT_TYPE_02" name="By soldering (solder)" value="2"/>
            </family-param>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="ec_tc" name="Tantalum capacitors">
            <family-param code="ec_tc_tech" name="Technology" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="EC_TC_TECH_01" name="Wet tantalum capacitor, silver case, elastomer-sealed"
                                 value="1"/>
                <list-param-item code="EC_TC_TECH_02" name="Wet tantalum capacitor, silver case, glass-sealed"
                                 value="2"/>
                <list-param-item code="EC_TC_TECH_03" name="Wet tantalum capacitor, tantalum case, glass-sealed"
                                 value="3"/>
                <list-param-item code="EC_TC_TECH_04" name="Solid tantalum capacitor, bead packaging" value="4"/>
                <list-param-item code="EC_TC_TECH_05" name="Solid tantalum capacitor, SMD packaging" value="5"/>
                <list-param-item code="EC_TC_TECH_06" name="Solid tantalum capacitor, axial metal packaging" value="6"/>
            </family-param>
            <family-param code="ec_v_rated" name="V_rated" value-type="NUMERIC" unit="V" optional="false"
                          in-hmc="false"/>
            <app-stress code="ec_v_appl" name="V_applied" value-type="NUMERIC" unit="V" optional="false"
                        in-hmc="false"/>
            <family-param code="hmc_mount_type" name="Mount type (H&amp;M)" value-type="LIST" optional="false"
                          in-hmc="true">
                <list-param-item code="HMC_MOUNT_TYPE_01" name="By gluing (conductive glue)" value="1"/>
                <list-param-item code="HMC_MOUNT_TYPE_02" name="By soldering (solder)" value="2"/>
            </family-param>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="ec_pfc" name="Plastic film capacitors">
            <family-param code="ec_pfc_type" name="Type" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="EC_PFC_TYPE_01" name="Polypropylene (PP) film capacitor" value="1"/>
                <list-param-item code="EC_PFC_TYPE_02" name="Polyethylene terephtalate (PET) film capacitor" value="2"/>
                <list-param-item code="EC_PFC_TYPE_03" name="Polyethylene naphtalate (PEN) film capacitor" value="3"/>
                <list-param-item code="EC_PFC_TYPE_04" name="Polyphenylene sulfide (PPS) film capacitor" value="4"/>
                <list-param-item code="EC_PFC_TYPE_05" name="Teflon (PTFE) film capacitor" value="5"/>
            </family-param>
            <family-param code="ec_v_rated" name="V_rated" value-type="NUMERIC" unit="V" optional="false"
                          in-hmc="false"/>
            <app-stress code="ec_v_appl" name="V_applied" value-type="NUMERIC" unit="V" optional="false"
                        in-hmc="false"/>
            <family-param code="hmc_mount_type" name="Mount type (H&amp;M)" value-type="LIST" optional="false"
                          in-hmc="true">
                <list-param-item code="HMC_MOUNT_TYPE_01" name="By gluing (conductive glue)" value="1"/>
                <list-param-item code="HMC_MOUNT_TYPE_02" name="By soldering (solder)" value="2"/>
            </family-param>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="ec_mc" name="Magnetic components">
            <family-param code="ec_mc_type" name="Type" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="EC_MC_TYPE_01" name="Low-current (or low-level) wirewound inductor" value="1"/>
                <list-param-item code="EC_MC_TYPE_02" name="High-current (or power) wirewound inductor" value="2"/>
                <list-param-item code="EC_MC_TYPE_03" name="Multilayer inductor" value="3"/>
                <list-param-item code="EC_MC_TYPE_04" name="Low-power (or low-level) transformer" value="4"/>
                <list-param-item code="EC_MC_TYPE_05" name="High-power transformer" value="5"/>
            </family-param>
            <app-stress code="ec_delta_t" name="ΔT" value-type="NUMERIC" unit="°C" optional="false" in-hmc="false"/>
            <family-param code="hmc_mount_type" name="Mount type (H&amp;M)" value-type="LIST" optional="false"
                          in-hmc="true">
                <list-param-item code="HMC_MOUNT_TYPE_01" name="By gluing (conductive glue)" value="1"/>
                <list-param-item code="HMC_MOUNT_TYPE_02" name="By soldering (solder)" value="2"/>
            </family-param>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="ec_pec" name="Piezoelectric components">
            <family-param code="ec_pec_type" name="Type" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="EC_PEC_TYPE_01" name="Quartz crystal resonator (HCxx package, through-hole)"
                                 value="1"/>
                <list-param-item code="EC_PEC_TYPE_02" name="Quartz crystal resonator (surface-mounted)" value="2"/>
                <list-param-item code="EC_PEC_TYPE_03" name="Quartz crystal oscillator (XO package through-hole)"
                                 value="3"/>
                <list-param-item code="EC_PEC_TYPE_04"
                                 name="Quartz crystal oscillator (XO, MCSO package, surface-mounted)" value="4"/>
            </family-param>
            <family-param code="ec_i_out_max" name="I_output_max" value-type="NUMERIC" unit="A" optional="false"
                          in-hmc="false"/>
            <app-stress code="ec_i_out" name="I_output" value-type="NUMERIC" unit="A" optional="false" in-hmc="false"/>
            <family-param code="ec_t_max_manuf" name="T_max_manufacturer" value-type="NUMERIC" unit="°C"
                          optional="false" in-hmc="false"/>
            <family-param code="hmc_mount_type" name="Mount type (H&amp;M)" value-type="LIST" optional="false"
                          in-hmc="true">
                <list-param-item code="HMC_MOUNT_TYPE_01" name="By gluing (conductive glue)" value="1"/>
                <list-param-item code="HMC_MOUNT_TYPE_02" name="By soldering (solder)" value="2"/>
            </family-param>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="ec_memr" name="Monostable electromechanical relays">
            <family-param code="ec_n_dt" name="N_DT" value-type="NUMERIC" optional="false" in-hmc="false"/>
            <family-param code="ec_n_st" name="N_ST" value-type="NUMERIC" optional="false" in-hmc="false"/>
            <family-param code="ec_contact_type" name="Contact type" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="EC_CONTACT_01" name="Gold-plated" value="1"/>
                <list-param-item code="EC_CONTACT_02" name="Silver" value="2"/>
            </family-param>
            <family-param code="ec_break_cpty" name="Breaking capacity" value-type="NUMERIC" unit="A" optional="false"
                          in-hmc="false"/>
            <family-param code="ec_herme_type" name="Hermeticity type" value-type="LIST" optional="false"
                          in-hmc="false">
                <list-param-item code="EC_HERMETICITY_01" name="Hermetic" value="1"/>
                <list-param-item code="EC_HERMETICITY_02" name="Sealed" value="2"/>
                <list-param-item code="EC_HERMETICITY_03" name="Not sealed" value="3"/>
            </family-param>
            <family-param code="ec_v_rated" name="V_rated" value-type="NUMERIC" unit="V" optional="false"
                          in-hmc="false"/>
            <family-param code="ec_i_rated" name="I_rated" value-type="NUMERIC" unit="A" optional="false"
                          in-hmc="false"/>
            <family-param code="ec_u_appl" name="U_applied" value-type="NUMERIC" unit="V" optional="false"
                          in-hmc="false"/>
            <app-stress code="ec_op_nb" name="Nb op/h" value-type="NUMERIC" unit="Op/H" optional="false"
                        in-hmc="false"/>
            <app-stress code="ec_load_type" name="Load type" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="EC_LOAD_01" name="Resistive" value="1"/>
                <list-param-item code="EC_LOAD_02" name="Inductive" value="2"/>
                <list-param-item code="EC_LOAD_03" name="Incandescent lamp" value="3"/>
                <list-param-item code="EC_LOAD_04" name="Capacitive" value="4"/>
            </app-stress>
            <app-stress code="ec_v_contact" name="V_contact" value-type="NUMERIC" unit="V" optional="false"
                        in-hmc="false"/>
            <app-stress code="ec_i_contact" name="I_contact" value-type="NUMERIC" unit="A" optional="false"
                        in-hmc="false"/>
            <app-stress code="ec_u_coil" name="U_coil" value-type="NUMERIC" unit="V" optional="false" in-hmc="false"/>
            <app-stress code="ec_delta_t" name="ΔT" value-type="NUMERIC" unit="°C" optional="false" in-hmc="false"/>
            <family-param code="hmc_mount_type" name="Mount type (H&amp;M)" value-type="LIST" optional="false"
                          in-hmc="true">
                <list-param-item code="HMC_MOUNT_TYPE_01" name="By gluing (conductive glue)" value="1"/>
                <list-param-item code="HMC_MOUNT_TYPE_02" name="By soldering (solder)" value="2"/>
            </family-param>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="ec_sw" name="Switches">
            <family-param code="ec_sw_type" name="Type" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="EC_SW_TYPE_01" name="Limit switch, microcontacts" value="1"/>
                <list-param-item code="EC_SW_TYPE_02" name="Toggle" value="2"/>
                <list-param-item code="EC_SW_TYPE_03" name="Slide" value="3"/>
                <list-param-item code="EC_SW_TYPE_04" name="Lever" value="4"/>
                <list-param-item code="EC_SW_TYPE_05" name="DIP" value="5"/>
                <list-param-item code="EC_SW_TYPE_06" name="Rotary" value="6"/>
                <list-param-item code="EC_SW_TYPE_07" name="Encoder" value="7"/>
                <list-param-item code="EC_SW_TYPE_08" name="Momentary push button (monostable)" value="8"/>
                <list-param-item code="EC_SW_TYPE_09" name="Permanent push button (bistable)" value="9"/>
            </family-param>
            <family-param code="ec_contact_type" name="Contact type" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="EC_CONTACT_01" name="Gold-plated" value="1"/>
                <list-param-item code="EC_CONTACT_02" name="Silver" value="2"/>
            </family-param>
            <family-param code="ec_break_cpty" name="Breaking capacity" value-type="NUMERIC" unit="A" optional="false"
                          in-hmc="false"/>
            <family-param code="ec_herme_type" name="Hermeticity type" value-type="LIST" optional="false"
                          in-hmc="false">
                <list-param-item code="EC_HERMETICITY_01" name="Hermetic" value="1"/>
                <list-param-item code="EC_HERMETICITY_02" name="Sealed" value="2"/>
                <list-param-item code="EC_HERMETICITY_03" name="Not sealed" value="3"/>
            </family-param>
            <family-param code="ec_n_dt" name="N_DT" value-type="NUMERIC" optional="false" in-hmc="false"/>
            <family-param code="ec_n_st" name="N_ST" value-type="NUMERIC" optional="false" in-hmc="false"/>
            <family-param code="ec_v_rated" name="V_rated" value-type="NUMERIC" unit="V" optional="false"
                          in-hmc="false"/>
            <family-param code="ec_i_rated" name="I_rated" value-type="NUMERIC" unit="A" optional="false"
                          in-hmc="false"/>
            <app-stress code="ec_op_nb" name="Nb op/h" value-type="NUMERIC" unit="Op/H" optional="false"
                        in-hmc="false"/>
            <app-stress code="ec_load_type" name="Load type" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="EC_LOAD_01" name="Resistive" value="1"/>
                <list-param-item code="EC_LOAD_02" name="Inductive" value="2"/>
                <list-param-item code="EC_LOAD_03" name="Incandescent lamp" value="3"/>
                <list-param-item code="EC_LOAD_04" name="Capacitive" value="4"/>
            </app-stress>
            <app-stress code="ec_v_contact" name="V_contact" value-type="NUMERIC" unit="V" optional="false"
                        in-hmc="false"/>
            <app-stress code="ec_i_contact" name="I_contact" value-type="NUMERIC" unit="A" optional="false"
                        in-hmc="false"/>
            <family-param code="hmc_mount_type" name="Mount type (H&amp;M)" value-type="LIST" optional="false"
                          in-hmc="true">
                <list-param-item code="HMC_MOUNT_TYPE_01" name="By gluing (conductive glue)" value="1"/>
                <list-param-item code="HMC_MOUNT_TYPE_02" name="By soldering (solder)" value="2"/>
            </family-param>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="ec_pcb" name="Printed circuit boards">
            <family-param code="ec_pcb_class" name="Class" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="EC_PCB_CLASS_01" name="800 / 800" value="1"/>
                <list-param-item code="EC_PCB_CLASS_02" name="500 / 500" value="2"/>
                <list-param-item code="EC_PCB_CLASS_03" name="310 / 310" value="3"/>
                <list-param-item code="EC_PCB_CLASS_04" name="210 / 210" value="4"/>
                <list-param-item code="EC_PCB_CLASS_05" name="150 / 150" value="5"/>
                <list-param-item code="EC_PCB_CLASS_06" name="125 / 125" value="6"/>
                <list-param-item code="EC_PCB_CLASS_07" name="100 / 100" value="7"/>
            </family-param>
            <family-param code="ec_pcb_tech" name="Technology" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="EC_PCB_TECH_01" name="Through-holes" value="1"/>
                <list-param-item code="EC_PCB_TECH_02" name="Blind holes" value="2"/>
                <list-param-item code="EC_PCB_TECH_03" name="Micro-via technology" value="3"/>
                <list-param-item code="EC_PCB_TECH_04" name="Pad on via technology" value="4"/>
            </family-param>
            <family-param code="ec_n_layer" name="N_layers" value-type="NUMERIC" optional="false" in-hmc="false"/>
            <family-param code="ec_n_mount" name="N_mount" value-type="NUMERIC" optional="false" in-hmc="false"/>
            <family-param code="hmc_mount_type" name="Mount type (H&amp;M)" value-type="LIST" optional="false"
                          in-hmc="true">
                <list-param-item code="HMC_MOUNT_TYPE_01" name="By gluing (conductive glue)" value="1"/>
                <list-param-item code="HMC_MOUNT_TYPE_02" name="By soldering (solder)" value="2"/>
            </family-param>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="ec_co" name="Connectors">
            <family-param code="ec_co_type" name="Type" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="EC_CO_TYPE_01" name="Round and rectangular connectors" value="1"/>
                <list-param-item code="EC_CO_TYPE_02" name="Coaxial connectors" value="2"/>
                <list-param-item code="EC_CO_TYPE_03" name="Connectors for printed (and assimilated) circuits"
                                 value="3"/>
                <list-param-item code="EC_CO_TYPE_04" name="Component supports" value="4"/>
            </family-param>
            <family-param code="ec_mount_type" name="Mount Type" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="EC_CO_MOUNT_01" name="Insertion (press fit)" value="1"/>
                <list-param-item code="EC_CO_MOUNT_02" name="Soldered (through-hole)" value="2"/>
                <list-param-item code="EC_CO_MOUNT_03" name="Soldered (SMD)" value="3"/>
                <list-param-item code="EC_CO_MOUNT_04" name="Wrapping (braid)" value="4"/>
                <list-param-item code="EC_CO_MOUNT_05" name="Wrapping (wire)" value="5"/>
            </family-param>
            <family-param code="ec_n_contact" name="Contact Number" value-type="NUMERIC" optional="false"
                          in-hmc="false"/>
            <family-param code="ec_co_n_cycle" name="Nb mated/unmated Cycles" value-type="NUMERIC" optional="false"
                          in-hmc="false"/>
            <app-stress code="ec_delta_t" name="ΔT" value-type="NUMERIC" unit="°C" optional="false" in-hmc="false"/>
            <family-param code="hmc_mount_type" name="Mount type (H&amp;M)" value-type="LIST" optional="false"
                          in-hmc="true">
                <list-param-item code="HMC_MOUNT_TYPE_01" name="By gluing (conductive glue)" value="1"/>
                <list-param-item code="HMC_MOUNT_TYPE_02" name="By soldering (solder)" value="2"/>
            </family-param>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
    </macro-family>
    <macro-family code="hmc">
        <family code="hmc_hmc" name="Hybrid and multi-chip module">
            <family-param code="hmc_csens_cs" name="Case &amp; substrate C_sensitivity" value-type="LIST"
                          optional="false" in-hmc="false">
                <list-param-item code="HMC_CSENS_CS_01" name="Metal case, ceramic case, ceramic substrate" value="1"/>
                <list-param-item code="HMC_CSENS_CS_02" name="Glass/epoxy substrate with moulding" value="2"/>
                <list-param-item code="HMC_CSENS_CS_03" name="Glass/epoxy substrate without moulding" value="3"/>
            </family-param>
            <family-param code="hmc_mounting_type" name="Mounting type" value-type="LIST" optional="false"
                          in-hmc="false">
                <list-param-item code="HMC_MOUNTING_TYPE_01"
                                 name="Soldered surface-mount component with flat pins - With copper or copper alloy pins"
                                 value="1"/>
                <list-param-item code="HMC_MOUNTING_TYPE_02"
                                 name="Soldered surface-mount component with flat pins - With iron-nickel alloy pins (alloy 42, Kovar, etc.)"
                                 value="2"/>
                <list-param-item code="HMC_MOUNTING_TYPE_03"
                                 name="Soldered through-hole component with pins - With copper or copper alloy pins"
                                 value="3"/>
                <list-param-item code="HMC_MOUNTING_TYPE_04"
                                 name="Soldered through-hole component with pins - With iron-nickel alloy pins (alloy 42, Kovar, etc.)"
                                 value="4"/>
                <list-param-item code="HMC_MOUNTING_TYPE_05" name="Surface-mount soldered component without pins"
                                 value="5"/>
                <list-param-item code="HMC_MOUNTING_TYPE_06" name="Component without pins, assembled by contact"
                                 value="6"/>
            </family-param>
            <family-param code="hmc_attach_mode" name="Attachment mode" value-type="LIST" optional="false"
                          in-hmc="false">
                <list-param-item code="HMC_ATTACH_MODE_01"
                                 name="None (Allows for a degree of movement between the component and the printed circuit)"
                                 value="1"/>
                <list-param-item code="HMC_ATTACH_MODE_02"
                                 name="Flexible (Allows for limited movement of the component on its support)"
                                 value="2"/>
                <list-param-item code="HMC_ATTACH_MODE_03"
                                 name="Rigid (Allows for little or no movement between the component and the printed circuit)"
                                 value="3"/>
            </family-param>
            <family-param code="hmc_np" name="N_pin" value-type="NUMERIC" optional="false" in-hmc="false"/>
            <family-param code="hmc_l_pin" name="L_pin" value-type="NUMERIC" unit="mm" optional="false" in-hmc="false"/>
            <family-param code="hmc_s_pin" name="S_pin" value-type="NUMERIC" unit="mm2" optional="false"
                          in-hmc="false"/>
            <family-param code="hmc_d" name="D" value-type="NUMERIC" unit="mm" optional="false" in-hmc="false"/>
            <family-param code="hmc_m" name="M" value-type="NUMERIC" unit="g" optional="false" in-hmc="false"/>
            <family-param code="hmc_delta_cte" name="ΔCTE" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="HMC_DELTA_CTE_01" name="Metal (Kovar) without Cu/In/Cu" value="1"/>
                <list-param-item code="HMC_DELTA_CTE_02" name="Metal (Kovar) with Cu/In/Cu" value="2"/>
                <list-param-item code="HMC_DELTA_CTE_03" name="Ceramic (alumina or cofired) without Cu/In/Cu"
                                 value="3"/>
                <list-param-item code="HMC_DELTA_CTE_04" name="Ceramic (alumina or cofired) with Cu/In/Cu" value="4"/>
                <list-param-item code="HMC_DELTA_CTE_05" name="Moulded (organic substrate or ceramic) without Cu/In/Cu"
                                 value="5"/>
                <list-param-item code="HMC_DELTA_CTE_06" name="Moulded (organic substrate or ceramic) with Cu/In/Cu"
                                 value="6"/>
            </family-param>
            <app-stress code="hmc_delta_thm" name="ΔT_H&amp;M" value-type="NUMERIC" unit="°C" optional="false"
                        in-hmc="false"/>
        </family>
        <family code="hmc_ca" name="Cavity">
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
            <family-param code="hmc_c_herme" name="C_hermeticity" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="HMC_C_HERMETICITY_01" name="Hermetic circuit (with or without internal coating)"
                                 value="1"/>
                <list-param-item code="HMC_C_HERMETICITY_02" name="Sealed cavity circuit (non-hermetic)" value="2"/>
                <list-param-item code="HMC_C_HERMETICITY_03" name="Moulded circuit" value="3"/>
            </family-param>
            <family-param code="hmc_c_particle" name="C_particle" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="HMC_C_PARTICLE_01"
                                 name="Moulded circuit or chip interconnection by flip-chip, with underfill" value="1"/>
                <list-param-item code="HMC_C_PARTICLE_02"
                                 name="Non-moulded hermetic circuit with particle trap and gold wire*" value="2"/>
                <list-param-item code="HMC_C_PARTICLE_03"
                                 name="Non-moulded hermetic circuit with particle trap and aluminium wire* or chip interconnection by flip-chip without underfill"
                                 value="3"/>
                <list-param-item code="HMC_C_PARTICLE_04"
                                 name="Non-moulded hermetic circuit without particle trap and gold wire*" value="4"/>
                <list-param-item code="HMC_C_PARTICLE_05"
                                 name="Non-moulded hermetic circuit without particle trap and aluminium wire*"
                                 value="5"/>
            </family-param>
            <family-param code="hmc_nb_wire" name="N_wires" value-type="NUMERIC" optional="false" in-hmc="false"/>
            <family-param code="hmc_n_track" name="N_tracks" value-type="NUMERIC" optional="false" in-hmc="false"/>
            <family-param code="hmc_n_layer" name="N_layers" value-type="NUMERIC" optional="false" in-hmc="false"/>
            <family-param code="hmc_pi_class" name="&amp;Pi;_Class" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="HMC_PI_CLASS_01" name="800 / 800" value="1"/>
                <list-param-item code="HMC_PI_CLASS_02" name="500 / 500" value="2"/>
                <list-param-item code="HMC_PI_CLASS_03" name="310 / 310" value="3"/>
                <list-param-item code="HMC_PI_CLASS_04" name="210 / 210" value="4"/>
                <list-param-item code="HMC_PI_CLASS_05" name="150 / 150" value="5"/>
                <list-param-item code="HMC_PI_CLASS_06" name="125 / 125" value="6"/>
                <list-param-item code="HMC_PI_CLASS_07" name="100 / 100" value="7"/>
            </family-param>
            <family-param code="hmc_cs_tech" name="Case &amp; substrate technology" value-type="LIST" optional="false"
                          in-hmc="false">
                <list-param-item code="HMC_CS_TECH_01" name="Hermetic ceramic case (cofired MCM package, etc.)"
                                 value="1"/>
                <list-param-item code="HMC_CS_TECH_02" name="Alumina substrate with hermetic metal case" value="2"/>
                <list-param-item code="HMC_CS_TECH_03" name="Alumina substrate with moulding" value="3"/>
                <list-param-item code="HMC_CS_TECH_04" name="Alumina substrate without case or moulding" value="4"/>
                <list-param-item code="HMC_CS_TECH_05" name="Organic substrate (glass/epoxy) with hermetic metal case"
                                 value="5"/>
                <list-param-item code="HMC_CS_TECH_06" name="Organic substrate (glass/epoxy) with moulding" value="6"/>
                <list-param-item code="HMC_CS_TECH_07" name="Glass/epoxy substrate without case or moulding" value="7"/>
            </family-param>
            <family-param code="hmc_cs_type" name="Substrate type" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="HMC_CS_TYPE_01" name="Ceramic" value="1"/>
                <list-param-item code="HMC_CS_TYPE_02" name="Glass/epoxy - Through-holes" value="2"/>
                <list-param-item code="HMC_CS_TYPE_03" name="Glass/epoxy - Blind holes" value="3"/>
                <list-param-item code="HMC_CS_TYPE_04" name="Glass/epoxy - Micro-via technology" value="4"/>
                <list-param-item code="HMC_CS_TYPE_05" name="Glass/epoxy - Pad on via technology" value="5"/>
            </family-param>
            <family-param code="hmc_w_type" name="Wiring type" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="HMC_WIRING_TYPE_01" name="Wires and strips (aluminium and gold)" value="1"/>
                <list-param-item code="HMC_WIRING_TYPE_02" name="Bumps" value="2"/>
            </family-param>
        </family>
        <family code="hmc_bc_ic" name="Micro-components - Bare chips (Integrated circuit)">
            <family-param code="hmc_icds_chip" name="Chip" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="HMC_ICDS_CHIP_01" name="FPGA, CPLD, FPGA Antifuse, PAL" value="1"/>
                <list-param-item code="HMC_ICDS_CHIP_02" name="Analog and mixed circuit (MOS, Bipolar, BiCMOS)"
                                 value="2"/>
                <list-param-item code="HMC_ICDS_CHIP_03" name="Microprocessor, Microcontroller, DSP" value="3"/>
                <list-param-item code="HMC_ICDS_CHIP_04" name="Flash, EEPROM, EPROM" value="4"/>
                <list-param-item code="HMC_ICDS_CHIP_05" name="SRAM" value="5"/>
                <list-param-item code="HMC_ICDS_CHIP_06" name="DRAM" value="6"/>
                <list-param-item code="HMC_ICDS_CHIP_07" name="Digital circuit (MOS, Bipolar, BiCMOS)" value="7"/>
                <list-param-item code="HMC_ICDS_CHIP_08" name="Silicon MOS - Digital ASIC, simple function" value="8"/>
                <list-param-item code="HMC_ICDS_CHIP_09"
                                 name="Silicon MOS - Digital ASIC, complex function (with IP and/or ?P core, memory blocks)"
                                 value="9"/>
                <list-param-item code="HMC_ICDS_CHIP_10" name="Silicon MOS - Analog, mixed ASIC" value="10"/>
                <list-param-item code="HMC_ICDS_CHIP_11" name="Silicon bipolar, BICMOS - Digital ASIC" value="11"/>
                <list-param-item code="HMC_ICDS_CHIP_12" name="Silicon bipolar, BICMOS - Mixed, analog ASIC"
                                 value="12"/>
                <list-param-item code="HMC_ICDS_CHIP_13"
                                 name="Low-power diodes - Signal diodes up to 1A (PIN, Schottky, signal, varactor)"
                                 value="13"/>
                <list-param-item code="HMC_ICDS_CHIP_14" name="Low-power diodes - Rectifier diodes 1A to 3A"
                                 value="14"/>
                <list-param-item code="HMC_ICDS_CHIP_15" name="Low-power diodes - Zener regulation diodes up to 1.5W"
                                 value="15"/>
                <list-param-item code="HMC_ICDS_CHIP_16"
                                 name="Low-power diodes - Protection diodes up to 3kW (peak 10ms / 100ms) (TVS)"
                                 value="16"/>
                <list-param-item code="HMC_ICDS_CHIP_17" name="Power diodes - Thyristors, triacs over 3A" value="17"/>
                <list-param-item code="HMC_ICDS_CHIP_18" name="Power diodes - Rectifier diodes &gt; 3A" value="18"/>
                <list-param-item code="HMC_ICDS_CHIP_19" name="Power diodes - Zener regulation diodes over 1.5W"
                                 value="19"/>
                <list-param-item code="HMC_ICDS_CHIP_20"
                                 name="Power diodes - Protection diodes over 3kW (peak 10ms / 100ms) (TVS)" value="20"/>
                <list-param-item code="HMC_ICDS_CHIP_21" name="Low-power transistors - Silicon, bipolar &lt; 5W"
                                 value="21"/>
                <list-param-item code="HMC_ICDS_CHIP_22" name="Low-power transistors - Silicon, MOS &lt; 5W"
                                 value="22"/>
                <list-param-item code="HMC_ICDS_CHIP_23" name="Low-power transistors - Silicon, JFET &lt; 5W"
                                 value="23"/>
                <list-param-item code="HMC_ICDS_CHIP_24" name="Power transistors - Silicon, bipolar &gt; 5W"
                                 value="24"/>
                <list-param-item code="HMC_ICDS_CHIP_25" name="Power transistors - Silicon, MOS &gt; 5W" value="25"/>
                <list-param-item code="HMC_ICDS_CHIP_26" name="Power transistors - IGBT" value="26"/>
            </family-param>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
            <family-param code="hmc_bc_s" name="S" value-type="NUMERIC" unit="mm2" optional="false" in-hmc="false"/>
            <family-param code="hmc_bc_d" name="d" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="HMC_BC_D_01" name="Silicon digital integrated circuits (MOS, Bipolar and BiCMOS)"
                                 value="1"/>
                <list-param-item code="HMC_BC_D_02" name="Silicon analog integrated circuits (MOS, Bipolar and BiCMOS)"
                                 value="2"/>
                <list-param-item code="HMC_BC_D_03" name="Discrete circuits" value="3"/>
            </family-param>
            <family-param code="hmc_v_rated" name="V_rated" value-type="NUMERIC" optional="false" in-hmc="false"/>
            <app-stress code="hmc_v_appl" name="V_applied" value-type="NUMERIC" optional="false" in-hmc="false"/>
            <app-stress code="hmc_delta_t" name="ΔT" value-type="NUMERIC" unit="°C" optional="false" in-hmc="false"/>
        </family>
        <family code="hmc_bc_ds" name="Micro-components - Bare chips (Discrete semiconductor)">
            <family-param code="hmc_icds_chip" name="Chip" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="HMC_ICDS_CHIP_01" name="FPGA, CPLD, FPGA Antifuse, PAL" value="1"/>
                <list-param-item code="HMC_ICDS_CHIP_02" name="Analog and mixed circuit (MOS, Bipolar, BiCMOS)"
                                 value="2"/>
                <list-param-item code="HMC_ICDS_CHIP_03" name="Microprocessor, Microcontroller, DSP" value="3"/>
                <list-param-item code="HMC_ICDS_CHIP_04" name="Flash, EEPROM, EPROM" value="4"/>
                <list-param-item code="HMC_ICDS_CHIP_05" name="SRAM" value="5"/>
                <list-param-item code="HMC_ICDS_CHIP_06" name="DRAM" value="6"/>
                <list-param-item code="HMC_ICDS_CHIP_07" name="Digital circuit (MOS, Bipolar, BiCMOS)" value="7"/>
                <list-param-item code="HMC_ICDS_CHIP_08" name="Silicon MOS - Digital ASIC, simple function" value="8"/>
                <list-param-item code="HMC_ICDS_CHIP_09"
                                 name="Silicon MOS - Digital ASIC, complex function (with IP and/or ?P core, memory blocks)"
                                 value="9"/>
                <list-param-item code="HMC_ICDS_CHIP_10" name="Silicon MOS - Analog, mixed ASIC" value="10"/>
                <list-param-item code="HMC_ICDS_CHIP_11" name="Silicon bipolar, BICMOS - Digital ASIC" value="11"/>
                <list-param-item code="HMC_ICDS_CHIP_12" name="Silicon bipolar, BICMOS - Mixed, analog ASIC"
                                 value="12"/>
                <list-param-item code="HMC_ICDS_CHIP_13"
                                 name="Low-power diodes - Signal diodes up to 1A (PIN, Schottky, signal, varactor)"
                                 value="13"/>
                <list-param-item code="HMC_ICDS_CHIP_14" name="Low-power diodes - Rectifier diodes 1A to 3A"
                                 value="14"/>
                <list-param-item code="HMC_ICDS_CHIP_15" name="Low-power diodes - Zener regulation diodes up to 1.5W"
                                 value="15"/>
                <list-param-item code="HMC_ICDS_CHIP_16"
                                 name="Low-power diodes - Protection diodes up to 3kW (peak 10ms / 100ms) (TVS)"
                                 value="16"/>
                <list-param-item code="HMC_ICDS_CHIP_17" name="Power diodes - Thyristors, triacs over 3A" value="17"/>
                <list-param-item code="HMC_ICDS_CHIP_18" name="Power diodes - Rectifier diodes &gt; 3A" value="18"/>
                <list-param-item code="HMC_ICDS_CHIP_19" name="Power diodes - Zener regulation diodes over 1.5W"
                                 value="19"/>
                <list-param-item code="HMC_ICDS_CHIP_20"
                                 name="Power diodes - Protection diodes over 3kW (peak 10ms / 100ms) (TVS)" value="20"/>
                <list-param-item code="HMC_ICDS_CHIP_21" name="Low-power transistors - Silicon, bipolar &lt; 5W"
                                 value="21"/>
                <list-param-item code="HMC_ICDS_CHIP_22" name="Low-power transistors - Silicon, MOS &lt; 5W"
                                 value="22"/>
                <list-param-item code="HMC_ICDS_CHIP_23" name="Low-power transistors - Silicon, JFET &lt; 5W"
                                 value="23"/>
                <list-param-item code="HMC_ICDS_CHIP_24" name="Power transistors - Silicon, bipolar &gt; 5W"
                                 value="24"/>
                <list-param-item code="HMC_ICDS_CHIP_25" name="Power transistors - Silicon, MOS &gt; 5W" value="25"/>
                <list-param-item code="HMC_ICDS_CHIP_26" name="Power transistors - IGBT" value="26"/>
            </family-param>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
            <family-param code="hmc_bc_s" name="S" value-type="NUMERIC" unit="mm2" optional="false" in-hmc="false"/>
            <family-param code="hmc_bc_d" name="d" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="HMC_BC_D_01" name="Silicon digital integrated circuits (MOS, Bipolar and BiCMOS)"
                                 value="1"/>
                <list-param-item code="HMC_BC_D_02" name="Silicon analog integrated circuits (MOS, Bipolar and BiCMOS)"
                                 value="2"/>
                <list-param-item code="HMC_BC_D_03" name="Discrete circuits" value="3"/>
            </family-param>
            <family-param code="hmc_v_rated" name="V_rated" value-type="NUMERIC" optional="false" in-hmc="false"/>
            <app-stress code="hmc_v_appl" name="V_applied" value-type="NUMERIC" optional="false" in-hmc="false"/>
            <app-stress code="hmc_delta_t" name="ΔT" value-type="NUMERIC" unit="°C" optional="false" in-hmc="false"/>
        </family>
        <family code="hmc_mpc_ic" name="Micro-components - Micro-packaged components (Integrated circuit)">
            <family-param code="hmc_icds_chip" name="Chip" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="HMC_ICDS_CHIP_01" name="FPGA, CPLD, FPGA Antifuse, PAL" value="1"/>
                <list-param-item code="HMC_ICDS_CHIP_02" name="Analog and mixed circuit (MOS, Bipolar, BiCMOS)"
                                 value="2"/>
                <list-param-item code="HMC_ICDS_CHIP_03" name="Microprocessor, Microcontroller, DSP" value="3"/>
                <list-param-item code="HMC_ICDS_CHIP_04" name="Flash, EEPROM, EPROM" value="4"/>
                <list-param-item code="HMC_ICDS_CHIP_05" name="SRAM" value="5"/>
                <list-param-item code="HMC_ICDS_CHIP_06" name="DRAM" value="6"/>
                <list-param-item code="HMC_ICDS_CHIP_07" name="Digital circuit (MOS, Bipolar, BiCMOS)" value="7"/>
                <list-param-item code="HMC_ICDS_CHIP_08" name="Silicon MOS - Digital ASIC, simple function" value="8"/>
                <list-param-item code="HMC_ICDS_CHIP_09"
                                 name="Silicon MOS - Digital ASIC, complex function (with IP and/or ?P core, memory blocks)"
                                 value="9"/>
                <list-param-item code="HMC_ICDS_CHIP_10" name="Silicon MOS - Analog, mixed ASIC" value="10"/>
                <list-param-item code="HMC_ICDS_CHIP_11" name="Silicon bipolar, BICMOS - Digital ASIC" value="11"/>
                <list-param-item code="HMC_ICDS_CHIP_12" name="Silicon bipolar, BICMOS - Mixed, analog ASIC"
                                 value="12"/>
                <list-param-item code="HMC_ICDS_CHIP_13"
                                 name="Low-power diodes - Signal diodes up to 1A (PIN, Schottky, signal, varactor)"
                                 value="13"/>
                <list-param-item code="HMC_ICDS_CHIP_14" name="Low-power diodes - Rectifier diodes 1A to 3A"
                                 value="14"/>
                <list-param-item code="HMC_ICDS_CHIP_15" name="Low-power diodes - Zener regulation diodes up to 1.5W"
                                 value="15"/>
                <list-param-item code="HMC_ICDS_CHIP_16"
                                 name="Low-power diodes - Protection diodes up to 3kW (peak 10ms / 100ms) (TVS)"
                                 value="16"/>
                <list-param-item code="HMC_ICDS_CHIP_17" name="Power diodes - Thyristors, triacs over 3A" value="17"/>
                <list-param-item code="HMC_ICDS_CHIP_18" name="Power diodes - Rectifier diodes &gt; 3A" value="18"/>
                <list-param-item code="HMC_ICDS_CHIP_19" name="Power diodes - Zener regulation diodes over 1.5W"
                                 value="19"/>
                <list-param-item code="HMC_ICDS_CHIP_20"
                                 name="Power diodes - Protection diodes over 3kW (peak 10ms / 100ms) (TVS)" value="20"/>
                <list-param-item code="HMC_ICDS_CHIP_21" name="Low-power transistors - Silicon, bipolar &lt; 5W"
                                 value="21"/>
                <list-param-item code="HMC_ICDS_CHIP_22" name="Low-power transistors - Silicon, MOS &lt; 5W"
                                 value="22"/>
                <list-param-item code="HMC_ICDS_CHIP_23" name="Low-power transistors - Silicon, JFET &lt; 5W"
                                 value="23"/>
                <list-param-item code="HMC_ICDS_CHIP_24" name="Power transistors - Silicon, bipolar &gt; 5W"
                                 value="24"/>
                <list-param-item code="HMC_ICDS_CHIP_25" name="Power transistors - Silicon, MOS &gt; 5W" value="25"/>
                <list-param-item code="HMC_ICDS_CHIP_26" name="Power transistors - IGBT" value="26"/>
            </family-param>
            <family-param code="hmc_icds_pkg" name="Package" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="HMC_ICDS_PACKAGE_01" name="PQFP [IC]" value="1"/>
                <list-param-item code="HMC_ICDS_PACKAGE_02" name="SQFP, TQFP, VQFP, LQFP [IC]" value="2"/>
                <list-param-item code="HMC_ICDS_PACKAGE_03" name="Power QFP (RQFP, HQFP, PowerQuad, EdQuad, etc.) [IC]"
                                 value="3"/>
                <list-param-item code="HMC_ICDS_PACKAGE_04" name="CERPACK [IC]" value="4"/>
                <list-param-item code="HMC_ICDS_PACKAGE_05" name="CQFP, Cerquad [IC]" value="5"/>
                <list-param-item code="HMC_ICDS_PACKAGE_06" name="PLCC [IC]" value="6"/>
                <list-param-item code="HMC_ICDS_PACKAGE_07" name="J-CLCC [IC]" value="7"/>
                <list-param-item code="HMC_ICDS_PACKAGE_08" name="CLCC [IC]" value="8"/>
                <list-param-item code="HMC_ICDS_PACKAGE_09" name="SOJ [IC]" value="9"/>
                <list-param-item code="HMC_ICDS_PACKAGE_10" name="SO, SOP, GROUND, SOIC, SOW [IC]" value="10"/>
                <list-param-item code="HMC_ICDS_PACKAGE_11" name="TSOP I, TSOP II [IC]" value="11"/>
                <list-param-item code="HMC_ICDS_PACKAGE_12" name="SSOP, VSOP, QSOP [IC]" value="12"/>
                <list-param-item code="HMC_ICDS_PACKAGE_13" name="TSSOP, MSOP, ?SO, ?MAX, TVSOP [IC]" value="13"/>
                <list-param-item code="HMC_ICDS_PACKAGE_14" name="PBGA CSP BT 0.8 and 0.75 mm [IC]" value="14"/>
                <list-param-item code="HMC_ICDS_PACKAGE_15" name="PBGA flex 0.8 mm [IC]" value="15"/>
                <list-param-item code="HMC_ICDS_PACKAGE_16" name="PBGA BT 1.00 mm [IC]" value="16"/>
                <list-param-item code="HMC_ICDS_PACKAGE_17" name="PBGA 1.27mm [IC]" value="17"/>
                <list-param-item code="HMC_ICDS_PACKAGE_18" name="Power BGA (TBGA, SBGA, etc.) [IC]" value="18"/>
                <list-param-item code="HMC_ICDS_PACKAGE_19" name="CBGA [IC]" value="19"/>
                <list-param-item code="HMC_ICDS_PACKAGE_20" name="DBGA [IC]" value="20"/>
                <list-param-item code="HMC_ICDS_PACKAGE_21" name="CGA IC [IC]" value="21"/>
                <list-param-item code="HMC_ICDS_PACKAGE_22" name="SOT23-3 [DS]" value="22"/>
                <list-param-item code="HMC_ICDS_PACKAGE_23" name="SOT23-5 [DS]" value="23"/>
                <list-param-item code="HMC_ICDS_PACKAGE_24" name="SOT23-6 [DS]" value="24"/>
                <list-param-item code="HMC_ICDS_PACKAGE_25" name="SOT143 [DS]" value="25"/>
                <list-param-item code="HMC_ICDS_PACKAGE_26" name="SOT323 [DS]" value="26"/>
                <list-param-item code="HMC_ICDS_PACKAGE_27" name="SOT346 [DS]" value="27"/>
                <list-param-item code="HMC_ICDS_PACKAGE_28" name="SOT353 [DS]" value="28"/>
                <list-param-item code="HMC_ICDS_PACKAGE_29" name="SOT363 [DS]" value="29"/>
                <list-param-item code="HMC_ICDS_PACKAGE_30" name="SOD123 [DS]" value="30"/>
                <list-param-item code="HMC_ICDS_PACKAGE_31" name="SOD323 [DS]" value="31"/>
                <list-param-item code="HMC_ICDS_PACKAGE_32" name="SOD523 [DS]" value="32"/>
                <list-param-item code="HMC_ICDS_PACKAGE_33" name="SOT223 [DS]" value="33"/>
                <list-param-item code="HMC_ICDS_PACKAGE_34" name="SOT243 [DS]" value="34"/>
                <list-param-item code="HMC_ICDS_PACKAGE_35" name="SOT343 [DS]" value="35"/>
                <list-param-item code="HMC_ICDS_PACKAGE_36" name="SOT89 [DS]" value="36"/>
                <list-param-item code="HMC_ICDS_PACKAGE_37" name="SOT194 [DS]" value="37"/>
                <list-param-item code="HMC_ICDS_PACKAGE_38" name="SOD6 [DS]" value="38"/>
                <list-param-item code="HMC_ICDS_PACKAGE_39" name="SOD15 [DS]" value="39"/>
                <list-param-item code="HMC_ICDS_PACKAGE_40" name="DPAK [DS]" value="40"/>
                <list-param-item code="HMC_ICDS_PACKAGE_41" name="D2PAK [DS]" value="41"/>
                <list-param-item code="HMC_ICDS_PACKAGE_42" name="D3PAK [DS]" value="42"/>
                <list-param-item code="HMC_ICDS_PACKAGE_43" name="ISOTOP [DS]" value="43"/>
                <list-param-item code="HMC_ICDS_PACKAGE_44" name="SOD80 [DS]" value="44"/>
                <list-param-item code="HMC_ICDS_PACKAGE_45" name="SOD87 [DS]" value="45"/>
            </family-param>
            <family-param code="hmc_np" name="N_pin" value-type="NUMERIC" optional="false" in-hmc="false"/>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
            <family-param code="hmc_v_rated" name="V_rated" value-type="NUMERIC" optional="false" in-hmc="false"/>
            <app-stress code="hmc_v_appl" name="V_applied" value-type="NUMERIC" optional="false" in-hmc="false"/>
            <app-stress code="hmc_delta_t" name="ΔT" value-type="NUMERIC" unit="°C" optional="false" in-hmc="false"/>
        </family>
        <family code="hmc_mpc_ds" name="Micro-components - Micro-packaged components (Discrete semicondutor)">
            <family-param code="hmc_icds_chip" name="Chip" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="HMC_ICDS_CHIP_01" name="FPGA, CPLD, FPGA Antifuse, PAL" value="1"/>
                <list-param-item code="HMC_ICDS_CHIP_02" name="Analog and mixed circuit (MOS, Bipolar, BiCMOS)"
                                 value="2"/>
                <list-param-item code="HMC_ICDS_CHIP_03" name="Microprocessor, Microcontroller, DSP" value="3"/>
                <list-param-item code="HMC_ICDS_CHIP_04" name="Flash, EEPROM, EPROM" value="4"/>
                <list-param-item code="HMC_ICDS_CHIP_05" name="SRAM" value="5"/>
                <list-param-item code="HMC_ICDS_CHIP_06" name="DRAM" value="6"/>
                <list-param-item code="HMC_ICDS_CHIP_07" name="Digital circuit (MOS, Bipolar, BiCMOS)" value="7"/>
                <list-param-item code="HMC_ICDS_CHIP_08" name="Silicon MOS - Digital ASIC, simple function" value="8"/>
                <list-param-item code="HMC_ICDS_CHIP_09"
                                 name="Silicon MOS - Digital ASIC, complex function (with IP and/or ?P core, memory blocks)"
                                 value="9"/>
                <list-param-item code="HMC_ICDS_CHIP_10" name="Silicon MOS - Analog, mixed ASIC" value="10"/>
                <list-param-item code="HMC_ICDS_CHIP_11" name="Silicon bipolar, BICMOS - Digital ASIC" value="11"/>
                <list-param-item code="HMC_ICDS_CHIP_12" name="Silicon bipolar, BICMOS - Mixed, analog ASIC"
                                 value="12"/>
                <list-param-item code="HMC_ICDS_CHIP_13"
                                 name="Low-power diodes - Signal diodes up to 1A (PIN, Schottky, signal, varactor)"
                                 value="13"/>
                <list-param-item code="HMC_ICDS_CHIP_14" name="Low-power diodes - Rectifier diodes 1A to 3A"
                                 value="14"/>
                <list-param-item code="HMC_ICDS_CHIP_15" name="Low-power diodes - Zener regulation diodes up to 1.5W"
                                 value="15"/>
                <list-param-item code="HMC_ICDS_CHIP_16"
                                 name="Low-power diodes - Protection diodes up to 3kW (peak 10ms / 100ms) (TVS)"
                                 value="16"/>
                <list-param-item code="HMC_ICDS_CHIP_17" name="Power diodes - Thyristors, triacs over 3A" value="17"/>
                <list-param-item code="HMC_ICDS_CHIP_18" name="Power diodes - Rectifier diodes &gt; 3A" value="18"/>
                <list-param-item code="HMC_ICDS_CHIP_19" name="Power diodes - Zener regulation diodes over 1.5W"
                                 value="19"/>
                <list-param-item code="HMC_ICDS_CHIP_20"
                                 name="Power diodes - Protection diodes over 3kW (peak 10ms / 100ms) (TVS)" value="20"/>
                <list-param-item code="HMC_ICDS_CHIP_21" name="Low-power transistors - Silicon, bipolar &lt; 5W"
                                 value="21"/>
                <list-param-item code="HMC_ICDS_CHIP_22" name="Low-power transistors - Silicon, MOS &lt; 5W"
                                 value="22"/>
                <list-param-item code="HMC_ICDS_CHIP_23" name="Low-power transistors - Silicon, JFET &lt; 5W"
                                 value="23"/>
                <list-param-item code="HMC_ICDS_CHIP_24" name="Power transistors - Silicon, bipolar &gt; 5W"
                                 value="24"/>
                <list-param-item code="HMC_ICDS_CHIP_25" name="Power transistors - Silicon, MOS &gt; 5W" value="25"/>
                <list-param-item code="HMC_ICDS_CHIP_26" name="Power transistors - IGBT" value="26"/>
            </family-param>
            <family-param code="hmc_icds_pkg" name="Package" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="HMC_ICDS_PACKAGE_01" name="PQFP [IC]" value="1"/>
                <list-param-item code="HMC_ICDS_PACKAGE_02" name="SQFP, TQFP, VQFP, LQFP [IC]" value="2"/>
                <list-param-item code="HMC_ICDS_PACKAGE_03" name="Power QFP (RQFP, HQFP, PowerQuad, EdQuad, etc.) [IC]"
                                 value="3"/>
                <list-param-item code="HMC_ICDS_PACKAGE_04" name="CERPACK [IC]" value="4"/>
                <list-param-item code="HMC_ICDS_PACKAGE_05" name="CQFP, Cerquad [IC]" value="5"/>
                <list-param-item code="HMC_ICDS_PACKAGE_06" name="PLCC [IC]" value="6"/>
                <list-param-item code="HMC_ICDS_PACKAGE_07" name="J-CLCC [IC]" value="7"/>
                <list-param-item code="HMC_ICDS_PACKAGE_08" name="CLCC [IC]" value="8"/>
                <list-param-item code="HMC_ICDS_PACKAGE_09" name="SOJ [IC]" value="9"/>
                <list-param-item code="HMC_ICDS_PACKAGE_10" name="SO, SOP, GROUND, SOIC, SOW [IC]" value="10"/>
                <list-param-item code="HMC_ICDS_PACKAGE_11" name="TSOP I, TSOP II [IC]" value="11"/>
                <list-param-item code="HMC_ICDS_PACKAGE_12" name="SSOP, VSOP, QSOP [IC]" value="12"/>
                <list-param-item code="HMC_ICDS_PACKAGE_13" name="TSSOP, MSOP, ?SO, ?MAX, TVSOP [IC]" value="13"/>
                <list-param-item code="HMC_ICDS_PACKAGE_14" name="PBGA CSP BT 0.8 and 0.75 mm [IC]" value="14"/>
                <list-param-item code="HMC_ICDS_PACKAGE_15" name="PBGA flex 0.8 mm [IC]" value="15"/>
                <list-param-item code="HMC_ICDS_PACKAGE_16" name="PBGA BT 1.00 mm [IC]" value="16"/>
                <list-param-item code="HMC_ICDS_PACKAGE_17" name="PBGA 1.27mm [IC]" value="17"/>
                <list-param-item code="HMC_ICDS_PACKAGE_18" name="Power BGA (TBGA, SBGA, etc.) [IC]" value="18"/>
                <list-param-item code="HMC_ICDS_PACKAGE_19" name="CBGA [IC]" value="19"/>
                <list-param-item code="HMC_ICDS_PACKAGE_20" name="DBGA [IC]" value="20"/>
                <list-param-item code="HMC_ICDS_PACKAGE_21" name="CGA IC [IC]" value="21"/>
                <list-param-item code="HMC_ICDS_PACKAGE_22" name="SOT23-3 [DS]" value="22"/>
                <list-param-item code="HMC_ICDS_PACKAGE_23" name="SOT23-5 [DS]" value="23"/>
                <list-param-item code="HMC_ICDS_PACKAGE_24" name="SOT23-6 [DS]" value="24"/>
                <list-param-item code="HMC_ICDS_PACKAGE_25" name="SOT143 [DS]" value="25"/>
                <list-param-item code="HMC_ICDS_PACKAGE_26" name="SOT323 [DS]" value="26"/>
                <list-param-item code="HMC_ICDS_PACKAGE_27" name="SOT346 [DS]" value="27"/>
                <list-param-item code="HMC_ICDS_PACKAGE_28" name="SOT353 [DS]" value="28"/>
                <list-param-item code="HMC_ICDS_PACKAGE_29" name="SOT363 [DS]" value="29"/>
                <list-param-item code="HMC_ICDS_PACKAGE_30" name="SOD123 [DS]" value="30"/>
                <list-param-item code="HMC_ICDS_PACKAGE_31" name="SOD323 [DS]" value="31"/>
                <list-param-item code="HMC_ICDS_PACKAGE_32" name="SOD523 [DS]" value="32"/>
                <list-param-item code="HMC_ICDS_PACKAGE_33" name="SOT223 [DS]" value="33"/>
                <list-param-item code="HMC_ICDS_PACKAGE_34" name="SOT243 [DS]" value="34"/>
                <list-param-item code="HMC_ICDS_PACKAGE_35" name="SOT343 [DS]" value="35"/>
                <list-param-item code="HMC_ICDS_PACKAGE_36" name="SOT89 [DS]" value="36"/>
                <list-param-item code="HMC_ICDS_PACKAGE_37" name="SOT194 [DS]" value="37"/>
                <list-param-item code="HMC_ICDS_PACKAGE_38" name="SOD6 [DS]" value="38"/>
                <list-param-item code="HMC_ICDS_PACKAGE_39" name="SOD15 [DS]" value="39"/>
                <list-param-item code="HMC_ICDS_PACKAGE_40" name="DPAK [DS]" value="40"/>
                <list-param-item code="HMC_ICDS_PACKAGE_41" name="D2PAK [DS]" value="41"/>
                <list-param-item code="HMC_ICDS_PACKAGE_42" name="D3PAK [DS]" value="42"/>
                <list-param-item code="HMC_ICDS_PACKAGE_43" name="ISOTOP [DS]" value="43"/>
                <list-param-item code="HMC_ICDS_PACKAGE_44" name="SOD80 [DS]" value="44"/>
                <list-param-item code="HMC_ICDS_PACKAGE_45" name="SOD87 [DS]" value="45"/>
            </family-param>
            <family-param code="hmc_np" name="N_pin" value-type="NUMERIC" optional="false" in-hmc="false"/>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
            <family-param code="hmc_v_rated" name="V_rated" value-type="NUMERIC" optional="false" in-hmc="false"/>
            <app-stress code="hmc_v_appl" name="V_applied" value-type="NUMERIC" optional="false" in-hmc="false"/>
            <app-stress code="hmc_delta_t" name="ΔT" value-type="NUMERIC" unit="°C" optional="false" in-hmc="false"/>
        </family>
        <family code="hmc_dr" name="Micro-components - Deposited resistors">
            <family-param code="hmc_mount_type" name="Mount type (H&amp;M)" value-type="LIST" optional="false"
                          in-hmc="false">
                <list-param-item code="HMC_MOUNT_TYPE_01" name="By gluing (conductive glue)" value="1"/>
                <list-param-item code="HMC_MOUNT_TYPE_02" name="By soldering (solder)" value="2"/>
            </family-param>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
            <family-param code="hmc_dr_tole" name="Tolerance" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="HMC_DR_TOLERANCE_01" name="Tolerance above 5%" value="1"/>
                <list-param-item code="HMC_DR_TOLERANCE_02" name="Tolerance from 1 to 5%" value="2"/>
                <list-param-item code="HMC_DR_TOLERANCE_03" name="Tolerance less than 1%" value="3"/>
            </family-param>
            <family-param code="hmc_dr_re" name="R_e" value-type="NUMERIC" optional="false" in-hmc="false"/>
            <family-param code="hmc_dr_rm" name="R_m" value-type="NUMERIC" optional="false" in-hmc="false"/>
        </family>
        <family code="hmc_dc" name="Micro-components - Deposited capacitor">
            <family-param code="hmc_mount_type" name="Mount type (H&amp;M)" value-type="LIST" optional="false"
                          in-hmc="false">
                <list-param-item code="HMC_MOUNT_TYPE_01" name="By gluing (conductive glue)" value="1"/>
                <list-param-item code="HMC_MOUNT_TYPE_02" name="By soldering (solder)" value="2"/>
            </family-param>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
            <family-param code="ec_v_rated" name="V_rated" value-type="NUMERIC" unit="V" optional="false"
                          in-hmc="false"/>
            <app-stress code="ec_v_appl" name="V_applied" value-type="NUMERIC" unit="V" optional="false"
                        in-hmc="false"/>
        </family>
    </macro-family>
    <macro-family code="mwrf">
        <family code="mwrf_ganic" name="GaN MMIC RF/MW components">
            <family-param code="ec_icds_pkg" name="Package" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="EC_IC_PKG_01" name="PDIP [EC_IC]" value="1"/>
                <list-param-item code="EC_IC_PKG_02" name="CERDIP, CDIP [EC_IC]" value="2"/>
                <list-param-item code="EC_IC_PKG_03" name="PQFP [EC_IC]" value="3"/>
                <list-param-item code="EC_IC_PKG_04" name="TQFP, LQFP [EC_IC]" value="4"/>
                <list-param-item code="EC_IC_PKG_05" name="Power QFP [EC_IC]" value="5"/>
                <list-param-item code="EC_IC_PKG_06" name="CERPACK [EC_IC]" value="6"/>
                <list-param-item code="EC_IC_PKG_07" name="CQFP [EC_IC]" value="7"/>
                <list-param-item code="EC_IC_PKG_08" name="PLCC [EC_IC]" value="8"/>
                <list-param-item code="EC_IC_PKG_09" name="J-LCC [EC_IC]" value="9"/>
                <list-param-item code="EC_IC_PKG_10" name="CLCC [EC_IC]" value="10"/>
                <list-param-item code="EC_IC_PKG_11" name="SOJ [EC_IC]" value="11"/>
                <list-param-item code="EC_IC_PKG_12" name="SO [EC_IC]" value="12"/>
                <list-param-item code="EC_IC_PKG_13" name="TSOP [EC_IC]" value="13"/>
                <list-param-item code="EC_IC_PKG_14" name="SSOP, QSOP [EC_IC]" value="14"/>
                <list-param-item code="EC_IC_PKG_15" name="TSSOP, MSOP [EC_IC]" value="15"/>
                <list-param-item code="EC_IC_PKG_16" name="QFN, DFN ≥0.5 mm [EC_IC]" value="16"/>
                <list-param-item code="EC_IC_PKG_17" name="QFN 0.4 mm [EC_IC]" value="17"/>
                <list-param-item code="EC_IC_PKG_18" name="LGA Plastic [EC_IC]" value="18"/>
                <list-param-item code="EC_IC_PKG_19" name="PBGA &lt;0.5 mm [EC_IC]" value="19"/>
                <list-param-item code="EC_IC_PKG_20" name="PBGA 0.5 mm [EC_IC]" value="20"/>
                <list-param-item code="EC_IC_PKG_21" name="PBGA 0.65 mm [EC_IC]" value="21"/>
                <list-param-item code="EC_IC_PKG_22" name="PBGA BT 0.8 mm [EC_IC]" value="22"/>
                <list-param-item code="EC_IC_PKG_23" name="PBGA flex 0.8 mm [EC_IC]" value="23"/>
                <list-param-item code="EC_IC_PKG_24" name="PBGA BOC 0.8 mm (memories) [EC_IC]" value="24"/>
                <list-param-item code="EC_IC_PKG_25" name="PBGA BT 1.00 mm [EC_IC]" value="25"/>
                <list-param-item code="EC_IC_PKG_26" name="PBGA 1.27 mm [EC_IC]" value="26"/>
                <list-param-item code="EC_IC_PKG_27" name="Power BGA [EC_IC]" value="27"/>
                <list-param-item code="EC_IC_PKG_28" name="BGA WLP &lt;0.5 mm [EC_IC]" value="28"/>
                <list-param-item code="EC_IC_PKG_29" name="BGA WLP 0.5 mm [EC_IC]" value="29"/>
                <list-param-item code="EC_IC_PKG_30" name="FC-PBGA 0.8 mm [EC_IC]" value="30"/>
                <list-param-item code="EC_IC_PKG_31" name="FC-PBGA 1 mm [EC_IC]" value="31"/>
                <list-param-item code="EC_IC_PKG_32" name="CBGA [EC_IC]" value="32"/>
                <list-param-item code="EC_IC_PKG_33" name="DBGA [EC_IC]" value="33"/>
                <list-param-item code="EC_IC_PKG_34" name="CI CGA [EC_IC]" value="34"/>
                <list-param-item code="EC_IC_PKG_35" name="CPGA [EC_IC]" value="35"/>
                <list-param-item code="EC_DS_PKG_01" name="CB417 [EC_DS]" value="101"/>
                <list-param-item code="EC_DS_PKG_02" name="CB429 [EC_DS]" value="102"/>
                <list-param-item code="EC_DS_PKG_03" name="DO13, DO202AA [EC_DS]" value="103"/>
                <list-param-item code="EC_DS_PKG_04" name="DO15, DO204AC [EC_DS]" value="104"/>
                <list-param-item code="EC_DS_PKG_05" name="DO27, DO201AA [EC_DS]" value="105"/>
                <list-param-item code="EC_DS_PKG_06" name="DO35, DO204AH [EC_DS]" value="106"/>
                <list-param-item code="EC_DS_PKG_07" name="DO41, DO204AL [EC_DS]" value="107"/>
                <list-param-item code="EC_DS_PKG_08" name="DO92 [EC_DS]" value="108"/>
                <list-param-item code="EC_DS_PKG_09" name="F126 [EC_DS]" value="109"/>
                <list-param-item code="EC_DS_PKG_10" name="SIL, SIP, ZIP [EC_DS]" value="110"/>
                <list-param-item code="EC_DS_PKG_11" name="TO92, SOT54, SC43, TO226AA [EC_DS]" value="111"/>
                <list-param-item code="EC_DS_PKG_12" name="TO126, SOT32, TO225AA [EC_DS]" value="112"/>
                <list-param-item code="EC_DS_PKG_13" name="TO202 [EC_DS]" value="113"/>
                <list-param-item code="EC_DS_PKG_14" name="SOT23-3, TO236AB [EC_DS]" value="114"/>
                <list-param-item code="EC_DS_PKG_15" name="SOT23-5, SC74A, SOT25 [EC_DS]" value="115"/>
                <list-param-item code="EC_DS_PKG_16" name="SOT23-6, SC74, SOT26, SOT457 [EC_DS]" value="116"/>
                <list-param-item code="EC_DS_PKG_17" name="SOT143, TO253AA, SC61B [EC_DS]" value="117"/>
                <list-param-item code="EC_DS_PKG_18" name="SOT323, SC70 [EC_DS]" value="118"/>
                <list-param-item code="EC_DS_PKG_19" name="SOT346, SC59, TO236AA [EC_DS]" value="119"/>
                <list-param-item code="EC_DS_PKG_20" name="SOT353, SC70-5, SC88A [EC_DS]" value="120"/>
                <list-param-item code="EC_DS_PKG_21" name="SOT363, SC70-6, SC88 [EC_DS]" value="121"/>
                <list-param-item code="EC_DS_PKG_22" name="SOD123 [EC_DS]" value="122"/>
                <list-param-item code="EC_DS_PKG_23" name="SOD323, SC76 [EC_DS]" value="123"/>
                <list-param-item code="EC_DS_PKG_24" name="SOD523, SC79 [EC_DS]" value="124"/>
                <list-param-item code="EC_DS_PKG_25" name="SOT223, SC73, TO261AA [EC_DS]" value="125"/>
                <list-param-item code="EC_DS_PKG_26" name="SOT243 [EC_DS]" value="126"/>
                <list-param-item code="EC_DS_PKG_27" name="SOT343, SC82 [EC_DS]" value="127"/>
                <list-param-item code="EC_DS_PKG_28" name="SOT89, SC62, TO243AA [EC_DS]" value="128"/>
                <list-param-item code="EC_DS_PKG_29" name="SOT194 [EC_DS]" value="129"/>
                <list-param-item code="EC_DS_PKG_30" name="TO218, ISOWATT218 [EC_DS]" value="130"/>
                <list-param-item code="EC_DS_PKG_31" name="TO220, TO220-5, ISOWATT220, TO220XX [EC_DS]" value="131"/>
                <list-param-item code="EC_DS_PKG_32" name="TO247, Max247, Super247, SOT429 [EC_DS]" value="132"/>
                <list-param-item code="EC_DS_PKG_33" name="ISOWATT [EC_DS]" value="133"/>
                <list-param-item code="EC_DS_PKG_34" name="DO220 [EC_DS]" value="134"/>
                <list-param-item code="EC_DS_PKG_35" name="IPACK, TO251AA [EC_DS]" value="135"/>
                <list-param-item code="EC_DS_PKG_36" name="SOT82, TO225 [EC_DS]" value="136"/>
                <list-param-item code="EC_DS_PKG_37" name="SOD6, DO214AA, SMB-J [EC_DS]" value="137"/>
                <list-param-item code="EC_DS_PKG_38" name="SOD15, DO214AB, SMC-J [EC_DS]" value="138"/>
                <list-param-item code="EC_DS_PKG_39" name="DPAK, TO252AA, SC63, SOT428 [EC_DS]" value="139"/>
                <list-param-item code="EC_DS_PKG_40" name="D2PAK, TO263, SC83A, SMD220 [EC_DS]" value="140"/>
                <list-param-item code="EC_DS_PKG_41" name="D3PAK, TO268 [EC_DS]" value="141"/>
                <list-param-item code="EC_DS_PKG_42" name="ISOTOP, SOT227, TO244, Half-Pak [EC_DS]" value="142"/>
                <list-param-item code="EC_DS_PKG_43" name="SOD80, Mini-MELF, DO213AA [EC_DS]" value="143"/>
                <list-param-item code="EC_DS_PKG_44" name="SOD87, MELF, DO213AB [EC_DS]" value="144"/>
                <list-param-item code="EC_DS_PKG_45" name="TO18, TO71, TO72, SOT31, SOT18 [EC_DS]" value="145"/>
                <list-param-item code="EC_DS_PKG_46" name="TO39, SOT5 [EC_DS]" value="146"/>
                <list-param-item code="EC_DS_PKG_47" name="TO52 [EC_DS]" value="147"/>
                <list-param-item code="EC_DS_PKG_48" name="SOT553 [EC_DS]" value="148"/>
                <list-param-item code="EC_DS_PKG_49" name="SOT563 [EC_DS]" value="149"/>
                <list-param-item code="EC_DS_PKG_50" name="SOT563F [EC_DS]" value="150"/>
                <list-param-item code="EC_DS_PKG_51" name="SOT663 [EC_DS]" value="151"/>
                <list-param-item code="EC_DS_PKG_52" name="SOT666 [EC_DS]" value="152"/>
                <list-param-item code="EC_DS_PKG_53" name="SOT66 [EC_DS]" value="153"/>
                <list-param-item code="EC_DS_PKG_54" name="SOT665 [EC_DS]" value="154"/>
                <list-param-item code="EC_DS_PKG_55" name="SOT490 [EC_DS]" value="155"/>
            </family-param>
            <family-param code="ec_np" name="Np" value-type="NUMERIC" optional="false" in-hmc="false"/>
            <family-param code="ec_underfill" name="Underfill" value-type="BOOL" optional="false" in-hmc="false"/>
            <app-stress code="mwrf_delta_t" name="Rise of temperature" value-type="NUMERIC" unit="°C" optional="false"
                        in-hmc="false"/>
            <app-stress code="mwrf_eta" name="&amp;eta;" value-type="NUMERIC" optional="false" in-hmc="false"/>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="mwrf_gands" name="GaN discrete semiconductors RF/MW components">
            <family-param code="ec_icds_pkg" name="Package" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="EC_IC_PKG_01" name="PDIP [EC_IC]" value="1"/>
                <list-param-item code="EC_IC_PKG_02" name="CERDIP, CDIP [EC_IC]" value="2"/>
                <list-param-item code="EC_IC_PKG_03" name="PQFP [EC_IC]" value="3"/>
                <list-param-item code="EC_IC_PKG_04" name="TQFP, LQFP [EC_IC]" value="4"/>
                <list-param-item code="EC_IC_PKG_05" name="Power QFP [EC_IC]" value="5"/>
                <list-param-item code="EC_IC_PKG_06" name="CERPACK [EC_IC]" value="6"/>
                <list-param-item code="EC_IC_PKG_07" name="CQFP [EC_IC]" value="7"/>
                <list-param-item code="EC_IC_PKG_08" name="PLCC [EC_IC]" value="8"/>
                <list-param-item code="EC_IC_PKG_09" name="J-LCC [EC_IC]" value="9"/>
                <list-param-item code="EC_IC_PKG_10" name="CLCC [EC_IC]" value="10"/>
                <list-param-item code="EC_IC_PKG_11" name="SOJ [EC_IC]" value="11"/>
                <list-param-item code="EC_IC_PKG_12" name="SO [EC_IC]" value="12"/>
                <list-param-item code="EC_IC_PKG_13" name="TSOP [EC_IC]" value="13"/>
                <list-param-item code="EC_IC_PKG_14" name="SSOP, QSOP [EC_IC]" value="14"/>
                <list-param-item code="EC_IC_PKG_15" name="TSSOP, MSOP [EC_IC]" value="15"/>
                <list-param-item code="EC_IC_PKG_16" name="QFN, DFN ≥0.5 mm [EC_IC]" value="16"/>
                <list-param-item code="EC_IC_PKG_17" name="QFN 0.4 mm [EC_IC]" value="17"/>
                <list-param-item code="EC_IC_PKG_18" name="LGA Plastic [EC_IC]" value="18"/>
                <list-param-item code="EC_IC_PKG_19" name="PBGA &lt;0.5 mm [EC_IC]" value="19"/>
                <list-param-item code="EC_IC_PKG_20" name="PBGA 0.5 mm [EC_IC]" value="20"/>
                <list-param-item code="EC_IC_PKG_21" name="PBGA 0.65 mm [EC_IC]" value="21"/>
                <list-param-item code="EC_IC_PKG_22" name="PBGA BT 0.8 mm [EC_IC]" value="22"/>
                <list-param-item code="EC_IC_PKG_23" name="PBGA flex 0.8 mm [EC_IC]" value="23"/>
                <list-param-item code="EC_IC_PKG_24" name="PBGA BOC 0.8 mm (memories) [EC_IC]" value="24"/>
                <list-param-item code="EC_IC_PKG_25" name="PBGA BT 1.00 mm [EC_IC]" value="25"/>
                <list-param-item code="EC_IC_PKG_26" name="PBGA 1.27 mm [EC_IC]" value="26"/>
                <list-param-item code="EC_IC_PKG_27" name="Power BGA [EC_IC]" value="27"/>
                <list-param-item code="EC_IC_PKG_28" name="BGA WLP &lt;0.5 mm [EC_IC]" value="28"/>
                <list-param-item code="EC_IC_PKG_29" name="BGA WLP 0.5 mm [EC_IC]" value="29"/>
                <list-param-item code="EC_IC_PKG_30" name="FC-PBGA 0.8 mm [EC_IC]" value="30"/>
                <list-param-item code="EC_IC_PKG_31" name="FC-PBGA 1 mm [EC_IC]" value="31"/>
                <list-param-item code="EC_IC_PKG_32" name="CBGA [EC_IC]" value="32"/>
                <list-param-item code="EC_IC_PKG_33" name="DBGA [EC_IC]" value="33"/>
                <list-param-item code="EC_IC_PKG_34" name="CI CGA [EC_IC]" value="34"/>
                <list-param-item code="EC_IC_PKG_35" name="CPGA [EC_IC]" value="35"/>
                <list-param-item code="EC_DS_PKG_01" name="CB417 [EC_DS]" value="101"/>
                <list-param-item code="EC_DS_PKG_02" name="CB429 [EC_DS]" value="102"/>
                <list-param-item code="EC_DS_PKG_03" name="DO13, DO202AA [EC_DS]" value="103"/>
                <list-param-item code="EC_DS_PKG_04" name="DO15, DO204AC [EC_DS]" value="104"/>
                <list-param-item code="EC_DS_PKG_05" name="DO27, DO201AA [EC_DS]" value="105"/>
                <list-param-item code="EC_DS_PKG_06" name="DO35, DO204AH [EC_DS]" value="106"/>
                <list-param-item code="EC_DS_PKG_07" name="DO41, DO204AL [EC_DS]" value="107"/>
                <list-param-item code="EC_DS_PKG_08" name="DO92 [EC_DS]" value="108"/>
                <list-param-item code="EC_DS_PKG_09" name="F126 [EC_DS]" value="109"/>
                <list-param-item code="EC_DS_PKG_10" name="SIL, SIP, ZIP [EC_DS]" value="110"/>
                <list-param-item code="EC_DS_PKG_11" name="TO92, SOT54, SC43, TO226AA [EC_DS]" value="111"/>
                <list-param-item code="EC_DS_PKG_12" name="TO126, SOT32, TO225AA [EC_DS]" value="112"/>
                <list-param-item code="EC_DS_PKG_13" name="TO202 [EC_DS]" value="113"/>
                <list-param-item code="EC_DS_PKG_14" name="SOT23-3, TO236AB [EC_DS]" value="114"/>
                <list-param-item code="EC_DS_PKG_15" name="SOT23-5, SC74A, SOT25 [EC_DS]" value="115"/>
                <list-param-item code="EC_DS_PKG_16" name="SOT23-6, SC74, SOT26, SOT457 [EC_DS]" value="116"/>
                <list-param-item code="EC_DS_PKG_17" name="SOT143, TO253AA, SC61B [EC_DS]" value="117"/>
                <list-param-item code="EC_DS_PKG_18" name="SOT323, SC70 [EC_DS]" value="118"/>
                <list-param-item code="EC_DS_PKG_19" name="SOT346, SC59, TO236AA [EC_DS]" value="119"/>
                <list-param-item code="EC_DS_PKG_20" name="SOT353, SC70-5, SC88A [EC_DS]" value="120"/>
                <list-param-item code="EC_DS_PKG_21" name="SOT363, SC70-6, SC88 [EC_DS]" value="121"/>
                <list-param-item code="EC_DS_PKG_22" name="SOD123 [EC_DS]" value="122"/>
                <list-param-item code="EC_DS_PKG_23" name="SOD323, SC76 [EC_DS]" value="123"/>
                <list-param-item code="EC_DS_PKG_24" name="SOD523, SC79 [EC_DS]" value="124"/>
                <list-param-item code="EC_DS_PKG_25" name="SOT223, SC73, TO261AA [EC_DS]" value="125"/>
                <list-param-item code="EC_DS_PKG_26" name="SOT243 [EC_DS]" value="126"/>
                <list-param-item code="EC_DS_PKG_27" name="SOT343, SC82 [EC_DS]" value="127"/>
                <list-param-item code="EC_DS_PKG_28" name="SOT89, SC62, TO243AA [EC_DS]" value="128"/>
                <list-param-item code="EC_DS_PKG_29" name="SOT194 [EC_DS]" value="129"/>
                <list-param-item code="EC_DS_PKG_30" name="TO218, ISOWATT218 [EC_DS]" value="130"/>
                <list-param-item code="EC_DS_PKG_31" name="TO220, TO220-5, ISOWATT220, TO220XX [EC_DS]" value="131"/>
                <list-param-item code="EC_DS_PKG_32" name="TO247, Max247, Super247, SOT429 [EC_DS]" value="132"/>
                <list-param-item code="EC_DS_PKG_33" name="ISOWATT [EC_DS]" value="133"/>
                <list-param-item code="EC_DS_PKG_34" name="DO220 [EC_DS]" value="134"/>
                <list-param-item code="EC_DS_PKG_35" name="IPACK, TO251AA [EC_DS]" value="135"/>
                <list-param-item code="EC_DS_PKG_36" name="SOT82, TO225 [EC_DS]" value="136"/>
                <list-param-item code="EC_DS_PKG_37" name="SOD6, DO214AA, SMB-J [EC_DS]" value="137"/>
                <list-param-item code="EC_DS_PKG_38" name="SOD15, DO214AB, SMC-J [EC_DS]" value="138"/>
                <list-param-item code="EC_DS_PKG_39" name="DPAK, TO252AA, SC63, SOT428 [EC_DS]" value="139"/>
                <list-param-item code="EC_DS_PKG_40" name="D2PAK, TO263, SC83A, SMD220 [EC_DS]" value="140"/>
                <list-param-item code="EC_DS_PKG_41" name="D3PAK, TO268 [EC_DS]" value="141"/>
                <list-param-item code="EC_DS_PKG_42" name="ISOTOP, SOT227, TO244, Half-Pak [EC_DS]" value="142"/>
                <list-param-item code="EC_DS_PKG_43" name="SOD80, Mini-MELF, DO213AA [EC_DS]" value="143"/>
                <list-param-item code="EC_DS_PKG_44" name="SOD87, MELF, DO213AB [EC_DS]" value="144"/>
                <list-param-item code="EC_DS_PKG_45" name="TO18, TO71, TO72, SOT31, SOT18 [EC_DS]" value="145"/>
                <list-param-item code="EC_DS_PKG_46" name="TO39, SOT5 [EC_DS]" value="146"/>
                <list-param-item code="EC_DS_PKG_47" name="TO52 [EC_DS]" value="147"/>
                <list-param-item code="EC_DS_PKG_48" name="SOT553 [EC_DS]" value="148"/>
                <list-param-item code="EC_DS_PKG_49" name="SOT563 [EC_DS]" value="149"/>
                <list-param-item code="EC_DS_PKG_50" name="SOT563F [EC_DS]" value="150"/>
                <list-param-item code="EC_DS_PKG_51" name="SOT663 [EC_DS]" value="151"/>
                <list-param-item code="EC_DS_PKG_52" name="SOT666 [EC_DS]" value="152"/>
                <list-param-item code="EC_DS_PKG_53" name="SOT66 [EC_DS]" value="153"/>
                <list-param-item code="EC_DS_PKG_54" name="SOT665 [EC_DS]" value="154"/>
                <list-param-item code="EC_DS_PKG_55" name="SOT490 [EC_DS]" value="155"/>
            </family-param>
            <family-param code="ec_np" name="Np" value-type="NUMERIC" optional="false" in-hmc="false"/>
            <family-param code="ec_underfill" name="Underfill" value-type="BOOL" optional="false" in-hmc="false"/>
            <app-stress code="mwrf_delta_t" name="Rise of temperature" value-type="NUMERIC" unit="°C" optional="false"
                        in-hmc="false"/>
            <app-stress code="mwrf_eta" name="&amp;eta;" value-type="NUMERIC" optional="false" in-hmc="false"/>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="mwrf_gaas" name="GaAs RF/MW components">
            <family-param code="mwrf_gaas_type" name="Type" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="MWRF_GAAS_TYPE_01" name="GaAs components, MMICs (incl. LNAs)" value="1"/>
                <list-param-item code="MWRF_GAAS_TYPE_02"
                                 name="GaAs components, discrete semiconductors (incl. transistors)" value="2"/>
            </family-param>
            <family-param code="ec_icds_pkg" name="Package" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="EC_IC_PKG_01" name="PDIP [EC_IC]" value="1"/>
                <list-param-item code="EC_IC_PKG_02" name="CERDIP, CDIP [EC_IC]" value="2"/>
                <list-param-item code="EC_IC_PKG_03" name="PQFP [EC_IC]" value="3"/>
                <list-param-item code="EC_IC_PKG_04" name="TQFP, LQFP [EC_IC]" value="4"/>
                <list-param-item code="EC_IC_PKG_05" name="Power QFP [EC_IC]" value="5"/>
                <list-param-item code="EC_IC_PKG_06" name="CERPACK [EC_IC]" value="6"/>
                <list-param-item code="EC_IC_PKG_07" name="CQFP [EC_IC]" value="7"/>
                <list-param-item code="EC_IC_PKG_08" name="PLCC [EC_IC]" value="8"/>
                <list-param-item code="EC_IC_PKG_09" name="J-LCC [EC_IC]" value="9"/>
                <list-param-item code="EC_IC_PKG_10" name="CLCC [EC_IC]" value="10"/>
                <list-param-item code="EC_IC_PKG_11" name="SOJ [EC_IC]" value="11"/>
                <list-param-item code="EC_IC_PKG_12" name="SO [EC_IC]" value="12"/>
                <list-param-item code="EC_IC_PKG_13" name="TSOP [EC_IC]" value="13"/>
                <list-param-item code="EC_IC_PKG_14" name="SSOP, QSOP [EC_IC]" value="14"/>
                <list-param-item code="EC_IC_PKG_15" name="TSSOP, MSOP [EC_IC]" value="15"/>
                <list-param-item code="EC_IC_PKG_16" name="QFN, DFN ≥0.5 mm [EC_IC]" value="16"/>
                <list-param-item code="EC_IC_PKG_17" name="QFN 0.4 mm [EC_IC]" value="17"/>
                <list-param-item code="EC_IC_PKG_18" name="LGA Plastic [EC_IC]" value="18"/>
                <list-param-item code="EC_IC_PKG_19" name="PBGA &lt;0.5 mm [EC_IC]" value="19"/>
                <list-param-item code="EC_IC_PKG_20" name="PBGA 0.5 mm [EC_IC]" value="20"/>
                <list-param-item code="EC_IC_PKG_21" name="PBGA 0.65 mm [EC_IC]" value="21"/>
                <list-param-item code="EC_IC_PKG_22" name="PBGA BT 0.8 mm [EC_IC]" value="22"/>
                <list-param-item code="EC_IC_PKG_23" name="PBGA flex 0.8 mm [EC_IC]" value="23"/>
                <list-param-item code="EC_IC_PKG_24" name="PBGA BOC 0.8 mm (memories) [EC_IC]" value="24"/>
                <list-param-item code="EC_IC_PKG_25" name="PBGA BT 1.00 mm [EC_IC]" value="25"/>
                <list-param-item code="EC_IC_PKG_26" name="PBGA 1.27 mm [EC_IC]" value="26"/>
                <list-param-item code="EC_IC_PKG_27" name="Power BGA [EC_IC]" value="27"/>
                <list-param-item code="EC_IC_PKG_28" name="BGA WLP &lt;0.5 mm [EC_IC]" value="28"/>
                <list-param-item code="EC_IC_PKG_29" name="BGA WLP 0.5 mm [EC_IC]" value="29"/>
                <list-param-item code="EC_IC_PKG_30" name="FC-PBGA 0.8 mm [EC_IC]" value="30"/>
                <list-param-item code="EC_IC_PKG_31" name="FC-PBGA 1 mm [EC_IC]" value="31"/>
                <list-param-item code="EC_IC_PKG_32" name="CBGA [EC_IC]" value="32"/>
                <list-param-item code="EC_IC_PKG_33" name="DBGA [EC_IC]" value="33"/>
                <list-param-item code="EC_IC_PKG_34" name="CI CGA [EC_IC]" value="34"/>
                <list-param-item code="EC_IC_PKG_35" name="CPGA [EC_IC]" value="35"/>
                <list-param-item code="EC_DS_PKG_01" name="CB417 [EC_DS]" value="101"/>
                <list-param-item code="EC_DS_PKG_02" name="CB429 [EC_DS]" value="102"/>
                <list-param-item code="EC_DS_PKG_03" name="DO13, DO202AA [EC_DS]" value="103"/>
                <list-param-item code="EC_DS_PKG_04" name="DO15, DO204AC [EC_DS]" value="104"/>
                <list-param-item code="EC_DS_PKG_05" name="DO27, DO201AA [EC_DS]" value="105"/>
                <list-param-item code="EC_DS_PKG_06" name="DO35, DO204AH [EC_DS]" value="106"/>
                <list-param-item code="EC_DS_PKG_07" name="DO41, DO204AL [EC_DS]" value="107"/>
                <list-param-item code="EC_DS_PKG_08" name="DO92 [EC_DS]" value="108"/>
                <list-param-item code="EC_DS_PKG_09" name="F126 [EC_DS]" value="109"/>
                <list-param-item code="EC_DS_PKG_10" name="SIL, SIP, ZIP [EC_DS]" value="110"/>
                <list-param-item code="EC_DS_PKG_11" name="TO92, SOT54, SC43, TO226AA [EC_DS]" value="111"/>
                <list-param-item code="EC_DS_PKG_12" name="TO126, SOT32, TO225AA [EC_DS]" value="112"/>
                <list-param-item code="EC_DS_PKG_13" name="TO202 [EC_DS]" value="113"/>
                <list-param-item code="EC_DS_PKG_14" name="SOT23-3, TO236AB [EC_DS]" value="114"/>
                <list-param-item code="EC_DS_PKG_15" name="SOT23-5, SC74A, SOT25 [EC_DS]" value="115"/>
                <list-param-item code="EC_DS_PKG_16" name="SOT23-6, SC74, SOT26, SOT457 [EC_DS]" value="116"/>
                <list-param-item code="EC_DS_PKG_17" name="SOT143, TO253AA, SC61B [EC_DS]" value="117"/>
                <list-param-item code="EC_DS_PKG_18" name="SOT323, SC70 [EC_DS]" value="118"/>
                <list-param-item code="EC_DS_PKG_19" name="SOT346, SC59, TO236AA [EC_DS]" value="119"/>
                <list-param-item code="EC_DS_PKG_20" name="SOT353, SC70-5, SC88A [EC_DS]" value="120"/>
                <list-param-item code="EC_DS_PKG_21" name="SOT363, SC70-6, SC88 [EC_DS]" value="121"/>
                <list-param-item code="EC_DS_PKG_22" name="SOD123 [EC_DS]" value="122"/>
                <list-param-item code="EC_DS_PKG_23" name="SOD323, SC76 [EC_DS]" value="123"/>
                <list-param-item code="EC_DS_PKG_24" name="SOD523, SC79 [EC_DS]" value="124"/>
                <list-param-item code="EC_DS_PKG_25" name="SOT223, SC73, TO261AA [EC_DS]" value="125"/>
                <list-param-item code="EC_DS_PKG_26" name="SOT243 [EC_DS]" value="126"/>
                <list-param-item code="EC_DS_PKG_27" name="SOT343, SC82 [EC_DS]" value="127"/>
                <list-param-item code="EC_DS_PKG_28" name="SOT89, SC62, TO243AA [EC_DS]" value="128"/>
                <list-param-item code="EC_DS_PKG_29" name="SOT194 [EC_DS]" value="129"/>
                <list-param-item code="EC_DS_PKG_30" name="TO218, ISOWATT218 [EC_DS]" value="130"/>
                <list-param-item code="EC_DS_PKG_31" name="TO220, TO220-5, ISOWATT220, TO220XX [EC_DS]" value="131"/>
                <list-param-item code="EC_DS_PKG_32" name="TO247, Max247, Super247, SOT429 [EC_DS]" value="132"/>
                <list-param-item code="EC_DS_PKG_33" name="ISOWATT [EC_DS]" value="133"/>
                <list-param-item code="EC_DS_PKG_34" name="DO220 [EC_DS]" value="134"/>
                <list-param-item code="EC_DS_PKG_35" name="IPACK, TO251AA [EC_DS]" value="135"/>
                <list-param-item code="EC_DS_PKG_36" name="SOT82, TO225 [EC_DS]" value="136"/>
                <list-param-item code="EC_DS_PKG_37" name="SOD6, DO214AA, SMB-J [EC_DS]" value="137"/>
                <list-param-item code="EC_DS_PKG_38" name="SOD15, DO214AB, SMC-J [EC_DS]" value="138"/>
                <list-param-item code="EC_DS_PKG_39" name="DPAK, TO252AA, SC63, SOT428 [EC_DS]" value="139"/>
                <list-param-item code="EC_DS_PKG_40" name="D2PAK, TO263, SC83A, SMD220 [EC_DS]" value="140"/>
                <list-param-item code="EC_DS_PKG_41" name="D3PAK, TO268 [EC_DS]" value="141"/>
                <list-param-item code="EC_DS_PKG_42" name="ISOTOP, SOT227, TO244, Half-Pak [EC_DS]" value="142"/>
                <list-param-item code="EC_DS_PKG_43" name="SOD80, Mini-MELF, DO213AA [EC_DS]" value="143"/>
                <list-param-item code="EC_DS_PKG_44" name="SOD87, MELF, DO213AB [EC_DS]" value="144"/>
                <list-param-item code="EC_DS_PKG_45" name="TO18, TO71, TO72, SOT31, SOT18 [EC_DS]" value="145"/>
                <list-param-item code="EC_DS_PKG_46" name="TO39, SOT5 [EC_DS]" value="146"/>
                <list-param-item code="EC_DS_PKG_47" name="TO52 [EC_DS]" value="147"/>
                <list-param-item code="EC_DS_PKG_48" name="SOT553 [EC_DS]" value="148"/>
                <list-param-item code="EC_DS_PKG_49" name="SOT563 [EC_DS]" value="149"/>
                <list-param-item code="EC_DS_PKG_50" name="SOT563F [EC_DS]" value="150"/>
                <list-param-item code="EC_DS_PKG_51" name="SOT663 [EC_DS]" value="151"/>
                <list-param-item code="EC_DS_PKG_52" name="SOT666 [EC_DS]" value="152"/>
                <list-param-item code="EC_DS_PKG_53" name="SOT66 [EC_DS]" value="153"/>
                <list-param-item code="EC_DS_PKG_54" name="SOT665 [EC_DS]" value="154"/>
                <list-param-item code="EC_DS_PKG_55" name="SOT490 [EC_DS]" value="155"/>
            </family-param>
            <family-param code="ec_np" name="Np" value-type="NUMERIC" optional="false" in-hmc="false"/>
            <family-param code="ec_underfill" name="Underfill" value-type="BOOL" optional="false" in-hmc="false"/>
            <app-stress code="mwrf_delta_t" name="Rise of temperature" value-type="NUMERIC" unit="°C" optional="false"
                        in-hmc="false"/>
            <app-stress code="mwrf_eta" name="&amp;eta;" value-type="NUMERIC" optional="false" in-hmc="false"/>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="mwrf_siic" name="Si and SiGe RF/MW integrated circuits">
            <family-param code="mwrf_siic_chip" name="Chip" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="MWRF_SIIC_CHIP_01" name="Analog circuit (power amplifier) RF and MW (MOS)"
                                 value="1"/>
                <list-param-item code="MWRF_SIIC_CHIP_02"
                                 name="Analog and mixed circuit (MOS, Bipolar, BiCMOS, MESFET, PHEMT), RF and MW"
                                 value="2"/>
                <list-param-item code="MWRF_SIIC_CHIP_03" name="Digital circuit (MOS, Bipolar, BiCMOS), RF and MW"
                                 value="3"/>
            </family-param>
            <family-param code="ec_icds_pkg" name="Package" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="EC_IC_PKG_01" name="PDIP [EC_IC]" value="1"/>
                <list-param-item code="EC_IC_PKG_02" name="CERDIP, CDIP [EC_IC]" value="2"/>
                <list-param-item code="EC_IC_PKG_03" name="PQFP [EC_IC]" value="3"/>
                <list-param-item code="EC_IC_PKG_04" name="TQFP, LQFP [EC_IC]" value="4"/>
                <list-param-item code="EC_IC_PKG_05" name="Power QFP [EC_IC]" value="5"/>
                <list-param-item code="EC_IC_PKG_06" name="CERPACK [EC_IC]" value="6"/>
                <list-param-item code="EC_IC_PKG_07" name="CQFP [EC_IC]" value="7"/>
                <list-param-item code="EC_IC_PKG_08" name="PLCC [EC_IC]" value="8"/>
                <list-param-item code="EC_IC_PKG_09" name="J-LCC [EC_IC]" value="9"/>
                <list-param-item code="EC_IC_PKG_10" name="CLCC [EC_IC]" value="10"/>
                <list-param-item code="EC_IC_PKG_11" name="SOJ [EC_IC]" value="11"/>
                <list-param-item code="EC_IC_PKG_12" name="SO [EC_IC]" value="12"/>
                <list-param-item code="EC_IC_PKG_13" name="TSOP [EC_IC]" value="13"/>
                <list-param-item code="EC_IC_PKG_14" name="SSOP, QSOP [EC_IC]" value="14"/>
                <list-param-item code="EC_IC_PKG_15" name="TSSOP, MSOP [EC_IC]" value="15"/>
                <list-param-item code="EC_IC_PKG_16" name="QFN, DFN ≥0.5 mm [EC_IC]" value="16"/>
                <list-param-item code="EC_IC_PKG_17" name="QFN 0.4 mm [EC_IC]" value="17"/>
                <list-param-item code="EC_IC_PKG_18" name="LGA Plastic [EC_IC]" value="18"/>
                <list-param-item code="EC_IC_PKG_19" name="PBGA &lt;0.5 mm [EC_IC]" value="19"/>
                <list-param-item code="EC_IC_PKG_20" name="PBGA 0.5 mm [EC_IC]" value="20"/>
                <list-param-item code="EC_IC_PKG_21" name="PBGA 0.65 mm [EC_IC]" value="21"/>
                <list-param-item code="EC_IC_PKG_22" name="PBGA BT 0.8 mm [EC_IC]" value="22"/>
                <list-param-item code="EC_IC_PKG_23" name="PBGA flex 0.8 mm [EC_IC]" value="23"/>
                <list-param-item code="EC_IC_PKG_24" name="PBGA BOC 0.8 mm (memories) [EC_IC]" value="24"/>
                <list-param-item code="EC_IC_PKG_25" name="PBGA BT 1.00 mm [EC_IC]" value="25"/>
                <list-param-item code="EC_IC_PKG_26" name="PBGA 1.27 mm [EC_IC]" value="26"/>
                <list-param-item code="EC_IC_PKG_27" name="Power BGA [EC_IC]" value="27"/>
                <list-param-item code="EC_IC_PKG_28" name="BGA WLP &lt;0.5 mm [EC_IC]" value="28"/>
                <list-param-item code="EC_IC_PKG_29" name="BGA WLP 0.5 mm [EC_IC]" value="29"/>
                <list-param-item code="EC_IC_PKG_30" name="FC-PBGA 0.8 mm [EC_IC]" value="30"/>
                <list-param-item code="EC_IC_PKG_31" name="FC-PBGA 1 mm [EC_IC]" value="31"/>
                <list-param-item code="EC_IC_PKG_32" name="CBGA [EC_IC]" value="32"/>
                <list-param-item code="EC_IC_PKG_33" name="DBGA [EC_IC]" value="33"/>
                <list-param-item code="EC_IC_PKG_34" name="CI CGA [EC_IC]" value="34"/>
                <list-param-item code="EC_IC_PKG_35" name="CPGA [EC_IC]" value="35"/>
                <list-param-item code="EC_DS_PKG_01" name="CB417 [EC_DS]" value="101"/>
                <list-param-item code="EC_DS_PKG_02" name="CB429 [EC_DS]" value="102"/>
                <list-param-item code="EC_DS_PKG_03" name="DO13, DO202AA [EC_DS]" value="103"/>
                <list-param-item code="EC_DS_PKG_04" name="DO15, DO204AC [EC_DS]" value="104"/>
                <list-param-item code="EC_DS_PKG_05" name="DO27, DO201AA [EC_DS]" value="105"/>
                <list-param-item code="EC_DS_PKG_06" name="DO35, DO204AH [EC_DS]" value="106"/>
                <list-param-item code="EC_DS_PKG_07" name="DO41, DO204AL [EC_DS]" value="107"/>
                <list-param-item code="EC_DS_PKG_08" name="DO92 [EC_DS]" value="108"/>
                <list-param-item code="EC_DS_PKG_09" name="F126 [EC_DS]" value="109"/>
                <list-param-item code="EC_DS_PKG_10" name="SIL, SIP, ZIP [EC_DS]" value="110"/>
                <list-param-item code="EC_DS_PKG_11" name="TO92, SOT54, SC43, TO226AA [EC_DS]" value="111"/>
                <list-param-item code="EC_DS_PKG_12" name="TO126, SOT32, TO225AA [EC_DS]" value="112"/>
                <list-param-item code="EC_DS_PKG_13" name="TO202 [EC_DS]" value="113"/>
                <list-param-item code="EC_DS_PKG_14" name="SOT23-3, TO236AB [EC_DS]" value="114"/>
                <list-param-item code="EC_DS_PKG_15" name="SOT23-5, SC74A, SOT25 [EC_DS]" value="115"/>
                <list-param-item code="EC_DS_PKG_16" name="SOT23-6, SC74, SOT26, SOT457 [EC_DS]" value="116"/>
                <list-param-item code="EC_DS_PKG_17" name="SOT143, TO253AA, SC61B [EC_DS]" value="117"/>
                <list-param-item code="EC_DS_PKG_18" name="SOT323, SC70 [EC_DS]" value="118"/>
                <list-param-item code="EC_DS_PKG_19" name="SOT346, SC59, TO236AA [EC_DS]" value="119"/>
                <list-param-item code="EC_DS_PKG_20" name="SOT353, SC70-5, SC88A [EC_DS]" value="120"/>
                <list-param-item code="EC_DS_PKG_21" name="SOT363, SC70-6, SC88 [EC_DS]" value="121"/>
                <list-param-item code="EC_DS_PKG_22" name="SOD123 [EC_DS]" value="122"/>
                <list-param-item code="EC_DS_PKG_23" name="SOD323, SC76 [EC_DS]" value="123"/>
                <list-param-item code="EC_DS_PKG_24" name="SOD523, SC79 [EC_DS]" value="124"/>
                <list-param-item code="EC_DS_PKG_25" name="SOT223, SC73, TO261AA [EC_DS]" value="125"/>
                <list-param-item code="EC_DS_PKG_26" name="SOT243 [EC_DS]" value="126"/>
                <list-param-item code="EC_DS_PKG_27" name="SOT343, SC82 [EC_DS]" value="127"/>
                <list-param-item code="EC_DS_PKG_28" name="SOT89, SC62, TO243AA [EC_DS]" value="128"/>
                <list-param-item code="EC_DS_PKG_29" name="SOT194 [EC_DS]" value="129"/>
                <list-param-item code="EC_DS_PKG_30" name="TO218, ISOWATT218 [EC_DS]" value="130"/>
                <list-param-item code="EC_DS_PKG_31" name="TO220, TO220-5, ISOWATT220, TO220XX [EC_DS]" value="131"/>
                <list-param-item code="EC_DS_PKG_32" name="TO247, Max247, Super247, SOT429 [EC_DS]" value="132"/>
                <list-param-item code="EC_DS_PKG_33" name="ISOWATT [EC_DS]" value="133"/>
                <list-param-item code="EC_DS_PKG_34" name="DO220 [EC_DS]" value="134"/>
                <list-param-item code="EC_DS_PKG_35" name="IPACK, TO251AA [EC_DS]" value="135"/>
                <list-param-item code="EC_DS_PKG_36" name="SOT82, TO225 [EC_DS]" value="136"/>
                <list-param-item code="EC_DS_PKG_37" name="SOD6, DO214AA, SMB-J [EC_DS]" value="137"/>
                <list-param-item code="EC_DS_PKG_38" name="SOD15, DO214AB, SMC-J [EC_DS]" value="138"/>
                <list-param-item code="EC_DS_PKG_39" name="DPAK, TO252AA, SC63, SOT428 [EC_DS]" value="139"/>
                <list-param-item code="EC_DS_PKG_40" name="D2PAK, TO263, SC83A, SMD220 [EC_DS]" value="140"/>
                <list-param-item code="EC_DS_PKG_41" name="D3PAK, TO268 [EC_DS]" value="141"/>
                <list-param-item code="EC_DS_PKG_42" name="ISOTOP, SOT227, TO244, Half-Pak [EC_DS]" value="142"/>
                <list-param-item code="EC_DS_PKG_43" name="SOD80, Mini-MELF, DO213AA [EC_DS]" value="143"/>
                <list-param-item code="EC_DS_PKG_44" name="SOD87, MELF, DO213AB [EC_DS]" value="144"/>
                <list-param-item code="EC_DS_PKG_45" name="TO18, TO71, TO72, SOT31, SOT18 [EC_DS]" value="145"/>
                <list-param-item code="EC_DS_PKG_46" name="TO39, SOT5 [EC_DS]" value="146"/>
                <list-param-item code="EC_DS_PKG_47" name="TO52 [EC_DS]" value="147"/>
                <list-param-item code="EC_DS_PKG_48" name="SOT553 [EC_DS]" value="148"/>
                <list-param-item code="EC_DS_PKG_49" name="SOT563 [EC_DS]" value="149"/>
                <list-param-item code="EC_DS_PKG_50" name="SOT563F [EC_DS]" value="150"/>
                <list-param-item code="EC_DS_PKG_51" name="SOT663 [EC_DS]" value="151"/>
                <list-param-item code="EC_DS_PKG_52" name="SOT666 [EC_DS]" value="152"/>
                <list-param-item code="EC_DS_PKG_53" name="SOT66 [EC_DS]" value="153"/>
                <list-param-item code="EC_DS_PKG_54" name="SOT665 [EC_DS]" value="154"/>
                <list-param-item code="EC_DS_PKG_55" name="SOT490 [EC_DS]" value="155"/>
            </family-param>
            <family-param code="ec_np" name="Np" value-type="NUMERIC" optional="false" in-hmc="false"/>
            <family-param code="ec_underfill" name="Underfill" value-type="BOOL" optional="false" in-hmc="false"/>
            <app-stress code="mwrf_delta_t" name="Rise of temperature" value-type="NUMERIC" unit="°C" optional="false"
                        in-hmc="false"/>
            <app-stress code="mwrf_eta" name="&amp;eta;" value-type="NUMERIC" optional="false" in-hmc="false"/>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="mwrf_sids" name="Si and SiGe RF/MW discrete semiconductors">
            <family-param code="mwrf_sids_type" name="Type" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="MWRF_SIDS_TYPE_01" name="Discrete semiconductor circuit, Si and SiGe, RF and MW"
                                 value="1"/>
                <list-param-item code="MWRF_SIDS_TYPE_02" name="Discrete semiconductor circuit, GaAs, RF and MW"
                                 value="2"/>
            </family-param>
            <family-param code="mwrf_sids_chip" name="Chip" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="MWRF_SIDS_CHIP_01" name="PIN, Schottky, Tunnel, varactor diodes (RF/MW)"
                                 value="1"/>
                <list-param-item code="MWRF_SIDS_CHIP_02" name="Silicon, bipolar &lt; 5W, SiGe, bipolar &lt;1W"
                                 value="2"/>
                <list-param-item code="MWRF_SIDS_CHIP_03" name="Silicon, bipolar &gt; 5W" value="3"/>
                <list-param-item code="MWRF_SIDS_CHIP_04" name="Silicon, MOS &gt; 5W" value="4"/>
            </family-param>
            <family-param code="ec_icds_pkg" name="Package" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="EC_IC_PKG_01" name="PDIP [EC_IC]" value="1"/>
                <list-param-item code="EC_IC_PKG_02" name="CERDIP, CDIP [EC_IC]" value="2"/>
                <list-param-item code="EC_IC_PKG_03" name="PQFP [EC_IC]" value="3"/>
                <list-param-item code="EC_IC_PKG_04" name="TQFP, LQFP [EC_IC]" value="4"/>
                <list-param-item code="EC_IC_PKG_05" name="Power QFP [EC_IC]" value="5"/>
                <list-param-item code="EC_IC_PKG_06" name="CERPACK [EC_IC]" value="6"/>
                <list-param-item code="EC_IC_PKG_07" name="CQFP [EC_IC]" value="7"/>
                <list-param-item code="EC_IC_PKG_08" name="PLCC [EC_IC]" value="8"/>
                <list-param-item code="EC_IC_PKG_09" name="J-LCC [EC_IC]" value="9"/>
                <list-param-item code="EC_IC_PKG_10" name="CLCC [EC_IC]" value="10"/>
                <list-param-item code="EC_IC_PKG_11" name="SOJ [EC_IC]" value="11"/>
                <list-param-item code="EC_IC_PKG_12" name="SO [EC_IC]" value="12"/>
                <list-param-item code="EC_IC_PKG_13" name="TSOP [EC_IC]" value="13"/>
                <list-param-item code="EC_IC_PKG_14" name="SSOP, QSOP [EC_IC]" value="14"/>
                <list-param-item code="EC_IC_PKG_15" name="TSSOP, MSOP [EC_IC]" value="15"/>
                <list-param-item code="EC_IC_PKG_16" name="QFN, DFN ≥0.5 mm [EC_IC]" value="16"/>
                <list-param-item code="EC_IC_PKG_17" name="QFN 0.4 mm [EC_IC]" value="17"/>
                <list-param-item code="EC_IC_PKG_18" name="LGA Plastic [EC_IC]" value="18"/>
                <list-param-item code="EC_IC_PKG_19" name="PBGA &lt;0.5 mm [EC_IC]" value="19"/>
                <list-param-item code="EC_IC_PKG_20" name="PBGA 0.5 mm [EC_IC]" value="20"/>
                <list-param-item code="EC_IC_PKG_21" name="PBGA 0.65 mm [EC_IC]" value="21"/>
                <list-param-item code="EC_IC_PKG_22" name="PBGA BT 0.8 mm [EC_IC]" value="22"/>
                <list-param-item code="EC_IC_PKG_23" name="PBGA flex 0.8 mm [EC_IC]" value="23"/>
                <list-param-item code="EC_IC_PKG_24" name="PBGA BOC 0.8 mm (memories) [EC_IC]" value="24"/>
                <list-param-item code="EC_IC_PKG_25" name="PBGA BT 1.00 mm [EC_IC]" value="25"/>
                <list-param-item code="EC_IC_PKG_26" name="PBGA 1.27 mm [EC_IC]" value="26"/>
                <list-param-item code="EC_IC_PKG_27" name="Power BGA [EC_IC]" value="27"/>
                <list-param-item code="EC_IC_PKG_28" name="BGA WLP &lt;0.5 mm [EC_IC]" value="28"/>
                <list-param-item code="EC_IC_PKG_29" name="BGA WLP 0.5 mm [EC_IC]" value="29"/>
                <list-param-item code="EC_IC_PKG_30" name="FC-PBGA 0.8 mm [EC_IC]" value="30"/>
                <list-param-item code="EC_IC_PKG_31" name="FC-PBGA 1 mm [EC_IC]" value="31"/>
                <list-param-item code="EC_IC_PKG_32" name="CBGA [EC_IC]" value="32"/>
                <list-param-item code="EC_IC_PKG_33" name="DBGA [EC_IC]" value="33"/>
                <list-param-item code="EC_IC_PKG_34" name="CI CGA [EC_IC]" value="34"/>
                <list-param-item code="EC_IC_PKG_35" name="CPGA [EC_IC]" value="35"/>
                <list-param-item code="EC_DS_PKG_01" name="CB417 [EC_DS]" value="101"/>
                <list-param-item code="EC_DS_PKG_02" name="CB429 [EC_DS]" value="102"/>
                <list-param-item code="EC_DS_PKG_03" name="DO13, DO202AA [EC_DS]" value="103"/>
                <list-param-item code="EC_DS_PKG_04" name="DO15, DO204AC [EC_DS]" value="104"/>
                <list-param-item code="EC_DS_PKG_05" name="DO27, DO201AA [EC_DS]" value="105"/>
                <list-param-item code="EC_DS_PKG_06" name="DO35, DO204AH [EC_DS]" value="106"/>
                <list-param-item code="EC_DS_PKG_07" name="DO41, DO204AL [EC_DS]" value="107"/>
                <list-param-item code="EC_DS_PKG_08" name="DO92 [EC_DS]" value="108"/>
                <list-param-item code="EC_DS_PKG_09" name="F126 [EC_DS]" value="109"/>
                <list-param-item code="EC_DS_PKG_10" name="SIL, SIP, ZIP [EC_DS]" value="110"/>
                <list-param-item code="EC_DS_PKG_11" name="TO92, SOT54, SC43, TO226AA [EC_DS]" value="111"/>
                <list-param-item code="EC_DS_PKG_12" name="TO126, SOT32, TO225AA [EC_DS]" value="112"/>
                <list-param-item code="EC_DS_PKG_13" name="TO202 [EC_DS]" value="113"/>
                <list-param-item code="EC_DS_PKG_14" name="SOT23-3, TO236AB [EC_DS]" value="114"/>
                <list-param-item code="EC_DS_PKG_15" name="SOT23-5, SC74A, SOT25 [EC_DS]" value="115"/>
                <list-param-item code="EC_DS_PKG_16" name="SOT23-6, SC74, SOT26, SOT457 [EC_DS]" value="116"/>
                <list-param-item code="EC_DS_PKG_17" name="SOT143, TO253AA, SC61B [EC_DS]" value="117"/>
                <list-param-item code="EC_DS_PKG_18" name="SOT323, SC70 [EC_DS]" value="118"/>
                <list-param-item code="EC_DS_PKG_19" name="SOT346, SC59, TO236AA [EC_DS]" value="119"/>
                <list-param-item code="EC_DS_PKG_20" name="SOT353, SC70-5, SC88A [EC_DS]" value="120"/>
                <list-param-item code="EC_DS_PKG_21" name="SOT363, SC70-6, SC88 [EC_DS]" value="121"/>
                <list-param-item code="EC_DS_PKG_22" name="SOD123 [EC_DS]" value="122"/>
                <list-param-item code="EC_DS_PKG_23" name="SOD323, SC76 [EC_DS]" value="123"/>
                <list-param-item code="EC_DS_PKG_24" name="SOD523, SC79 [EC_DS]" value="124"/>
                <list-param-item code="EC_DS_PKG_25" name="SOT223, SC73, TO261AA [EC_DS]" value="125"/>
                <list-param-item code="EC_DS_PKG_26" name="SOT243 [EC_DS]" value="126"/>
                <list-param-item code="EC_DS_PKG_27" name="SOT343, SC82 [EC_DS]" value="127"/>
                <list-param-item code="EC_DS_PKG_28" name="SOT89, SC62, TO243AA [EC_DS]" value="128"/>
                <list-param-item code="EC_DS_PKG_29" name="SOT194 [EC_DS]" value="129"/>
                <list-param-item code="EC_DS_PKG_30" name="TO218, ISOWATT218 [EC_DS]" value="130"/>
                <list-param-item code="EC_DS_PKG_31" name="TO220, TO220-5, ISOWATT220, TO220XX [EC_DS]" value="131"/>
                <list-param-item code="EC_DS_PKG_32" name="TO247, Max247, Super247, SOT429 [EC_DS]" value="132"/>
                <list-param-item code="EC_DS_PKG_33" name="ISOWATT [EC_DS]" value="133"/>
                <list-param-item code="EC_DS_PKG_34" name="DO220 [EC_DS]" value="134"/>
                <list-param-item code="EC_DS_PKG_35" name="IPACK, TO251AA [EC_DS]" value="135"/>
                <list-param-item code="EC_DS_PKG_36" name="SOT82, TO225 [EC_DS]" value="136"/>
                <list-param-item code="EC_DS_PKG_37" name="SOD6, DO214AA, SMB-J [EC_DS]" value="137"/>
                <list-param-item code="EC_DS_PKG_38" name="SOD15, DO214AB, SMC-J [EC_DS]" value="138"/>
                <list-param-item code="EC_DS_PKG_39" name="DPAK, TO252AA, SC63, SOT428 [EC_DS]" value="139"/>
                <list-param-item code="EC_DS_PKG_40" name="D2PAK, TO263, SC83A, SMD220 [EC_DS]" value="140"/>
                <list-param-item code="EC_DS_PKG_41" name="D3PAK, TO268 [EC_DS]" value="141"/>
                <list-param-item code="EC_DS_PKG_42" name="ISOTOP, SOT227, TO244, Half-Pak [EC_DS]" value="142"/>
                <list-param-item code="EC_DS_PKG_43" name="SOD80, Mini-MELF, DO213AA [EC_DS]" value="143"/>
                <list-param-item code="EC_DS_PKG_44" name="SOD87, MELF, DO213AB [EC_DS]" value="144"/>
                <list-param-item code="EC_DS_PKG_45" name="TO18, TO71, TO72, SOT31, SOT18 [EC_DS]" value="145"/>
                <list-param-item code="EC_DS_PKG_46" name="TO39, SOT5 [EC_DS]" value="146"/>
                <list-param-item code="EC_DS_PKG_47" name="TO52 [EC_DS]" value="147"/>
                <list-param-item code="EC_DS_PKG_48" name="SOT553 [EC_DS]" value="148"/>
                <list-param-item code="EC_DS_PKG_49" name="SOT563 [EC_DS]" value="149"/>
                <list-param-item code="EC_DS_PKG_50" name="SOT563F [EC_DS]" value="150"/>
                <list-param-item code="EC_DS_PKG_51" name="SOT663 [EC_DS]" value="151"/>
                <list-param-item code="EC_DS_PKG_52" name="SOT666 [EC_DS]" value="152"/>
                <list-param-item code="EC_DS_PKG_53" name="SOT66 [EC_DS]" value="153"/>
                <list-param-item code="EC_DS_PKG_54" name="SOT665 [EC_DS]" value="154"/>
                <list-param-item code="EC_DS_PKG_55" name="SOT490 [EC_DS]" value="155"/>
            </family-param>
            <family-param code="ec_np" name="Np" value-type="NUMERIC" optional="false" in-hmc="false"/>
            <family-param code="ec_underfill" name="Underfill" value-type="BOOL" optional="false" in-hmc="false"/>
            <family-param code="mwrf_v_rated" name="V-rated" value-type="NUMERIC" unit="V" optional="false"
                          in-hmc="false"/>
            <app-stress code="mwrf_delta_t" name="Rise of temperature" value-type="NUMERIC" unit="°C" optional="false"
                        in-hmc="false"/>
            <app-stress code="mwrf_eta" name="&amp;eta;" value-type="NUMERIC" optional="false" in-hmc="false"/>
            <app-stress code="mwrf_v_appl" name="V-applied" value-type="NUMERIC" unit="V" optional="false"
                        in-hmc="false"/>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="mwrf_re" name="Surface-mounted RF/MW resistors">
            <family-param code="ec_re_type" name="Type" value-type="LIST" optional="false" in-hmc="false"
                          default-val="6">
                <list-param-item code="EC_RE_TYPE_01"
                                 name="&quot;MiniMELF&quot; fixed resistor, low-power, thin film, current use (RC), high-stability (RS)"
                                 value="1"/>
                <list-param-item code="EC_RE_TYPE_02" name="Fixed resistor, high-power (≥1W), thick film" value="2"/>
                <list-param-item code="EC_RE_TYPE_03" name="Fixed resistor, low-power, wirewound, precision" value="3"/>
                <list-param-item code="EC_RE_TYPE_04" name="Fixed resistor, high-power (≥1W), wirewound" value="4"/>
                <list-param-item code="EC_RE_TYPE_05" name="Potentiometer, non-wirewound" value="5"/>
                <list-param-item code="EC_RE_TYPE_06" name="Fixed resistor, SMD, thick film" value="6"/>
                <list-param-item code="EC_RE_TYPE_07" name="Resistor network, SMD" value="7"/>
                <list-param-item code="EC_RE_TYPE_08" name="Fixed resistor, thin film, precision, high-stability (SMD)"
                                 value="8"/>
            </family-param>
            <family-param code="ec_smd_thl" name="SMD/Through hole" value-type="LIST" optional="true" in-hmc="false">
                <list-param-item code="EC_SMD_THL_01" name="SMD" value="1"/>
                <list-param-item code="EC_SMD_THL_02" name="Through-hole" value="2"/>
            </family-param>
            <family-param code="ec_ohm" name="Ohm" value-type="NUMERIC" unit="kΩ" optional="true" in-hmc="false"/>
            <family-param code="ec_elmt_nb" name="Nb elements" value-type="NUMERIC" optional="false" in-hmc="false"/>
            <family-param code="ec_p_rated" name="P_rated" value-type="NUMERIC" unit="W" optional="false"
                          in-hmc="false"/>
            <app-stress code="ec_p_appl" name="P_applied" value-type="NUMERIC" unit="W" optional="false"
                        in-hmc="false"/>
            <app-stress code="mwrf_eta" name="&amp;eta;" value-type="NUMERIC" optional="false" in-hmc="false"/>
            <family-param code="hmc_mount_type" name="Mount type (H&amp;M)" value-type="LIST" optional="false"
                          in-hmc="true">
                <list-param-item code="HMC_MOUNT_TYPE_01" name="By gluing (conductive glue)" value="1"/>
                <list-param-item code="HMC_MOUNT_TYPE_02" name="By soldering (solder)" value="2"/>
            </family-param>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="mwrf_cc" name="Surface-mounted RF/MW ceramic capacitors">
            <family-param code="ec_cc_type" name="Type" value-type="LIST" optional="false" in-hmc="false"
                          default-val="1">
                <list-param-item code="EC_CC_TYPE_01"
                                 name="Ceramic capacitor with defined temperature coefficient (Type I)" value="1"/>
                <list-param-item code="EC_CC_TYPE_02"
                                 name="Ceramic capacitor with non-defined temperature coefficient (Type II X5R)"
                                 value="2"/>
                <list-param-item code="EC_CC_TYPE_03"
                                 name="Ceramic capacitor with non-defined temperature coefficient (Type II X7R)"
                                 value="3"/>
                <list-param-item code="EC_CC_TYPE_04"
                                 name="Ceramic capacitor with polymer terminations and a non-defined temperature coefficient (Type II X5R)"
                                 value="4"/>
                <list-param-item code="EC_CC_TYPE_05"
                                 name="Ceramic capacitor with polymer terminations and a non-defined temperature coefficient (Type II X7R)"
                                 value="5"/>
            </family-param>
            <family-param code="ec_top_end" name="Top end" value-type="BOOL" optional="false" in-hmc="false"/>
            <family-param code="ec_c_rated" name="C" value-type="NUMERIC" unit="F" optional="false" in-hmc="false"/>
            <family-param code="ec_v_rated" name="V_rated" value-type="NUMERIC" unit="V" optional="false"
                          in-hmc="false"/>
            <app-stress code="ec_v_appl" name="V_applied" value-type="NUMERIC" unit="V" optional="false"
                        in-hmc="false"/>
            <app-stress code="mwrf_eta" name="&amp;eta;" value-type="NUMERIC" optional="false" in-hmc="false"/>
            <family-param code="hmc_mount_type" name="Mount type (H&amp;M)" value-type="LIST" optional="false"
                          in-hmc="true">
                <list-param-item code="HMC_MOUNT_TYPE_01" name="By gluing (conductive glue)" value="1"/>
                <list-param-item code="HMC_MOUNT_TYPE_02" name="By soldering (solder)" value="2"/>
            </family-param>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="mwrf_mc" name="RF/MW Inductors">
            <family-param code="ec_mc_type" name="Type" value-type="LIST" optional="false" in-hmc="false"
                          default-val="3">
                <list-param-item code="EC_MC_TYPE_01" name="Low-current (or low-level) wirewound inductor" value="1"/>
                <list-param-item code="EC_MC_TYPE_02" name="High-current (or power) wirewound inductor" value="2"/>
                <list-param-item code="EC_MC_TYPE_03" name="Multilayer inductor" value="3"/>
                <list-param-item code="EC_MC_TYPE_04" name="Low-power (or low-level) transformer" value="4"/>
                <list-param-item code="EC_MC_TYPE_05" name="High-power transformer" value="5"/>
            </family-param>
            <app-stress code="ec_delta_t" name="ΔT" value-type="NUMERIC" unit="°C" optional="false" in-hmc="false"/>
            <app-stress code="mwrf_eta" name="&amp;eta;" value-type="NUMERIC" optional="false" in-hmc="false"/>
            <family-param code="hmc_mount_type" name="Mount type (H&amp;M)" value-type="LIST" optional="false"
                          in-hmc="true">
                <list-param-item code="HMC_MOUNT_TYPE_01" name="By gluing (conductive glue)" value="1"/>
                <list-param-item code="HMC_MOUNT_TYPE_02" name="By soldering (solder)" value="2"/>
            </family-param>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="mwrf_pa" name="Other RF/MW passive components">
            <family-param code="mwrf_pa_type" name="Type" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="MWRF_PA_TYPE_01"
                                 name="Passive components for microwave applications, fixed: attenuator, load (50 Ohm), filter, power divider (combiner, splitter)"
                                 value="1"/>
                <list-param-item code="MWRF_PA_TYPE_02"
                                 name="Passive components for microwave applications, variable: variable attenuator, tuneable filter"
                                 value="2"/>
                <list-param-item code="MWRF_PA_TYPE_03"
                                 name="Passive components for microwave applications, with ferrites: circulator, isolator, phase shifter"
                                 value="3"/>
                <list-param-item code="MWRF_PA_TYPE_04"
                                 name="Passive components for microwave applications: surface wave filters" value="4"/>
            </family-param>
            <app-stress code="mwrf_delta_t" name="Rise of temperature" value-type="NUMERIC" unit="°C" optional="false"
                        in-hmc="false"/>
            <app-stress code="mwrf_eta" name="&amp;eta;" value-type="NUMERIC" optional="false" in-hmc="false"/>
            <family-param code="hmc_mount_type" name="Mount type (H&amp;M)" value-type="LIST" optional="false"
                          in-hmc="true">
                <list-param-item code="HMC_MOUNT_TYPE_01" name="By gluing (conductive glue)" value="1"/>
                <list-param-item code="HMC_MOUNT_TYPE_02" name="By soldering (solder)" value="2"/>
            </family-param>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
    </macro-family>
    <macro-family code="cots">
        <family code="cots_co" name="Common functions">
            <family-param code="cots_ff" name="Form factor" value-type="NUMERIC" optional="false" in-hmc="false"/>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="cots_cpu" name="CPU function">
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="cots_fmb" name="Flash memory boot function">
            <family-param code="cots_d_fb" name="D_flash_boot" value-type="NUMERIC" optional="false" in-hmc="false"/>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="cots_fms" name="Flash memory storage function">
            <family-param code="cots_d_fs" name="D_flash_stock" value-type="NUMERIC" optional="false" in-hmc="false"/>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="cots_dm" name="DRAM memory function">
            <family-param code="cots_d_dram" name="D_DRAM" value-type="NUMERIC" optional="false" in-hmc="false"/>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="cots_llcs" name="L2, L3 cache or SRAM function">
            <family-param code="cots_d_sram" name="D_SRAM" value-type="NUMERIC" optional="false" in-hmc="false"/>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="cots_sc" name="SCSI controller function">
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="cots_ch" name="Chipset function">
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="cots_ec" name="Ethernet control function">
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="cots_gc" name="Graphic control function">
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="cots_fc" name="Fieldbus control function">
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="cots_wc" name="Wireless control function">
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="cots_adc" name="Analog-to-digital or digital-to-analog conversion function">
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="cots_pbd" name="Parallel bus digital line">
            <family-param code="cots_m_paral" name="M parallel" value-type="NUMERIC" optional="false" in-hmc="false"/>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="cots_adl" name="Analog or discrete line">
            <family-param code="cots_m_analog" name="M analog" value-type="NUMERIC" optional="false" in-hmc="false"/>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="cots_spl" name="Serial peripheral line">
            <family-param code="cots_m_serial" name="M serial" value-type="NUMERIC" optional="false" in-hmc="false"/>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="cots_sbl" name="Serial bus line">
            <family-param code="cots_m_serial" name="M serial" value-type="NUMERIC" optional="false" in-hmc="false"/>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="cots_ioio" name="Input/output isolation by optocoupling">
            <family-param code="cots_io_quantity" name="I/O Quantity" value-type="NUMERIC" optional="false"
                          in-hmc="false"/>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="cots_ioier" name="Input/output isolation or switching by electromechanical relay">
            <family-param code="cots_io_quantity" name="I/O Quantity" value-type="NUMERIC" optional="false"
                          in-hmc="false"/>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
    </macro-family>
    <macro-family code="misc">
        <family code="misc_ls" name="LCD (TFT,STN) screens">
            <family-param code="misc_op_life" name="Operating Life" value-type="NUMERIC" unit="h" optional="false"
                          in-hmc="false"/>
            <family-param code="misc_t_use" name="T-use" value-type="NUMERIC" optional="false" in-hmc="false"/>
            <family-param code="misc_prpm" name="PrPM" value-type="NUMERIC" unit="h" optional="false" in-hmc="false"/>
            <family-param code="misc_beta" name="&amp;beta;" value-type="NUMERIC" optional="false" in-hmc="false"/>
            <family-param code="misc_ls_type" name="Type" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="MISC_LS_TYPE_01" name="TFT" value="1"/>
                <list-param-item code="MISC_LS_TYPE_02" name="STN" value="2"/>
            </family-param>
            <family-param code="misc_ls_mob" name="Mobility" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="MISC_LS_MOBILITY_01" name="Portable" value="1"/>
                <list-param-item code="MISC_LS_MOBILITY_02" name="Fixed" value="2"/>
            </family-param>
            <family-param code="misc_ls_class" name="Class" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="MISC_LS_CLASS_01" name="I" value="1"/>
                <list-param-item code="MISC_LS_CLASS_02" name="II" value="2"/>
                <list-param-item code="MISC_LS_CLASS_03" name="III" value="3"/>
                <list-param-item code="MISC_LS_CLASS_04" name="IV" value="4"/>
            </family-param>
            <family-param code="misc_ls_diag" name="Diagonal" value-type="NUMERIC" unit="&quot;" optional="false"
                          in-hmc="false"/>
            <family-param code="misc_ls_pwr" name="Power" value-type="NUMERIC" unit="W" optional="false"
                          in-hmc="false"/>
        </family>
        <family code="misc_hd" name="Hard Drives">
            <family-param code="misc_op_life" name="Operating Life" value-type="NUMERIC" unit="h" optional="false"
                          in-hmc="false"/>
            <family-param code="misc_t_use" name="T-use" value-type="NUMERIC" optional="false" in-hmc="false"/>
            <family-param code="misc_prpm" name="PrPM" value-type="NUMERIC" unit="h" optional="false" in-hmc="false"/>
            <family-param code="misc_beta" name="&amp;beta;" value-type="NUMERIC" optional="false" in-hmc="false"/>
            <family-param code="misc_hd_use" name="Usage" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="MISC_HD_USE_01" name="Normal use" value="1"/>
                <list-param-item code="MISC_HD_USE_02" name="Intensive use, ventilated" value="2"/>
                <list-param-item code="MISC_HD_USE_03" name="Intensive use, non-ventilated" value="3"/>
            </family-param>
            <family-param code="misc_hd_prot" name="Shocks/vibrations protection" value-type="LIST" optional="false"
                          in-hmc="false">
                <list-param-item code="MISC_HD_PROT_01" name="Protection against shocks/vibrations" value="1"/>
                <list-param-item code="MISC_HD_PROT_02" name="Qualification for shocks/vibrations" value="2"/>
                <list-param-item code="MISC_HD_PROT_03" name="No specific protection or qualification" value="3"/>
            </family-param>
            <family-param code="misc_hd_mob" name="Mobility" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="MISC_HD_MOBILITY_01" name="Portable or rack" value="1"/>
                <list-param-item code="MISC_HD_MOBILITY_02" name="Fixed" value="2"/>
            </family-param>
            <family-param code="misc_hd_family" name="HD Family" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="MISC_HD_FAMILY_01"
                                 name="IDE hard drive family (IDE, EIDE, E-IDE, ATA, SATA,S-ATA, Ultra ATA, DMA, Ultra DMA, etc.)"
                                 value="1"/>
                <list-param-item code="MISC_HD_FAMILY_02"
                                 name="SCSI hard drive family (SCSI-1, 2, 3, Ultra Wide SCSI 1, 2, 3, 4, SAS, etc.)"
                                 value="2"/>
            </family-param>
            <family-param code="misc_hd_ta" name="Mean access time" value-type="NUMERIC" unit="ms" optional="false"
                          in-hmc="false"/>
            <family-param code="misc_hd_pc" name="Platter count" value-type="NUMERIC" optional="false" in-hmc="false"/>
            <family-param code="misc_hd_dc" name="Duty cycle" value-type="NUMERIC" optional="false" in-hmc="false"/>
            <family-param code="misc_hd_ft" name="Format" value-type="NUMERIC" unit="&quot;" optional="false"
                          in-hmc="false"/>
        </family>
        <family code="misc_cm" name="CRT Monitors">
            <family-param code="misc_op_life" name="Operating Life" value-type="NUMERIC" unit="h" optional="false"
                          in-hmc="false"/>
            <family-param code="misc_t_use" name="T-use" value-type="NUMERIC" optional="false" in-hmc="false"/>
            <family-param code="misc_prpm" name="PrPM" value-type="NUMERIC" unit="h" optional="false" in-hmc="false"/>
            <family-param code="misc_beta" name="&amp;beta;" value-type="NUMERIC" optional="false" in-hmc="false"/>
            <family-param code="misc_cm_wt" name="Weight" value-type="NUMERIC" unit="Kg" optional="false"
                          in-hmc="false"/>
            <family-param code="misc_cm_diag" name="Diagonal" value-type="NUMERIC" unit="&quot;" optional="false"
                          in-hmc="false"/>
            <family-param code="misc_cm_fh" name="Max Horizontal scanning frequency" value-type="NUMERIC" unit="KHz"
                          optional="false" in-hmc="false"/>
            <family-param code="misc_cm_pwr" name="Max operating power" value-type="NUMERIC" unit="W" optional="false"
                          in-hmc="false"/>
            <family-param code="sa_hermeticity" name="Hermeticity" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="SA_HERMETICITY_TYPE_01" name="Hermetic" value="1"/>
                <list-param-item code="SA_HERMETICITY_TYPE_02" name="Non-hermetic" value="2"/>
            </family-param>
            <family-param code="hmc_mount_type" name="Mount type (H&amp;M)" value-type="LIST" optional="false"
                          in-hmc="true">
                <list-param-item code="HMC_MOUNT_TYPE_01" name="By gluing (conductive glue)" value="1"/>
                <list-param-item code="HMC_MOUNT_TYPE_02" name="By soldering (solder)" value="2"/>
            </family-param>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="misc_vc" name="AC/DC and DC/DC voltage converters">
            <family-param code="misc_vc_tech" name="Technology" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="MISC_VM_TECH_AC" name="AC/DC" value="1"/>
                <list-param-item code="MISC_VM_TECH_DC" name="DC/DC" value="2"/>
            </family-param>
            <family-param code="misc_vc_pwr" name="Output Power" value-type="NUMERIC" unit="W" optional="false"
                          in-hmc="false"/>
            <family-param code="misc_vc_vol" name="Volume" value-type="NUMERIC" unit="cm3" optional="false"
                          in-hmc="false"/>
            <family-param code="misc_vc_case" name="Case type" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="MISC_VM_CASE_01" name="Moulded" value="1"/>
                <list-param-item code="MISC_VM_CASE_02" name="Others" value="2"/>
            </family-param>
            <family-param code="hmc_mount_type" name="Mount type (H&amp;M)" value-type="LIST" optional="false"
                          in-hmc="true">
                <list-param-item code="HMC_MOUNT_TYPE_01" name="By gluing (conductive glue)" value="1"/>
                <list-param-item code="HMC_MOUNT_TYPE_02" name="By soldering (solder)" value="2"/>
            </family-param>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="misc_lnb" name="Lithium and nickel batteries">
            <family-param code="misc_lnb_ol1" name="Operating Life 1" value-type="NUMERIC" unit="h" optional="false"
                          in-hmc="false"/>
            <family-param code="misc_lnb_ol2" name="Operating Life 2" value-type="NUMERIC" unit="h" optional="false"
                          in-hmc="false"/>
            <family-param code="misc_prpm" name="PrPM" value-type="NUMERIC" unit="h" optional="false" in-hmc="false"/>
            <family-param code="misc_beta" name="&amp;beta;" value-type="NUMERIC" optional="false" in-hmc="false"/>
            <family-param code="misc_lnb_type" name="Type" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="MISC_LNB_TYPE_01" name="Lithium - Li-ion Polymer" value="1"/>
                <list-param-item code="MISC_LNB_TYPE_02" name="Lithium - Li-ion" value="2"/>
                <list-param-item code="MISC_LNB_TYPE_03" name="Lithium - Li-metal Phosphate" value="3"/>
                <list-param-item code="MISC_LNB_TYPE_04" name="Lithium - Nano Titanium" value="4"/>
                <list-param-item code="MISC_LNB_TYPE_05" name="Nickel - NiMH Metal Hydride" value="5"/>
                <list-param-item code="MISC_LNB_TYPE_06" name="Nickel - Ni-Zn Zinc" value="6"/>
                <list-param-item code="MISC_LNB_TYPE_07" name="Nickel - Ni-Cd Cadmium" value="7"/>
            </family-param>
            <family-param code="misc_lnb_ncell" name="Number of cells" value-type="NUMERIC" optional="false"
                          in-hmc="false"/>
            <family-param code="hmc_mount_type" name="Mount type (H&amp;M)" value-type="LIST" optional="false"
                          in-hmc="true">
                <list-param-item code="HMC_MOUNT_TYPE_01" name="By gluing (conductive glue)" value="1"/>
                <list-param-item code="HMC_MOUNT_TYPE_02" name="By soldering (solder)" value="2"/>
            </family-param>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="misc_fa" name="Fans">
            <family-param code="misc_fa_ol" name="Operating Life Calendar" value-type="NUMERIC" unit="h"
                          optional="false" in-hmc="false"/>
            <family-param code="misc_prpm" name="PrPM" value-type="NUMERIC" unit="h" optional="false" in-hmc="false"/>
            <family-param code="misc_beta" name="&amp;beta;" value-type="NUMERIC" optional="false" in-hmc="false"/>
            <app-stress code="misc_fa_bear_t" name="Bearing Temperature" value-type="NUMERIC" unit="°C" optional="false"
                        in-hmc="false"/>
            <family-param code="hmc_mount_type" name="Mount type (H&amp;M)" value-type="LIST" optional="false"
                          in-hmc="true">
                <list-param-item code="HMC_MOUNT_TYPE_01" name="By gluing (conductive glue)" value="1"/>
                <list-param-item code="HMC_MOUNT_TYPE_02" name="By soldering (solder)" value="2"/>
            </family-param>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="misc_ke" name="Keyboards">
            <family-param code="misc_ke_ol" name="Operating Life" value-type="NUMERIC" unit="h" optional="false"
                          in-hmc="false"/>
            <family-param code="misc_prpm" name="PrPM" value-type="NUMERIC" unit="h" optional="false" in-hmc="false"/>
            <family-param code="misc_beta" name="&amp;beta;" value-type="NUMERIC" optional="false" in-hmc="false"/>
        </family>
        <family code="misc_ke_bd" name="Keyboards - Board">
        </family>
        <family code="misc_ke_kb" name="Keyboards - Keyboard">
            <family-param code="misc_ke_key" name="Number of keys" value-type="NUMERIC" optional="false"
                          in-hmc="false"/>
            <family-param code="hmc_mount_type" name="Mount type (H&amp;M)" value-type="LIST" optional="false"
                          in-hmc="true">
                <list-param-item code="HMC_MOUNT_TYPE_01" name="By gluing (conductive glue)" value="1"/>
                <list-param-item code="HMC_MOUNT_TYPE_02" name="By soldering (solder)" value="2"/>
            </family-param>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
    </macro-family>
    <macro-family code="pc">
        <family code="pc_dic" name="Digital integrated circuit">
            <family-param code="pc_herme" name="Hermeticity" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="PC_HERME_01" name="Hermetic" value="1"/>
                <list-param-item code="PC_HERME_02" name="Non-hermetic" value="2"/>
            </family-param>
            <family-param code="pc_np" name="Np" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="PC_NP_01" name="&lt;= 24 p" value="1"/>
                <list-param-item code="PC_NP_02" name="24 to 48 p" value="2"/>
                <list-param-item code="PC_NP_03" name="48 to 144 p" value="3"/>
                <list-param-item code="PC_NP_04" name="144 to 288 p" value="4"/>
                <list-param-item code="PC_NP_05" name="&gt; 288 p" value="5"/>
            </family-param>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="pc_mic" name="Memory integrated circuit">
            <family-param code="pc_herme" name="Hermeticity" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="PC_HERME_01" name="Hermetic" value="1"/>
                <list-param-item code="PC_HERME_02" name="Non-hermetic" value="2"/>
            </family-param>
            <family-param code="pc_np" name="Np" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="PC_NP_01" name="&lt;= 24 p" value="1"/>
                <list-param-item code="PC_NP_02" name="24 to 48 p" value="2"/>
                <list-param-item code="PC_NP_03" name="48 to 144 p" value="3"/>
                <list-param-item code="PC_NP_04" name="144 to 288 p" value="4"/>
                <list-param-item code="PC_NP_05" name="&gt; 288 p" value="5"/>
            </family-param>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="pc_sic" name="Micro*, DSP, simple ASIC integrated circuit">
            <family-param code="pc_herme" name="Hermeticity" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="PC_HERME_01" name="Hermetic" value="1"/>
                <list-param-item code="PC_HERME_02" name="Non-hermetic" value="2"/>
            </family-param>
            <family-param code="pc_np" name="Np" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="PC_NP_01" name="&lt;= 24 p" value="1"/>
                <list-param-item code="PC_NP_02" name="24 to 48 p" value="2"/>
                <list-param-item code="PC_NP_03" name="48 to 144 p" value="3"/>
                <list-param-item code="PC_NP_04" name="144 to 288 p" value="4"/>
                <list-param-item code="PC_NP_05" name="&gt; 288 p" value="5"/>
            </family-param>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="pc_cic" name="Integrated circuit Analog, Mixed, FPGA, CPLD, complex ASIC">
            <family-param code="pc_herme" name="Hermeticity" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="PC_HERME_01" name="Hermetic" value="1"/>
                <list-param-item code="PC_HERME_02" name="Non-hermetic" value="2"/>
            </family-param>
            <family-param code="pc_np" name="Np" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="PC_NP_01" name="&lt;= 24 p" value="1"/>
                <list-param-item code="PC_NP_02" name="24 to 48 p" value="2"/>
                <list-param-item code="PC_NP_03" name="48 to 144 p" value="3"/>
                <list-param-item code="PC_NP_04" name="144 to 288 p" value="4"/>
                <list-param-item code="PC_NP_05" name="&gt; 288 p" value="5"/>
            </family-param>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="pc_di" name="Diode">
            <family-param code="pc_herme" name="Hermeticity" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="PC_HERME_01" name="Hermetic" value="1"/>
                <list-param-item code="PC_HERME_02" name="Non-hermetic" value="2"/>
            </family-param>
            <family-param code="pc_smd_thl" name="SMD or through-hole" value-type="LIST" optional="false"
                          in-hmc="false">
                <list-param-item code="PC_SMD_THL_01" name="SMD" value="1"/>
                <list-param-item code="PC_SMD_THL_02" name="THL" value="2"/>
            </family-param>
            <family-param code="pc_dt_pwr" name="Power type" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="PC_DT_PWR_01" name="Low-power" value="1"/>
                <list-param-item code="PC_DT_PWR_02" name="Power" value="2"/>
            </family-param>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="pc_ts" name="Transistor">
            <family-param code="pc_herme" name="Hermeticity" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="PC_HERME_01" name="Hermetic" value="1"/>
                <list-param-item code="PC_HERME_02" name="Non-hermetic" value="2"/>
            </family-param>
            <family-param code="pc_smd_thl" name="SMD or through-hole" value-type="LIST" optional="false"
                          in-hmc="false">
                <list-param-item code="PC_SMD_THL_01" name="SMD" value="1"/>
                <list-param-item code="PC_SMD_THL_02" name="THL" value="2"/>
            </family-param>
            <family-param code="pc_dt_pwr" name="Power type" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="PC_DT_PWR_01" name="Low-power" value="1"/>
                <list-param-item code="PC_DT_PWR_02" name="Power" value="2"/>
            </family-param>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="pc_phd" name="Photodiode">
            <family-param code="pc_herme" name="Hermeticity" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="PC_HERME_01" name="Hermetic" value="1"/>
                <list-param-item code="PC_HERME_02" name="Non-hermetic" value="2"/>
            </family-param>
            <family-param code="pc_smd_thl" name="SMD or through-hole" value-type="LIST" optional="false"
                          in-hmc="false">
                <list-param-item code="PC_SMD_THL_01" name="SMD" value="1"/>
                <list-param-item code="PC_SMD_THL_02" name="THL" value="2"/>
            </family-param>
            <family-param code="pc_dt_pwr" name="Power type" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="PC_DT_PWR_01" name="Low-power" value="1"/>
                <list-param-item code="PC_DT_PWR_02" name="Power" value="2"/>
            </family-param>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="pc_pht" name="Phototransistor">
            <family-param code="pc_herme" name="Hermeticity" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="PC_HERME_01" name="Hermetic" value="1"/>
                <list-param-item code="PC_HERME_02" name="Non-hermetic" value="2"/>
            </family-param>
            <family-param code="pc_smd_thl" name="SMD or through-hole" value-type="LIST" optional="false"
                          in-hmc="false">
                <list-param-item code="PC_SMD_THL_01" name="SMD" value="1"/>
                <list-param-item code="PC_SMD_THL_02" name="THL" value="2"/>
            </family-param>
            <family-param code="pc_dt_pwr" name="Power type" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="PC_DT_PWR_01" name="Low-power" value="1"/>
                <list-param-item code="PC_DT_PWR_02" name="Power" value="2"/>
            </family-param>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="pc_po" name="Potentiometer">
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="pc_re" name="Resistor">
            <family-param code="pc_re_pwr" name="Power type" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="PC_RE_PWR_01" name="High-power" value="1"/>
                <list-param-item code="PC_RE_PWR_02" name="Low-power" value="2"/>
            </family-param>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="pc_emfr" name="Etched metal foil resistor">
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="pc_rnc" name="Resistor network, Resistor chip">
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="pc_cc" name="Ceramic capacitor">
            <family-param code="pc_cc_cv_cat" name="CV category" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="PC_CC_CV_CAT_01" name="Moderate CV product" value="1"/>
                <list-param-item code="PC_CC_CV_CAT_02" name="High CV product" value="2"/>
            </family-param>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="pc_ac" name="Aluminium capacitor">
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="pc_tc" name="Tantalum capacitor">
            <family-param code="pc_tc_tech" name="Technology" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="PC_TC_TECH_01" name="Gel" value="1"/>
                <list-param-item code="PC_TC_TECH_02" name="Solid" value="2"/>
            </family-param>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="pc_in" name="Inductor">
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="pc_tf" name="Transformer">
            <family-param code="pc_tf_pwr" name="Power type" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="PC_TF_PWR_01" name="Low-power" value="1"/>
                <list-param-item code="PC_TF_PWR_02" name="High-power" value="2"/>
            </family-param>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="pc_qcr" name="Quartz crystal resonator">
            <family-param code="pc_smd_thl" name="SMD or through-hole" value-type="LIST" optional="false"
                          in-hmc="false">
                <list-param-item code="PC_SMD_THL_01" name="SMD" value="1"/>
                <list-param-item code="PC_SMD_THL_02" name="THL" value="2"/>
            </family-param>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="pc_qco" name="Quartz crystal oscillator">
            <family-param code="pc_smd_thl" name="SMD or through-hole" value-type="LIST" optional="false"
                          in-hmc="false">
                <list-param-item code="PC_SMD_THL_01" name="SMD" value="1"/>
                <list-param-item code="PC_SMD_THL_02" name="THL" value="2"/>
            </family-param>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="pc_ri10c" name="Relay up to 10 contacts">
            <family-param code="pc_load_type" name="Load type" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="PC_LOAD_TYPE_01" name="Resistive load" value="1"/>
                <list-param-item code="PC_LOAD_TYPE_02" name="Non-resistive load" value="2"/>
            </family-param>
            <family-param code="pc_act_rate" name="Actuation rate" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="PC_ACT_RATE_01" name="&lt; 3 actuations/h" value="1"/>
                <list-param-item code="PC_ACT_RATE_02" name="≥ 3 actuations/h" value="2"/>
            </family-param>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="pc_rs10c" name="Relay &gt; 10 contacts">
            <family-param code="pc_load_type" name="Load type" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="PC_LOAD_TYPE_01" name="Resistive load" value="1"/>
                <list-param-item code="PC_LOAD_TYPE_02" name="Non-resistive load" value="2"/>
            </family-param>
            <family-param code="pc_act_rate" name="Actuation rate" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="PC_ACT_RATE_01" name="&lt; 3 actuations/h" value="1"/>
                <list-param-item code="PC_ACT_RATE_02" name="≥ 3 actuations/h" value="2"/>
            </family-param>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="pc_pbsi" name="Push button, switch, invertor (&lt; 4 pins)">
            <family-param code="pc_load_type" name="Load type" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="PC_LOAD_TYPE_01" name="Resistive load" value="1"/>
                <list-param-item code="PC_LOAD_TYPE_02" name="Non-resistive load" value="2"/>
            </family-param>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="pc_de" name="DIP, encoder (4 to 10 pins)">
            <family-param code="pc_load_type" name="Load type" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="PC_LOAD_TYPE_01" name="Resistive load" value="1"/>
                <list-param-item code="PC_LOAD_TYPE_02" name="Non-resistive load" value="2"/>
            </family-param>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="pc_sw" name="Switch (&gt; 10 pins)">
            <family-param code="pc_load_type" name="Load type" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="PC_LOAD_TYPE_01" name="Resistive load" value="1"/>
                <list-param-item code="PC_LOAD_TYPE_02" name="Non-resistive load" value="2"/>
            </family-param>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="pc_coic" name="Connector for printed circuits and IC supports">
            <family-param code="pc_contact" name="Contact count" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="PC_CONTACT_01" name="Up to 20 contacts" value="1"/>
                <list-param-item code="PC_CONTACT_02" name="20 to 200 contacts" value="2"/>
                <list-param-item code="PC_CONTACT_03" name="Over 200 contacts" value="3"/>
            </family-param>
            <family-param code="pc_co_tech" name="Technology" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="PC_CO_TECH_01" name="Soldered (PTH or SMD)" value="1"/>
                <list-param-item code="PC_CO_TECH_02" name="Wrapping or insertion" value="2"/>
            </family-param>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="pc_coo" name="Other connector">
            <family-param code="pc_contact" name="Contact count" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="PC_CONTACT_01" name="Up to 20 contacts" value="1"/>
                <list-param-item code="PC_CONTACT_02" name="20 to 200 contacts" value="2"/>
                <list-param-item code="PC_CONTACT_03" name="Over 200 contacts" value="3"/>
            </family-param>
            <family-param code="pc_co_tech" name="Technology" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="PC_CO_TECH_01" name="Soldered (PTH or SMD)" value="1"/>
                <list-param-item code="PC_CO_TECH_02" name="Wrapping or insertion" value="2"/>
            </family-param>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="pc_pcp" name="Printed circuit, PTH">
            <family-param code="pc_mount_pt" name="Mounting point count" value-type="LIST" optional="false"
                          in-hmc="false">
                <list-param-item code="PC_MOUNT_PT_01" name="Up to 2000 mounting points" value="1"/>
                <list-param-item code="PC_MOUNT_PT_02" name="&gt; 2000 mounting points" value="2"/>
            </family-param>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="pc_pcs" name="Printed circuit, SMD">
            <family-param code="pc_mount_pt" name="Mounting point count" value-type="LIST" optional="false"
                          in-hmc="false">
                <list-param-item code="PC_MOUNT_PT_01" name="Up to 2000 mounting points" value="1"/>
                <list-param-item code="PC_MOUNT_PT_02" name="&gt; 2000 mounting points" value="2"/>
            </family-param>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="pc_hd" name="Hard drive">
            <family-param code="pc_hd_tech" name="Technology" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="PC_HD_TECH_01" name="EIDE" value="1"/>
                <list-param-item code="PC_HD_TECH_02" name="SCSI" value="2"/>
            </family-param>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="pc_ls" name="LCD screen (Class III)">
            <family-param code="pc_ls_type" name="Type" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="PC_LS_TYPE_01" name="STN" value="1"/>
                <list-param-item code="PC_LS_TYPE_02" name="TFT" value="2"/>
            </family-param>
            <family-param code="pc_ls_diag" name="Diagonal" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="PC_LS_DIAG_01" name="Up to 14&quot;" value="1"/>
                <list-param-item code="PC_LS_DIAG_02" name="14&quot; to 20&quot;" value="2"/>
                <list-param-item code="PC_LS_DIAG_03" name="Over 20&quot;" value="3"/>
            </family-param>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="pc_crtm" name="CRT monitor">
            <family-param code="pc_crtm_diag" name="Diagonal" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="PC_CRTM_DIAG_01" name="Up to 20&quot;" value="1"/>
                <list-param-item code="PC_CRTM_DIAG_02" name="!!!PC_CRTM_DIAG_02_KEY!!!" value="2"/>
            </family-param>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="pc_sps" name="Switching power supply">
            <family-param code="pc_sps_pwr" name="Power" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="PC_SPS_PWR_01" name="Up to 500W" value="1"/>
                <list-param-item code="PC_SPS_PWR_02" name="Over 500W" value="2"/>
            </family-param>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
        <family code="pc_dc" name="DC/DC converter">
            <family-param code="pc_dc_pwr" name="Power" value-type="LIST" optional="false" in-hmc="false">
                <list-param-item code="PC_DC_PWR_01" name="Up to 50W" value="1"/>
                <list-param-item code="PC_DC_PWR_02" name="Over 50W" value="2"/>
            </family-param>
            <family-param code="hmc_c_mould" name="C_moulding" value-type="LIST" optional="false" in-hmc="true">
                <list-param-item code="HMC_C_MOULDING_01" name="Hermetic circuit non-moulded" value="1"/>
                <list-param-item code="HMC_C_MOULDING_02" name="Moulded circuit, silicon-embedded" value="2"/>
                <list-param-item code="HMC_C_MOULDING_03" name="Moulded circuit, polyurethane-embedded" value="3"/>
                <list-param-item code="HMC_C_MOULDING_04" name="Moulded circuit, epoxy-embedded" value="4"/>
            </family-param>
        </family>
    </macro-family>
</open-fides-notice>
